(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(J1-Pin_6-Pad6)")
	(net 2 "unconnected-(J1-Pin_3-Pad3)")
	(net 3 "unconnected-(J1-Pin_1-Pad1)")
	(net 4 "Net-(J1-Pin_12)")
	(net 5 "Net-(J1-Pin_9)")
	(net 6 "unconnected-(J1-Pin_11-Pad11)")
	(net 7 "Net-(J1-Pin_8)")
	(net 8 "Net-(J1-Pin_4)")
	(net 9 "Net-(J1-Pin_5)")
	(net 10 "unconnected-(J1-Pin_7-Pad7)")
	(net 11 "Net-(J1-Pin_10)")
	(net 12 "unconnected-(J1-Pin_2-Pad2)")
	(net 13 "Net-(J2-Pin_11)")
	(net 14 "unconnected-(J2-Pin_6-Pad6)")
	(net 15 "Net-(J10-Pin_2)")
	(net 16 "unconnected-(J2-Pin_5-Pad5)")
	(net 17 "Net-(J2-Pin_12)")
	(net 18 "Net-(J10-Pin_1)")
	(net 19 "Net-(J2-Pin_8)")
	(net 20 "unconnected-(J2-Pin_1-Pad1)")
	(net 21 "unconnected-(J2-Pin_3-Pad3)")
	(net 22 "Net-(J2-Pin_10)")
	(net 23 "unconnected-(J3-Pin_6-Pad6)")
	(net 24 "unconnected-(J3-Pin_2-Pad2)")
	(net 25 "Net-(J4-Pin_3)")
	(net 26 "Net-(J4-Pin_4)")
	(net 27 "unconnected-(J4-Pin_2-Pad2)")
	(net 28 "unconnected-(J4-Pin_1-Pad1)")
	(net 29 "Net-(J4-Pin_6)")
	(net 30 "unconnected-(J5-Pin_7-Pad7)")
	(net 31 "unconnected-(J6-Pin_1-Pad1)")
	(net 32 "unconnected-(J6-Pin_8-Pad8)")
	(net 33 "unconnected-(J6-Pin_5-Pad5)")
	(net 34 "unconnected-(J6-Pin_4-Pad4)")
	(net 35 "unconnected-(J6-Pin_7-Pad7)")
	(net 36 "unconnected-(J6-Pin_3-Pad3)")
	(net 37 "Net-(J9-Pin_1)")
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "025bfb2d-1779-4e95-ab00-770bc10a65d9")
		(at 89 75.46)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J9"
			(at 0 -3 0)
			(layer "F.SilkS")
			(uuid "f546f0fe-5b9c-4ea1-8400-58430354dc5e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 0 4.87 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1f50ec67-3cfd-460c-be80-115ff4bca509")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "515dd549-14f3-43b9-9abe-b8eacb1b4373")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "29a2cf06-1a58-44b1-aacb-933ff459be6e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "126fd40c-c5ee-4501-84cc-27ff0b9d9052")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/57fcdd4c-4343-42d3-8206-d354a4ed76a3")
		(sheetname "Root")
		(sheetfile "andrew watering 8.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.33 -1.33)
			(end 0 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ccbe36fc-26b7-4ca2-8f84-238c782713f5")
		)
		(fp_line
			(start -1.33 0)
			(end -1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "baa3dcd0-29ef-4c68-93c1-8536725bd770")
		)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "052305c7-552b-46ca-94f8-5c4cf051624c")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.33 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c11de355-8b2c-4c70-bba2-5c86f6287e94")
		)
		(fp_line
			(start -1.33 3.87)
			(end 1.33 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ceefa439-256f-4d1a-a5ff-e1c8822ef21c")
		)
		(fp_line
			(start 1.33 1.27)
			(end 1.33 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "123dd68d-08f0-4cdd-8fef-cfd38441b9ca")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 4.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ad4fe8f9-9d73-4330-838f-1277254aa902")
		)
		(fp_line
			(start -1.8 4.35)
			(end 1.8 4.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab08cbeb-01ed-4300-8ac8-3bedc1115ccc")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7d3ed981-5d37-4f65-b419-2f22de9256a5")
		)
		(fp_line
			(start 1.8 4.35)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4257e781-9000-4e84-b8b2-58f64b059fa4")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "59cf48ca-2fc6-47a9-af94-1b409dabd4d1")
		)
		(fp_line
			(start -1.27 3.81)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6707d3b6-1504-4ba0-a244-1dc5ac9939e8")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4037b71e-18cc-48c7-b5dc-7daf5a0f8b36")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac44f65c-8b25-4eb8-a9db-3f4039aa1fb6")
		)
		(fp_line
			(start 1.27 3.81)
			(end -1.27 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9dbabb84-eb88-468c-b31c-e2986c3e58f6")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J9-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "954bb57b-741b-410e-9fe6-e58b779e3a8c")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-Pin_4)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "fd46e1c3-152f-450d-afe0-e08e623ecc0b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(uuid "0e1a3d2d-17e8-48be-8105-61fa8dee4774")
		(at 96.3 75)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R2"
			(at 6.35 -2.72 0)
			(layer "F.SilkS")
			(uuid "3aae398e-dc15-43e2-b29b-4a33ad1d3277")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2.2k"
			(at 6 -0.28 0)
			(layer "F.Fab")
			(uuid "43937384-6815-427a-86c8-695f96e01565")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "11a67474-f787-4e74-a91e-ba574624947f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3c9b5eb8-dd83-44dd-9f33-819248fcdb1e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d6accfd9-453f-404c-a00c-b81295596bef")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/0a6ab40a-d6cd-44f7-99ef-fb87fe0f8c13")
		(sheetname "Root")
		(sheetfile "andrew watering 8.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.04 0)
			(end 1.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7f1a8623-afbb-4b52-bfb9-f6688bcdb361")
		)
		(fp_line
			(start 1.73 -1.72)
			(end 1.73 1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e91a3f1-a681-4d8e-a1c9-519c88a0480d")
		)
		(fp_line
			(start 1.73 1.72)
			(end 10.97 1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2e91aa3a-20bd-4196-8489-eb13c26c348b")
		)
		(fp_line
			(start 10.97 -1.72)
			(end 1.73 -1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aca0ca16-7f38-40fa-8362-0823d260890f")
		)
		(fp_line
			(start 10.97 1.72)
			(end 10.97 -1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "66b7e917-fdac-4b90-b69c-848622da3349")
		)
		(fp_line
			(start 11.66 0)
			(end 10.97 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "37cee5b4-9782-4162-85de-10f0227676b1")
		)
		(fp_line
			(start -1.05 -1.85)
			(end -1.05 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "42e6d1a4-033c-448c-9296-e679e3d91e33")
		)
		(fp_line
			(start -1.05 1.85)
			(end 13.75 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab0de37b-894b-40e7-a0b0-ba66f1642958")
		)
		(fp_line
			(start 13.75 -1.85)
			(end -1.05 -1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ecd17ef4-542c-49e9-b5b1-41848a372b87")
		)
		(fp_line
			(start 13.75 1.85)
			(end 13.75 -1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8b376d39-d827-4fce-9b37-57ffa741d3ef")
		)
		(fp_line
			(start 0 0)
			(end 1.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ae631e0-3299-46ba-9dc8-9c318e2bab89")
		)
		(fp_line
			(start 1.85 -1.6)
			(end 1.85 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "64c763b5-1230-4d44-b2f1-0f246ef41f0a")
		)
		(fp_line
			(start 1.85 1.6)
			(end 10.85 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "837aac3e-43d8-4acd-ac81-547d13681caa")
		)
		(fp_line
			(start 10.85 -1.6)
			(end 1.85 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "613719ef-cdd0-4a6a-a3ef-15243634fc6a")
		)
		(fp_line
			(start 10.85 1.6)
			(end 10.85 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce3b60fa-b14c-4737-a189-cb132714809d")
		)
		(fp_line
			(start 12.7 0)
			(end 10.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48c8c67e-3a1a-4dd5-b038-58f13581680b")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J9-Pin_1)")
			(pintype "passive")
			(uuid "9fa60999-3c00-4a0a-9330-bb073173a674")
		)
		(pad "2" thru_hole oval
			(at 12.7 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J2-Pin_8)")
			(pintype "passive")
			(uuid "5e6ada5d-48bd-46dd-915c-42fd6b8d54a6")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(uuid "23a0b786-c02f-47a6-89f0-32194ca73a7d")
		(at 109 79 180)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R1"
			(at 6.7 -2.72 0)
			(layer "F.SilkS")
			(uuid "23356710-f00e-4c4e-8bb7-c3661b36887a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2.2k"
			(at 6 0 0)
			(layer "F.Fab")
			(uuid "255f3180-c325-47f0-af61-400d6f3aea3d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1c1e4537-c408-4ef1-be99-8a7773e9cb04")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "426fe291-7027-4295-adf5-64884dc4c77d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1497e08e-4b72-4b98-bca1-d7bd9bfe6e80")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/130525a0-cca8-4024-880a-535a160dbaa0")
		(sheetname "Root")
		(sheetfile "andrew watering 8.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 11.66 0)
			(end 10.97 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a221a121-6bec-4934-b690-de7837ce3150")
		)
		(fp_line
			(start 10.97 1.72)
			(end 10.97 -1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84240c94-7a74-477f-9ec1-eaa75979a525")
		)
		(fp_line
			(start 10.97 -1.72)
			(end 1.73 -1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4a63d60b-bda9-4590-bb6b-1f117893edfb")
		)
		(fp_line
			(start 1.73 1.72)
			(end 10.97 1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "653b3c7a-0fdd-49c6-9297-aa8ee2590bea")
		)
		(fp_line
			(start 1.73 -1.72)
			(end 1.73 1.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f7c0b6e1-e000-40f0-b201-7753b02be693")
		)
		(fp_line
			(start 1.04 0)
			(end 1.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4d415b45-3e0e-47a5-b723-d95439646d79")
		)
		(fp_line
			(start 13.75 1.85)
			(end 13.75 -1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1717158c-f7fe-4689-be07-496706e65969")
		)
		(fp_line
			(start 13.75 -1.85)
			(end -1.05 -1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a14118b8-7c1d-42c9-98a2-9b93560ca07e")
		)
		(fp_line
			(start -1.05 1.85)
			(end 13.75 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3cf37529-cc4b-4763-a77b-fe5ee7699f36")
		)
		(fp_line
			(start -1.05 -1.85)
			(end -1.05 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6ba8fce4-71ca-462b-be6f-8749abc49a96")
		)
		(fp_line
			(start 12.7 0)
			(end 10.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ddee176-41c4-411a-9718-bf9ef6d67a69")
		)
		(fp_line
			(start 10.85 1.6)
			(end 10.85 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b7555ea2-e566-494c-b21e-38503ccd252a")
		)
		(fp_line
			(start 10.85 -1.6)
			(end 1.85 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f45a59b-270d-40d3-bd42-5a9898f19745")
		)
		(fp_line
			(start 1.85 1.6)
			(end 10.85 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a9765cf8-494e-43ea-b1d7-853ac60650f8")
		)
		(fp_line
			(start 1.85 -1.6)
			(end 1.85 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ef6bf00-4849-42d1-a7e0-b3c7a2c4129b")
		)
		(fp_line
			(start 0 0)
			(end 1.85 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "127c3a88-e680-4fca-a367-376495b2410b")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J2-Pin_8)")
			(pintype "passive")
			(uuid "d6b2dd66-599b-4537-b739-609e414e8edf")
		)
		(pad "2" thru_hole oval
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-Pin_4)")
			(pintype "passive")
			(uuid "dd8a626e-43ca-4765-8472-6901d33d2b8a")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "8c465a6c-0fb3-4f0f-8014-b160f825d7e3")
		(at 87 93.46)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J8"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(uuid "4453e037-3ce3-4b40-86f3-6177b073b4a3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 0 4.87 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6c2a0bff-592a-4bdb-bff0-f0d159e343d6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e2036a94-7007-434e-8549-d1d6f17ed4c8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bde28f74-f5bd-4d26-a48e-24615a0db094")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a8c4d382-3558-40ae-989c-efb1e25b82e7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/d3cb46b6-06d1-49e2-8bd3-7eb60167995a")
		(sheetname "Root")
		(sheetfile "andrew watering 8.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.33 -1.33)
			(end 0 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e5e986cf-7cf9-4d01-88c6-465c327e0a26")
		)
		(fp_line
			(start -1.33 0)
			(end -1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "959bacf9-62fd-48b1-a931-ad5b24f4bf1e")
		)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eed4ceae-a098-4ea0-b103-8ec1f89a989a")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.33 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "96175785-3b7c-419e-8e6a-c17fcfcbcacd")
		)
		(fp_line
			(start -1.33 3.87)
			(end 1.33 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe774993-9672-4558-9586-dbfc8744e431")
		)
		(fp_line
			(start 1.33 1.27)
			(end 1.33 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d66cb7f-409c-4fe0-a071-660b11ef8c56")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 4.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cfc40b28-8de7-46f7-9199-46ece2255c84")
		)
		(fp_line
			(start -1.8 4.35)
			(end 1.8 4.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9ae9b6bf-e632-4a3e-991f-fe7cc36aec8d")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2c232159-04ad-4667-953f-c6fef7ac6e5e")
		)
		(fp_line
			(start 1.8 4.35)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "84f0871c-77f0-47f1-9861-43cbafdeee43")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2d26a0ed-0eba-418f-82a5-4bbca12b01a8")
		)
		(fp_line
			(start -1.27 3.81)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2e75375f-a44a-4da1-a830-4ec7759ae49f")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f39f98bd-e913-4fb6-93d5-6e88c5d901bb")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c571149b-2780-4cd5-b9d2-57ea564a481b")
		)
		(fp_line
			(start 1.27 3.81)
			(end -1.27 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb7ee296-126f-4b6e-b2c2-e44a3a9dc508")
		)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
			(uuid "d6eb024d-ed15-49f4-897d-45354e6c0b83")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J4-Pin_4)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "e2d55507-336e-4e8a-a71c-76b27e230d98")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J4-Pin_3)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "3df0762e-ab6a-4230-bbbd-cc7173985d44")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "9cbf81fb-01e7-4d24-b11a-3aac9af21e27")
		(at 87 86.46)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J7"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(uuid "67419390-87df-4bbd-a1dd-08ec74585624")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 0 4.87 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ff43c2bc-84b1-4d19-a9ee-f371b88ca42e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "61bedc7f-ee9d-40d5-970e-8cf28fe2e628")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4317cb1b-6278-4089-a0b5-602443a1a6d3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "124c9901-923f-4b7a-b42e-98a4ae8ee3a9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/5f3f4f03-fda9-48ee-add6-d8342155705b")
		(sheetname "Root")
		(sheetfile "andrew watering 8.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.33 -1.33)
			(end 0 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8531e065-b7f8-4e93-9646-ecb536df588f")
		)
		(fp_line
			(start -1.33 0)
			(end -1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "961d9f91-9482-4844-9017-7940a688351e")
		)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7bc7b936-2efa-4fd4-ab76-ed44b3605b8b")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.33 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ccba7787-c854-44a5-b080-74b118a51bb2")
		)
		(fp_line
			(start -1.33 3.87)
			(end 1.33 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "364a7c9d-2cd8-4197-89b0-fe43d821962c")
		)
		(fp_line
			(start 1.33 1.27)
			(end 1.33 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3e438cf3-abc3-47a9-b0f4-4555812dfa6a")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 4.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4fbe8e73-ef0d-4666-a220-5491ad13dee3")
		)
		(fp_line
			(start -1.8 4.35)
			(end 1.8 4.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9ec72759-5152-4e68-8d25-21457aa4662a")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ba809c6a-2d23-4273-9164-8563b19209b3")
		)
		(fp_line
			(start 1.8 4.35)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "66c5de65-1dcd-45d0-b9fd-16b44e6ead0e")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "43dcc20a-fc6b-4cf6-8133-0f7bba0071e0")
		)
		(fp_line
			(start -1.27 3.81)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f1902e32-ff9d-4f09-8279-5503883ab752")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f432c7c9-574c-43d2-b9c5-f95cf53b49d5")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51d2a46b-f7ad-470c-b7eb-7f1ca491f6d5")
		)
		(fp_line
			(start 1.27 3.81)
			(end -1.27 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2106b168-71d0-4ea8-83ba-6e69cb478b3d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
			(uuid "9227bff3-9f51-471c-b0a4-080e5e7a601e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J4-Pin_6)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "6d7e6057-f9f5-49f6-b16d-accd193acf62")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-Pin_4)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "ad5bf7a4-bd57-4b57-ac1f-0ce98ed5356e")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "a4a45c5a-be7e-48c2-950a-f6a73be1ace8")
		(at 136 88.92)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J10"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(uuid "6ea68fe2-3661-435d-a385-052b9105c414")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x03_Socket"
			(at 0 7.41 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a4888f9e-4b21-4830-9757-ab86e2b67e4c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "619eea46-88c9-42e7-b94d-863a27d6e1e1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "65bcb3e8-7e0c-462b-ae13-3388796463b4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8ea2c2b6-bcfd-4031-a290-ba2a71f4ebf5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/f32487d1-4d1e-4fa0-b21f-ea749e072c8c")
		(sheetname "Root")
		(sheetfile "andrew watering 8.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.33 -1.33)
			(end 0 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8a4cf96c-cb52-4981-b0fc-2cd89df95e87")
		)
		(fp_line
			(start -1.33 0)
			(end -1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "14f6539d-9952-4f24-ac76-b48a0af30627")
		)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a85e025-51d9-4353-9350-c519f098643e")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.33 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e16218e-5ef4-42c4-a055-5467b4e491ba")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d84460c6-aad1-4715-a7cc-4db4f014b20f")
		)
		(fp_line
			(start 1.33 1.27)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6615b315-48b7-4d2d-afba-aab43810a9f6")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a553d619-280b-4d6e-b600-aeabe1ef3814")
		)
		(fp_line
			(start -1.8 6.85)
			(end 1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8d416833-c8c2-4fd3-8569-b8368ae845c2")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e2cd84fd-7980-4444-948a-cc939d604bec")
		)
		(fp_line
			(start 1.8 6.85)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1445920a-4f80-4d45-bceb-85736f116236")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac02f514-af06-4b7b-819b-0ee0e0d9cb98")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87179f0e-623f-40f6-b9f2-1e08ff1bb8e3")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b74624df-6cf4-4b7b-b302-eda1c0479019")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d14ac085-2fd3-40db-8f5f-b26b314e245e")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a4cc31c-9461-4c6c-aa48-b86fd64724ca")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "7a210a68-3dd9-4695-8771-b59e2c2dab3f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J10-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "70aaed6e-3b2f-4ba4-814d-8adf28b08745")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J10-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "10277ada-05a4-4b6a-ba97-6b8dbc3abb50")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-Pin_4)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "3df9610a-cb55-4ce8-b56c-cdfd260b56b8")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.00mm:PinHeader_1x08_P2.00mm_Vertical"
		(layer "F.Cu")
		(uuid "a8b017b9-cef6-45cd-a9db-358070bd8994")
		(at 142.3 96)
		(descr "Through hole straight pin header, 1x08, 2.00mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.00mm single row")
		(property "Reference" "J5"
			(at 0 -2.06 0)
			(layer "F.SilkS")
			(uuid "41b2a500-2364-46a2-9735-45a6f5c1d117")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x08_Socket"
			(at 0 16.06 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1a6c5b72-bd19-41b7-a046-ae1085427746")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x08_P2.00mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cc21005a-7490-42bb-b480-d0c70d1f9086")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "83b2d6c7-abb2-4bad-9c08-70022d747b96")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f60b48c9-3f6e-4d52-9dd1-525002944d00")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/64b3d246-d3ed-4c94-aac8-918cb3b78399")
		(sheetname "Root")
		(sheetfile "andrew watering 8.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.06 -1.06)
			(end 0 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "668599e8-652d-4304-a4d5-23cc9e7a5802")
		)
		(fp_line
			(start -1.06 0)
			(end -1.06 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b415de8-7aea-415b-862a-1af439571f39")
		)
		(fp_line
			(start -1.06 1)
			(end -1.06 15.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea098e89-13b1-4b53-9893-f5835b0da1b0")
		)
		(fp_line
			(start -1.06 1)
			(end 1.06 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a19a7192-d2b5-4476-88d9-82646cc100a1")
		)
		(fp_line
			(start -1.06 15.06)
			(end 1.06 15.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb88ab61-7a96-4c4f-83c8-b72c289c12e2")
		)
		(fp_line
			(start 1.06 1)
			(end 1.06 15.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed4e9f1d-b64d-445b-97d0-ddce38babae4")
		)
		(fp_line
			(start -1.5 -1.5)
			(end -1.5 15.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f701ec39-3d5c-469b-8a2b-793d7848d0f3")
		)
		(fp_line
			(start -1.5 15.5)
			(end 1.5 15.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1edcf3fa-51ed-45cf-bf1a-ebbf8fbabdb7")
		)
		(fp_line
			(start 1.5 -1.5)
			(end -1.5 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "06fb78b9-0e48-4824-8294-065778948346")
		)
		(fp_line
			(start 1.5 15.5)
			(end 1.5 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "83fe1ea4-f00c-48f8-975d-e5093aaf9cc2")
		)
		(fp_line
			(start -1 -0.5)
			(end -0.5 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6fbae78-d055-4e85-bbeb-e4939e23e643")
		)
		(fp_line
			(start -1 15)
			(end -1 -0.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6655cc49-9fb0-46b6-9e5e-fc61346531c1")
		)
		(fp_line
			(start -0.5 -1)
			(end 1 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5bfcce41-cba0-4ac3-b47b-2f612bd7de82")
		)
		(fp_line
			(start 1 -1)
			(end 1 15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39379724-2b70-4554-90c9-9c48e56d03ea")
		)
		(fp_line
			(start 1 15)
			(end -1 15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5972ec2d-75b7-47b5-92c5-d16400b862f2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7 90)
			(layer "F.Fab")
			(uuid "2c37c109-f195-4e0a-a696-9cf6ad8bf35d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-Pin_4)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "00273192-c57a-4dcf-8b91-aa147c2d6e7c")
		)
		(pad "2" thru_hole oval
			(at 0 2)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J2-Pin_11)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "791241b4-717c-4889-974f-15a6888141fd")
		)
		(pad "3" thru_hole oval
			(at 0 4)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J2-Pin_10)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "47f436d2-4983-4e6f-b248-a940ab681e61")
		)
		(pad "4" thru_hole oval
			(at 0 6)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J1-Pin_5)")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "477323c1-e2ca-4976-8fe8-446ebf3b16a1")
		)
		(pad "5" thru_hole oval
			(at 0 8)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J2-Pin_12)")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "9bf10e54-839e-416d-a8d8-cf2796a7bc80")
		)
		(pad "6" thru_hole oval
			(at 0 10)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J1-Pin_12)")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "aa2eebbe-f1b6-4568-9a58-b0a40700f106")
		)
		(pad "7" thru_hole oval
			(at 0 12)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(J5-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive")
			(uuid "b2ea6ea9-9cf9-4f2c-8280-5b0cf52be8cf")
		)
		(pad "8" thru_hole oval
			(at 0 14)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-Pin_4)")
			(pinfunction "Pin_8")
			(pintype "passive")
			(uuid "0e5693df-2f3e-419d-bb59-1b915ec8c33d")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x08_P2.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "b4101766-9822-4fff-8cf7-bba8653a00aa")
		(at 114 81.66)
		(descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x12 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.77 0)
			(layer "F.SilkS")
			(uuid "0a6402e6-1383-4a34-b222-7ad1327c5df7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x12_Socket"
			(at 0 30.71 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d7e65be4-4769-4358-8032-e73e80626ca6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1a7efa18-a7d7-4224-bf6a-a7ba4acbb94e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ab3c86fb-f07c-4a46-85e8-d14668ae3bde")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x12, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "75762575-b7d8-4fc2-bfdb-696efaf1cdf1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/2375d38f-984f-4b34-8e93-85f83ea85eb1")
		(sheetname "Root")
		(sheetfile "andrew watering 8.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 29.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ce3dbb4-4ea1-4c73-a516-7b93353cd1e2")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.33 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f7f4b3cb-dd2d-4b4b-a174-e544c9486921")
		)
		(fp_line
			(start -1.33 29.27)
			(end 1.33 29.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2742cdc2-e128-4aa0-805a-2299c0ffbb0f")
		)
		(fp_line
			(start 0 -1.33)
			(end 1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97e7b232-fa0e-4796-94c1-d362dd46f11f")
		)
		(fp_line
			(start 1.33 -1.33)
			(end 1.33 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7be36021-cb8a-4e32-ab4a-c871f35e0767")
		)
		(fp_line
			(start 1.33 1.27)
			(end 1.33 29.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5ee8a724-5c8b-466c-9cb4-6a640af5a878")
		)
		(fp_line
			(start -1.8 -1.8)
			(end 1.75 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f9c4877-cfb2-4fd4-a5de-5940fbae529a")
		)
		(fp_line
			(start -1.8 29.7)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ac130e79-f45d-42e2-94fe-51b76924ddc5")
		)
		(fp_line
			(start 1.75 -1.8)
			(end 1.75 29.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0648a62c-065f-4c04-9eee-c433b07ef617")
		)
		(fp_line
			(start 1.75 29.7)
			(end -1.8 29.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d3915114-b026-4b9d-855f-782fa364acbb")
		)
		(fp_line
			(start -1.27 -1.27)
			(end 0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4c50d2f-a569-4bc5-86ce-6d9f703931ab")
		)
		(fp_line
			(start -1.27 29.21)
			(end -1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c24501b9-cd16-4f4c-acba-f01b0257851b")
		)
		(fp_line
			(start 0.635 -1.27)
			(end 1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d77542fc-50e5-45d4-8cd7-1d13286d1da5")
		)
		(fp_line
			(start 1.27 -0.635)
			(end 1.27 29.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dd706fce-3507-454d-9a1c-aec90da90988")
		)
		(fp_line
			(start 1.27 29.21)
			(end -1.27 29.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4672c991-8043-4726-8ed0-f413af109355")
		)
		(fp_text user "${REFERENCE}"
			(at 0 13.97 90)
			(layer "F.Fab")
			(uuid "a34bf7c2-9e1b-4909-9935-6bae43458030")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(J1-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "2e25ed94-cc8d-4b1a-8c92-8b2eab58aa26")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(J1-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "fdfcceff-5f9e-40bb-8ee5-10d9bf96ff15")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "unconnected-(J1-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "1d676b23-82aa-441d-bb09-7ed019851acf")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "9558807b-ff0d-4e3a-941a-230922fc00f0")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J1-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "9f70f2ac-a5dc-4cab-87b1-77e1fcebfa72")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "unconnected-(J1-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "0208d185-27b1-42b3-9287-165a6a740337")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(J1-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive")
			(uuid "c54bff62-5f53-4a86-854c-cbca6f74b177")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
			(uuid "73f01136-e571-4dcf-9fb9-fa734ded69ae")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J1-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
			(uuid "3a081eca-b485-4243-b155-fe068d207786")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J1-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
			(uuid "c8752cea-3eeb-490a-9696-82e2029b3d38")
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J1-Pin_11-Pad11)")
			(pinfunction "Pin_11")
			(pintype "passive")
			(uuid "4bdf54f4-6dd8-46d7-8997-78411c320688")
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J1-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
			(uuid "37c68583-d968-4aea-a923-7c33e91e3f5b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.00mm:PinHeader_1x08_P2.00mm_Vertical"
		(layer "F.Cu")
		(uuid "e09e8e93-b1f2-43bd-b80b-6180da09145d")
		(at 155 110 180)
		(descr "Through hole straight pin header, 1x08, 2.00mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.00mm single row")
		(property "Reference" "J6"
			(at 0 17 0)
			(layer "F.SilkS")
			(uuid "60a106df-bb54-446b-a416-5e2b92b92100")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x08_Socket"
			(at 0 16.06 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a77f9ab0-05cd-40f1-9474-8912d61c50b3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x08_P2.00mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1e97f2fd-1578-4d2a-9343-13e7f1d6f8b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e9d08323-eb6c-4763-9be1-5fca416475f3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2b697440-ab7f-4a38-9bd4-13d4d8c2d83a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/62529c29-7563-49a6-9de5-5d992baae838")
		(sheetname "Root")
		(sheetfile "andrew watering 8.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.06 1)
			(end 1.06 15.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5517b079-c57b-409f-a990-d8a29b4dec5f")
		)
		(fp_line
			(start -1.06 15.06)
			(end 1.06 15.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "da66a4ef-3735-44ce-8238-21dda6fd0df2")
		)
		(fp_line
			(start -1.06 1)
			(end 1.06 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "36a95993-8f65-4fd5-8904-ba2d32c3be48")
		)
		(fp_line
			(start -1.06 1)
			(end -1.06 15.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b9a32d8-9247-44d5-85ab-4e6e4385aabd")
		)
		(fp_line
			(start -1.06 0)
			(end -1.06 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "13633221-b1ea-401c-9694-31e270d4185b")
		)
		(fp_line
			(start -1.06 -1.06)
			(end 0 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "42d12fc8-6fa7-4a26-94ef-01d7efe2c02b")
		)
		(fp_line
			(start 1.5 15.5)
			(end 1.5 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1f0a33af-e898-4534-af6d-6673938e921c")
		)
		(fp_line
			(start 1.5 -1.5)
			(end -1.5 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f06ca5e8-7a4e-455e-b955-1a7fba180304")
		)
		(fp_line
			(start -1.5 15.5)
			(end 1.5 15.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e446f749-4447-4a58-96f0-f62930f4c2ff")
		)
		(fp_line
			(start -1.5 -1.5)
			(end -1.5 15.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "103f39d8-d037-480e-8ba6-22e5f36dfbb0")
		)
		(fp_line
			(start 1 15)
			(end -1 15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d60b1bbe-18ca-4800-a8f0-bbb276957a8c")
		)
		(fp_line
			(start 1 -1)
			(end 1 15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "613cbc1f-945b-492e-ad83-79b281eef899")
		)
		(fp_line
			(start -0.5 -1)
			(end 1 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e537c938-6c19-490b-a449-3cc23cb19c3f")
		)
		(fp_line
			(start -1 15)
			(end -1 -0.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d042160c-b878-488b-98b7-f0f441244708")
		)
		(fp_line
			(start -1 -0.5)
			(end -0.5 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c48e8566-1360-4616-b74e-ede3d5dcb6c4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7 90)
			(layer "F.Fab")
			(uuid "ca804612-e606-43e3-ba74-6890620cef07")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(J6-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "212875bf-ec69-4cac-abd8-1f7b59969c4c")
		)
		(pad "2" thru_hole oval
			(at 0 2 180)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-Pin_4)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "3a61c2a0-450f-4ce7-a9a7-4ce9ef1bdfd5")
		)
		(pad "3" thru_hole oval
			(at 0 4 180)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(J6-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "cb0d9127-5756-4064-8281-7cde6d354666")
		)
		(pad "4" thru_hole oval
			(at 0 6 180)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(J6-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "9a6eeb59-2fdd-4677-88b5-ef6a66ddccb4")
		)
		(pad "5" thru_hole oval
			(at 0 8 180)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(J6-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "3e8cf202-e314-4946-bf2d-976f6288f612")
		)
		(pad "6" thru_hole oval
			(at 0 10 180)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J1-Pin_5)")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "eaeeb921-10c3-4e08-a316-1f4b94023fbb")
		)
		(pad "7" thru_hole oval
			(at 0 12 180)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(J6-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive")
			(uuid "bae321ff-93e9-4ca7-b2a7-297354b9a2b2")
		)
		(pad "8" thru_hole oval
			(at 0 14 180)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(J6-Pin_8-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive")
			(uuid "24272a24-be82-4006-aa1c-e74c149785cf")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x08_P2.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "e46a410a-3cf5-4bb2-bb96-010afa79abb0")
		(at 95 99 180)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J4"
			(at 0 16.51 0)
			(layer "F.SilkS")
			(uuid "a5fafb42-ada0-48f9-a1a7-674c4f0957a9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x06_Socket"
			(at 0 15.47 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a852be10-666c-4667-afd4-4265e721a738")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f482d3c-e366-46ee-9643-fc8d9815f6d3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3346803e-e912-4e9a-a7e5-7fd6bdeb254f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "253bf881-ca32-439e-9498-5395c8717754")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/d4310be7-e182-4fb1-8237-db85118b9660")
		(sheetname "Root")
		(sheetfile "andrew watering 8.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 1.27)
			(end 1.33 14.03)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49bd1b5d-20fe-451e-9189-14b4c9a02c4c")
		)
		(fp_line
			(start 1.33 -1.33)
			(end 1.33 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e6bcfafd-fcfe-4ba7-b426-224b9bce4ba6")
		)
		(fp_line
			(start 0 -1.33)
			(end 1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5dfdcb60-e19f-4d76-bd7b-db9d5ca4e274")
		)
		(fp_line
			(start -1.33 14.03)
			(end 1.33 14.03)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c2b41e2-1120-4a6c-b152-d736417d9115")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.33 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9229f626-9822-4d90-ab2c-188c8e5db3e2")
		)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 14.03)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d52372c-2b6e-48b7-a31b-e5be50e7df6b")
		)
		(fp_line
			(start 1.75 14.45)
			(end -1.8 14.45)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5214ae89-a0e6-4490-a3b8-360e29c3a3bb")
		)
		(fp_line
			(start 1.75 -1.8)
			(end 1.75 14.45)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c284445-6be3-4225-88c5-44046dc574d2")
		)
		(fp_line
			(start -1.8 14.45)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "580d3ef6-7475-4f47-a0bb-bd4435473ab9")
		)
		(fp_line
			(start -1.8 -1.8)
			(end 1.75 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ae9b58b4-d3be-4274-8f4d-1fc452468a8f")
		)
		(fp_line
			(start 1.27 13.97)
			(end -1.27 13.97)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "518ec310-d661-468d-a369-81dbeca132a1")
		)
		(fp_line
			(start 1.27 -0.635)
			(end 1.27 13.97)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a0bf6b44-c601-4455-867f-df508c9d9938")
		)
		(fp_line
			(start 0.635 -1.27)
			(end 1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9e42b6d-072c-4da8-b2c6-494e3001f68b")
		)
		(fp_line
			(start -1.27 13.97)
			(end -1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ed29bcdc-686e-4378-8c29-4247ba65a4c9")
		)
		(fp_line
			(start -1.27 -1.27)
			(end 0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4c399f1-1649-4e32-b805-cc4a3b4e27c1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 6.7 90)
			(layer "F.Fab")
			(uuid "9cea7c60-11f5-485b-af88-bba67e97140e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(J4-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "e5cde3c6-8e60-476c-bed9-ff16b3019fd4")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(J4-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "c23e482a-70c5-4b03-89d4-b3c543e4fd88")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J4-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "33fb04be-057b-4678-9e48-75d3c795eb57")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J4-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "95e2386f-b1f6-442b-91d8-c8d4e00726ee")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-Pin_4)")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "38457661-0133-40cd-8b35-03fe4eb1ee69")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J4-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "f94a7861-c74b-4449-aa16-a4eb9fdd4f41")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "e7b39d4e-fc16-43f6-b1ca-f4f5850d2777")
		(at 105 99 180)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J3"
			(at 0 16.16 0)
			(layer "F.SilkS")
			(uuid "d6dd4831-7fc3-4c24-bd48-5ea0e4830b66")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x06_Socket"
			(at 0 15.47 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ebb563b9-2d95-456d-9543-43f3272a3a7b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e19a1087-71df-433d-aabe-22c1051a62cd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0c20f882-5aa4-4269-995e-dbc85398f1cc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "64a03ec9-5b5a-48e9-bd22-9541c1a9deea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/84e478da-a081-48b7-abd1-fa19c6e99790")
		(sheetname "Root")
		(sheetfile "andrew watering 8.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 1.27)
			(end 1.33 14.03)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0aa723b5-81cb-4ace-b77e-4c37daa51950")
		)
		(fp_line
			(start 1.33 -1.33)
			(end 1.33 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bc1ddeee-04b1-4949-8edf-aa126ee9bbbe")
		)
		(fp_line
			(start 0 -1.33)
			(end 1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c8739305-7b22-44ea-8b28-5dee0ba464dd")
		)
		(fp_line
			(start -1.33 14.03)
			(end 1.33 14.03)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4c850696-b402-4e3f-9ebc-81717fc16899")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.33 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bc4a770c-27ec-4452-a076-58183a2e4398")
		)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 14.03)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4039e6d7-76ff-439f-bab5-8d68539e0d2d")
		)
		(fp_line
			(start 1.75 14.45)
			(end -1.8 14.45)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "48551162-e33d-4cc7-9a55-3bbf4cf8da1d")
		)
		(fp_line
			(start 1.75 -1.8)
			(end 1.75 14.45)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "03f51251-1818-4883-9402-df1aebef4a03")
		)
		(fp_line
			(start -1.8 14.45)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f3ed161b-df24-43d6-8479-d1d66fc4d54f")
		)
		(fp_line
			(start -1.8 -1.8)
			(end 1.75 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4e33cb4-0f36-4000-9971-a0ca925abe4f")
		)
		(fp_line
			(start 1.27 13.97)
			(end -1.27 13.97)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ee4140e7-826b-4156-a33d-41adcbd7cc67")
		)
		(fp_line
			(start 1.27 -0.635)
			(end 1.27 13.97)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c32e8e1d-d125-45f4-9928-5062c8f80721")
		)
		(fp_line
			(start 0.635 -1.27)
			(end 1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa128378-075b-4d94-94ab-f662a97698eb")
		)
		(fp_line
			(start -1.27 13.97)
			(end -1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "291fc99d-382a-4387-a013-c82e8d69543e")
		)
		(fp_line
			(start -1.27 -1.27)
			(end 0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7bbee1c-bbfd-42aa-843d-4dc403116560")
		)
		(fp_text user "${REFERENCE}"
			(at 0 6.35 90)
			(layer "F.Fab")
			(uuid "e1fa54d2-3ef8-4bc4-87ce-f464529f6a82")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pin_8)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "28918144-4fa1-47ef-b3cf-b8c809254288")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(J3-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "7e970a11-7afc-4471-9499-7ea993ed6c6d")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J1-Pin_9)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "d286b602-0673-4120-abeb-d1542d0b43ef")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J1-Pin_10)")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "2b550b79-73ad-48f1-8d6e-731618c43846")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-Pin_4)")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "2adf1a0b-a226-499c-81e1-7a481da781b9")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(J3-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "188a4cae-e1de-4142-b8ee-1b472f565c53")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "e942eb89-0b48-4d36-bca8-12e16427fb64")
		(at 129 81.66)
		(descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x12 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.77 0)
			(layer "F.SilkS")
			(uuid "ab45a3da-7476-424d-bb77-9556709e4e63")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x12_Socket"
			(at 0 30.71 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "968ac759-af67-46d7-9630-8f52ea1c4c4f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7e87fb10-232e-40ce-8850-25ef70739069")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a8fa57a5-d354-4fe3-ac8d-3b2fd5d97c70")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x12, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dbb16d97-6170-4b65-9944-5643b5162a56")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/28d92331-e1ac-49ed-88e9-5d4e151fb7ea")
		(sheetname "Root")
		(sheetfile "andrew watering 8.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 29.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "46ca09ed-4248-4306-97a6-e4d3e1a4fc60")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.33 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4cbb3d76-5808-4353-a537-a1d1d133f4f9")
		)
		(fp_line
			(start -1.33 29.27)
			(end 1.33 29.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9192f46f-8e95-4f18-bab0-20ed4fab9d43")
		)
		(fp_line
			(start 0 -1.33)
			(end 1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6c1f4ff5-6c34-4c2f-8025-1d4a5cd9e6b5")
		)
		(fp_line
			(start 1.33 -1.33)
			(end 1.33 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10c8dc1d-f0e4-460f-8f42-443fa093cbd0")
		)
		(fp_line
			(start 1.33 1.27)
			(end 1.33 29.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f66c21c-56cf-4413-b333-62b3f7feed14")
		)
		(fp_line
			(start -1.8 -1.8)
			(end 1.75 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4d6c292e-1d18-43de-be68-2e336cda6e91")
		)
		(fp_line
			(start -1.8 29.7)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6e5974bb-6526-4efc-b2bf-aec20a54bb60")
		)
		(fp_line
			(start 1.75 -1.8)
			(end 1.75 29.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "68496b03-93cb-452d-b4c3-96a4de26880b")
		)
		(fp_line
			(start 1.75 29.7)
			(end -1.8 29.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0518362b-752b-4226-a4eb-10a5e88d853a")
		)
		(fp_line
			(start -1.27 -1.27)
			(end 0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9b647bf-2913-42f4-a326-98c243bab0d6")
		)
		(fp_line
			(start -1.27 29.21)
			(end -1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e9c342e-6940-452d-abb1-5ea9421b5761")
		)
		(fp_line
			(start 0.635 -1.27)
			(end 1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c6ee311-2b4a-48df-a52a-0567d5a21beb")
		)
		(fp_line
			(start 1.27 -0.635)
			(end 1.27 29.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c25095b-4a9b-4451-a697-f5ee52608e65")
		)
		(fp_line
			(start 1.27 29.21)
			(end -1.27 29.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ebc1e56-2f2f-4dfd-9386-296713b5e3ab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 13.97 90)
			(layer "F.Fab")
			(uuid "9b21c659-c51a-4881-b8df-c98509037f78")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(J2-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "aaca162e-8de9-483b-9d98-1069f4eb1efc")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-Pin_4)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "0d288b3d-a3bd-469b-a057-c16b9c7c288c")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(J2-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "d2f494cf-8f27-48e2-a73f-14298837409c")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J10-Pin_1)")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "894dfa0b-c48e-4d0a-8a27-85745e22cfc5")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(J2-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "7011b818-f8d1-40b0-b51e-8d93851773d3")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(J2-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "22ab95ce-d1b0-425b-acd0-4e0f5588025d")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J10-Pin_2)")
			(pinfunction "Pin_7")
			(pintype "passive")
			(uuid "5f83ee57-8507-43bb-aa7b-d2ded2232b97")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J2-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
			(uuid "a0920e30-a1e7-43bb-82b1-d69641308a1d")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J1-Pin_5)")
			(pinfunction "Pin_9")
			(pintype "passive")
			(uuid "e077f1b5-8a08-4efe-ae69-d8f2071aae8b")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J2-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
			(uuid "dc377cd1-5d20-4a68-a605-4beee0c58701")
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J2-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
			(uuid "12f7a9dc-13f4-419e-bdf1-e29bb2f88984")
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J2-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
			(uuid "721846e9-f60f-48a8-894e-ee77a3af27c0")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 134 104)
		(end 134 113)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 22)
		(uuid "04687396-1a18-48a4-8446-181d8744b43b")
	)
	(gr_line
		(start 109 75)
		(end 126 75)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 19)
		(uuid "1698e58d-3b77-4ed6-a593-ce6b9b55c2ab")
	)
	(gr_line
		(start 126 75)
		(end 126 100)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 19)
		(uuid "1dc4f108-1d7e-4b34-973c-fd12d3057319")
	)
	(gr_line
		(start 146 100)
		(end 142 100)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 22)
		(uuid "2baccab1-81f0-44eb-8edc-80f3f3c92f08")
	)
	(gr_line
		(start 146 113)
		(end 146 100)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 22)
		(uuid "4739f1c3-2015-406c-8758-393a1e3f9fbe")
	)
	(gr_line
		(start 132 107)
		(end 132 115)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 13)
		(uuid "49a9c82b-6f66-4cfd-b29f-ee645537c0a8")
	)
	(gr_line
		(start 132 115)
		(end 147 115)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 13)
		(uuid "6bf352d3-8e9f-4e74-ab82-ee0c05101b9c")
	)
	(gr_line
		(start 126 100)
		(end 129 100)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 19)
		(uuid "6f295870-a271-40f6-b57d-5eebf0c22291")
	)
	(gr_line
		(start 147 98)
		(end 147 115)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 13)
		(uuid "9e66bfe7-40fd-4ab9-99f4-60d8ba5765bf")
	)
	(gr_line
		(start 134 113)
		(end 146 113)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 22)
		(uuid "cd9ecfba-1a01-4bbe-b678-7ebc13697fe4")
	)
	(gr_line
		(start 143 98)
		(end 147 98)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 13)
		(uuid "ee92624d-8c89-4269-a6dd-60c155ae1acf")
	)
	(gr_line
		(start 129 104)
		(end 134 104)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 22)
		(uuid "f10d1529-f399-48ee-a793-049261a35e4f")
	)
	(gr_line
		(start 129 107)
		(end 132 107)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 13)
		(uuid "f700d646-8e33-4842-a6e4-6dd720165aa8")
	)
	(gr_line
		(start 95 89)
		(end 95 88)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Cu")
		(net 8)
		(uuid "fc815eb4-5dc7-4654-8ea4-b95e52a51f83")
	)
	(gr_line
		(start 133 97)
		(end 133 92)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 15)
		(uuid "084dbb45-1bd4-4a75-ad51-cc62c436cb81")
	)
	(gr_line
		(start 136 94)
		(end 139 94)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "099ba2f4-844c-4dae-838b-489c22076bc4")
	)
	(gr_line
		(start 147 96)
		(end 147 84)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "0eb44230-4dd2-4644-82e9-be99a4df3920")
	)
	(gr_line
		(start 109 75)
		(end 109 79)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 19)
		(uuid "12ec3a7c-77fe-4c23-b146-838982aa629c")
	)
	(gr_line
		(start 138 114)
		(end 140 114)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 4)
		(uuid "139e1b6a-919b-4083-870d-8252987c0f5c")
	)
	(gr_line
		(start 142 102)
		(end 155 100)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 9)
		(uuid "16a99db0-5841-4ddc-9adf-f5b28e3a6889")
	)
	(gr_line
		(start 122 114)
		(end 138 114)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 4)
		(uuid "18803232-b2f2-4fcf-b604-398f9d4911c2")
	)
	(gr_line
		(start 157 108)
		(end 155 108)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "1b14b412-eda1-4caa-ba65-94d889030110")
	)
	(gr_line
		(start 140 114)
		(end 140 106)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 4)
		(uuid "1cc24a4a-6f41-4410-a522-b81dd3d811ab")
	)
	(gr_line
		(start 96 82)
		(end 99 82)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "246439f5-c99f-487b-a0e9-568824b1ead3")
	)
	(gr_line
		(start 138 104)
		(end 142.5 104)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 17)
		(uuid "2492462c-3618-46b0-89b1-cf06cf274ad9")
	)
	(gr_line
		(start 102 94)
		(end 102 102)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 5)
		(uuid "254d9106-be3c-472f-95da-fbe03367339e")
	)
	(gr_line
		(start 133 92)
		(end 136 92)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 15)
		(uuid "26217275-a553-4c97-804e-2d121ea31a8c")
	)
	(gr_line
		(start 99 82)
		(end 99 89)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "28619748-afa3-4b04-a3ce-f3ea2c1741c5")
	)
	(gr_line
		(start 129 109)
		(end 129 110)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 17)
		(uuid "2d6affa3-6f05-472d-bbec-44ae1a553288")
	)
	(gr_line
		(start 125 92)
		(end 125 102)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 9)
		(uuid "407e1cc6-4071-4818-a39b-d8c06e88bc42")
	)
	(gr_line
		(start 105 94)
		(end 102 94)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 5)
		(uuid "462e61c3-a262-4593-999a-b8dea67d7770")
	)
	(gr_line
		(start 97 79)
		(end 96 79)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "49845b4e-d17d-4709-9b22-13837b5adeb1")
	)
	(gr_line
		(start 114 109)
		(end 118 109)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 4)
		(uuid "49b5b30e-7b1b-470e-8f71-1290d138a31d")
	)
	(gr_line
		(start 129 97)
		(end 133 97)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 15)
		(uuid "5155e4f7-23fe-48bb-aed0-dd86563b9ddd")
	)
	(gr_line
		(start 142 104)
		(end 143 104)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 17)
		(uuid "5783fb12-5e9f-4711-975f-8fd187eb8918")
	)
	(gr_line
		(start 87 86)
		(end 95 86)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 29)
		(uuid "5b577a0d-53ee-44f6-b62c-73cfcca21930")
	)
	(gr_line
		(start 129 84)
		(end 145 84)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "6b67c4b7-1392-4297-ae2a-036c9a7a4bed")
	)
	(gr_line
		(start 139 94)
		(end 139 84)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "6d1c317d-1d07-44d7-b5b2-4ce6a7031f2c")
	)
	(gr_line
		(start 145 84)
		(end 157 84)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "70c0907f-916e-484b-92bb-386e1cadec06")
	)
	(gr_line
		(start 129 89)
		(end 136 89)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 18)
		(uuid "74e3afa1-fbaa-484b-973b-460cb5f6808c")
	)
	(gr_line
		(start 118 89)
		(end 125 89)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "776f23d8-33af-4ae0-aeb1-8b550d654f5f")
	)
	(gr_line
		(start 96 79)
		(end 96 82)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "81f81ad6-f4e9-4f2d-9ddf-ee3a91fa79a5")
	)
	(gr_line
		(start 105 99)
		(end 114 99)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 7)
		(uuid "83b9a760-1157-41d1-bb47-aae79fa4501b")
	)
	(gr_line
		(start 157 84)
		(end 157 108)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "a073b663-797d-4c8a-aa5e-dfb6646e7ff9")
	)
	(gr_line
		(start 118 109)
		(end 122 109)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 4)
		(uuid "a64814d6-7dda-4387-a206-3bb4cb8ba60f")
	)
	(gr_line
		(start 95 89)
		(end 97 89)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "a9eb6b25-15ea-4894-91f3-6296e62c34aa")
	)
	(gr_line
		(start 102 102)
		(end 114 102)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 5)
		(uuid "ac63e416-987b-426c-bb36-771fe1d4eb07")
	)
	(gr_line
		(start 140 106)
		(end 142 106)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 4)
		(uuid "ac6fa8c3-486e-4e4f-8dde-0e8d1f8227c9")
	)
	(gr_line
		(start 114 92)
		(end 125 92)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 9)
		(uuid "ae917f55-7c97-44c5-ab6a-33b7dc247119")
	)
	(gr_line
		(start 122 109)
		(end 122 114)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 4)
		(uuid "b0972333-599e-444c-b323-4e48b13d8b26")
	)
	(gr_line
		(start 87 93)
		(end 95 91)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 26)
		(uuid "b10a0968-cc8f-4298-8335-5bbee510cb79")
	)
	(gr_line
		(start 129 102)
		(end 142 102)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 9)
		(uuid "b2c3d157-be41-4644-9af3-b6ef3c7a8b86")
	)
	(gr_line
		(start 101 104)
		(end 114 104)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 11)
		(uuid "b471b2ef-c366-4443-9118-c2f7d9c18d76")
	)
	(gr_line
		(start 125 84)
		(end 129 84)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "b8d60966-8375-412e-b09b-88b532de0cc0")
	)
	(gr_line
		(start 125 89)
		(end 125 84)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "c28c5dc3-1f7c-487e-ac5f-881629415d93")
	)
	(gr_line
		(start 142 110)
		(end 155 108)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "cff67d5e-54c3-4a0d-a5d8-5194e6be3be5")
	)
	(gr_line
		(start 87 89)
		(end 95 89)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "d61ec2da-6415-4c98-8c5d-19558eb9b46c")
	)
	(gr_line
		(start 105 89)
		(end 118 89)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "d8f252fa-3c93-4a04-a0e1-3bd0935f1d12")
	)
	(gr_line
		(start 125 102)
		(end 129 102)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 9)
		(uuid "dd89650f-93d7-495d-916c-796ec957493d")
	)
	(gr_line
		(start 136 94)
		(end 137.5 94)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "ec78281e-aaa9-4fa2-b996-b9258b351408")
	)
	(gr_line
		(start 129 109.5)
		(end 138 104)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 17)
		(uuid "ecd8f550-5a53-4fe0-b773-4743776ef947")
	)
	(gr_line
		(start 136 94)
		(end 136 95)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "ee6e0b55-5331-42d4-8852-949da10c43db")
	)
	(gr_line
		(start 142 96)
		(end 147 96)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "efc8c60e-20b7-4b93-8294-6dddf0911c37")
	)
	(gr_line
		(start 101 91)
		(end 101 104)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 11)
		(uuid "f133234d-294b-484a-b4ee-ac8b05c41c59")
	)
	(gr_line
		(start 89 75)
		(end 96 75)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 37)
		(uuid "f1ed816e-eb8c-45e8-bd3c-3e984c89483a")
	)
	(gr_line
		(start 89 78)
		(end 97 79)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "f4133dcf-8aac-4900-85d7-09d4859f324b")
	)
	(gr_line
		(start 95 89)
		(end 105 89)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 8)
		(uuid "f6b859e3-f78f-4af9-88dd-f4b72e66e5f3")
	)
	(gr_line
		(start 105 91)
		(end 101 91)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 11)
		(uuid "f9d9ec8f-bfd7-446c-be80-2d5ee8f14666")
	)
	(gr_line
		(start 87 96)
		(end 95 94)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "B.Cu")
		(net 25)
		(uuid "fe6c9b08-8b31-4d5c-b044-43b0f3fd8f62")
	)
	(gr_rect
		(start 80 70)
		(end 160 124)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "Edge.Cuts")
		(uuid "b39678b1-a82d-4d61-abfd-20d817a1da36")
	)
	(gr_text "Motor"
		(at 97 104 0)
		(layer "F.Cu")
		(uuid "1a6e47da-2a80-4821-a957-aa0b7d872f2c")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "sensor"
		(at 139 92 0)
		(layer "F.Cu")
		(uuid "3043ce00-efbc-460f-a89e-e63905b57aed")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "arduino"
		(at 118 114 0)
		(layer "F.Cu")
		(uuid "32f7b27f-096e-4646-a792-86beaf0f6996")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "moisture"
		(at 138 90 0)
		(layer "F.Cu")
		(uuid "3372f332-41df-4bfe-a480-4d4be94a8ca1")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "Control"
		(at 96 107 0)
		(layer "F.Cu")
		(uuid "3ed46e41-2942-40bf-a289-55c048c73b7c")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "Vin"
		(at 81 87 0)
		(layer "F.Cu")
		(uuid "8c71a8c8-4cbc-4645-abad-d209b1979b46")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "Gnd"
		(at 82 79.46 0)
		(layer "F.Cu")
		(uuid "9148b641-763d-4f53-a45e-4f2e566dd575")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "RFM95"
		(at 146 118 0)
		(layer "F.Cu")
		(uuid "a941598b-6f9d-452e-8146-ced938227be4")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "Pro Mini"
		(at 117 116 0)
		(layer "F.Cu")
		(uuid "af9df3fd-73f6-429f-ab20-3f076226fe9f")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "motor"
		(at 84 98 90)
		(layer "F.Cu")
		(uuid "c14198c4-71c1-4bde-944c-6d10ea9f38f2")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "Gnd"
		(at 81 90 0)
		(layer "F.Cu")
		(uuid "df726b9a-7606-41f6-a7a8-4ff2e81f6de2")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "Batt"
		(at 82 76 0)
		(layer "F.Cu")
		(uuid "e22444d2-7c6b-45eb-a057-732308575da2")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(segment
		(start 115.193654 89)
		(end 118 89)
		(width 0.2)
		(layer "B.Cu")
		(net 8)
		(uuid "4ee45c59-db8d-4a90-8c6a-41353b70cb21")
	)
)
