(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(D1-A)")
	(net 2 "GND")
	(net 3 "Net-(A1-PadA0)")
	(net 4 "unconnected-(A1-PadD7)")
	(net 5 "Net-(A1-D13_SCK)")
	(net 6 "unconnected-(U1-GND-Pad8)")
	(net 7 "Net-(A1-D3_INT1)")
	(net 8 "unconnected-(U1-DIO3-Pad11)")
	(net 9 "unconnected-(U1-3.3V-Pad13)")
	(net 10 "Net-(A1-D10_CS)")
	(net 11 "Net-(A1-D2_INT0)")
	(net 12 "Net-(A1-D11_MOSI)")
	(net 13 "unconnected-(U1-GND-Pad1)")
	(net 14 "unconnected-(U1-GND-Pad10)")
	(net 15 "unconnected-(U1-DIO2-Pad16)")
	(net 16 "Net-(U1-RESET)")
	(net 17 "unconnected-(U1-DIO5-Pad7)")
	(net 18 "Net-(A1-D12_MISO)")
	(net 19 "unconnected-(U1-DIO4-Pad12)")
	(net 20 "unconnected-(A1-PadTXO)")
	(net 21 "Net-(MP1-IN2)")
	(net 22 "unconnected-(A1-PadA7)")
	(net 23 "Net-(J1-Pin_2)")
	(net 24 "unconnected-(A1-A5{slash}SCL-PadA5)")
	(net 25 "Net-(J1-Pin_1)")
	(net 26 "unconnected-(A1-Vcc-PadVcc2)")
	(net 27 "unconnected-(A1-PadA6)")
	(net 28 "unconnected-(A1-PadA3)")
	(net 29 "unconnected-(A1-~{DTR}-PadDTR)")
	(net 30 "unconnected-(A1-GND-PadGND5)")
	(net 31 "+BATT")
	(net 32 "Net-(MP1-nSLEEP_HB)")
	(net 33 "unconnected-(A1-GND-PadGND4)")
	(net 34 "Net-(MP1-IN1)")
	(net 35 "unconnected-(A1-A4{slash}SDA-PadA4)")
	(net 36 "unconnected-(A1-RESET-PadRST2)")
	(net 37 "unconnected-(A1-PadD8)")
	(net 38 "unconnected-(A1-PadRXI)")
	(net 39 "unconnected-(A1-D0{slash}RX-PadD0)")
	(net 40 "unconnected-(A1-GND-PadGND2)")
	(net 41 "unconnected-(A1-PadA2)")
	(net 42 "unconnected-(A1-RESET-PadRST1)")
	(net 43 "unconnected-(A1-D1{slash}TX-PadD1)")
	(net 44 "Net-(AE1-A)")
	(net 45 "Net-(M1-+)")
	(net 46 "Net-(M1--)")
	(net 47 "unconnected-(MP1-GND-Pad11)")
	(net 48 "unconnected-(MP1-VM-Pad1)")
	(net 49 "unconnected-(MP1-VISEN-Pad5)")
	(net 50 "unconnected-(MP1-ISET-Pad8)")
	(net 51 "unconnected-(MP1-V3P3-Pad7)")
	(footprint "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(uuid "3c23dbe1-ee0c-4f70-9437-29c8373abcc2")
		(at 57 82.96 90)
		(descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH vertical")
		(property "Reference" "M1"
			(at 1.25 -2.8 90)
			(layer "F.SilkS")
			(uuid "8c19fc6a-5fea-4790-b409-26e88ec83bc7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Motor_DC"
			(at 1.25 3.4 90)
			(layer "F.Fab")
			(uuid "0de03fe6-4f33-4226-8ef0-13446e354179")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0bffd24-5ef8-4ccb-81d7-ac16c4ca1140")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "00c0aa4c-c978-4705-b60e-a58ffcca0e44")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Motor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "39e070fc-2a28-4185-b464-7cf7246169f8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "PinHeader*P2.54mm* TerminalBlock*")
		(path "/877fcaa7-a06e-4def-936e-87f6bdceb164")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 5.11 -1.71)
			(end -2.61 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5db46407-fcf3-450c-a420-713c777ec99b")
		)
		(fp_line
			(start -2.61 -1.71)
			(end -2.61 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7e91682-5043-4a36-8318-b4799fdc448f")
		)
		(fp_line
			(start 4.61 -1.21)
			(end 4.61 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97e8a372-e5ed-4d09-a4ed-8be4f136ce0d")
		)
		(fp_line
			(start -2.11 -1.21)
			(end 4.61 -1.21)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b9a9351e-abfc-4a14-b59d-c53106fb04bb")
		)
		(fp_line
			(start 4.61 0)
			(end 5.11 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e95e9964-599a-48be-9df8-2903f57ee7b5")
		)
		(fp_line
			(start -2.11 0)
			(end -2.11 -1.21)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f4ac9c96-0705-44e5-a172-572d57d619e5")
		)
		(fp_line
			(start -2.61 0)
			(end -2.11 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d6b047f-f529-46dc-b50b-443abdd65fa3")
		)
		(fp_line
			(start -2.91 0.11)
			(end -2.91 2.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6827f383-624d-469e-ad50-f4a4f952c1c4")
		)
		(fp_line
			(start 5.11 0.81)
			(end 4.11 0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "54607380-91e2-4fb1-abd2-910637d92a5e")
		)
		(fp_line
			(start 4.11 0.81)
			(end 4.11 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c8b7ce8d-8081-4024-9946-4fc29c5c3a43")
		)
		(fp_line
			(start -1.61 0.81)
			(end -1.61 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "93ce87a4-43cc-4a66-9054-c1e49f59a9ec")
		)
		(fp_line
			(start -2.61 0.81)
			(end -1.61 0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "131210d8-8ab9-4025-8851-363e8079c412")
		)
		(fp_line
			(start 5.11 2.31)
			(end 5.11 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3a0cd983-d8df-4971-848f-9ee8965c66c3")
		)
		(fp_line
			(start -2.61 2.31)
			(end 5.11 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e5557b44-cb04-4323-bdba-44a3fec9fe31")
		)
		(fp_line
			(start -2.91 2.61)
			(end -0.41 2.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "af5db4d1-9cd1-4ada-95ac-21978f2c5eaa")
		)
		(fp_line
			(start 5.5 -2.1)
			(end -3 -2.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "05174474-ff96-4bff-8cff-aff7404d14e6")
		)
		(fp_line
			(start -3 -2.1)
			(end -3 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b7757527-dbb2-4b5a-8155-27b916e3f6a6")
		)
		(fp_line
			(start 5.5 2.7)
			(end 5.5 -2.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ceed186b-4a7d-4039-8ad6-888c8151bd83")
		)
		(fp_line
			(start -3 2.7)
			(end 5.5 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d07551ad-ba12-4d73-8fbe-e0985bc7fdd1")
		)
		(fp_line
			(start 5 -1.6)
			(end -2.5 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91f0c95d-7011-4fa7-86f7-e6e8f1d79c1e")
		)
		(fp_line
			(start -2.5 -1.6)
			(end -2.5 2.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf4cb1a1-df81-47da-944e-ab548abac5ab")
		)
		(fp_line
			(start -2.91 0.11)
			(end -2.91 2.61)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2fd3542d-d303-40b6-b1ad-697a0b47159e")
		)
		(fp_line
			(start 5 2.2)
			(end 5 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "299a66a4-f46b-422f-b9a8-48c01416d5b9")
		)
		(fp_line
			(start -2.5 2.2)
			(end 5 2.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b5dc93b7-b652-4c24-a16c-5f75f9892395")
		)
		(fp_line
			(start -2.91 2.61)
			(end -0.41 2.61)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f606d564-64d7-4445-9bd9-6ee969ef6242")
		)
		(fp_text user "${REFERENCE}"
			(at 1.25 1.5 90)
			(layer "F.Fab")
			(uuid "038d8b73-309e-44fc-aed1-7dcebef26255")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 45 "Net-(M1-+)")
			(pinfunction "+")
			(pintype "passive")
			(uuid "a256a6b4-b287-4413-a86e-8423521302be")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 46 "Net-(M1--)")
			(pinfunction "-")
			(pintype "passive")
			(uuid "feb3c5bc-4fc9-476f-9b5d-0aab4a52dca3")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(uuid "4613e042-980c-493e-bfc6-db60fca4675b")
		(at 120.7 66.75 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 5.25 2.7 90)
			(layer "F.SilkS")
			(uuid "1a95bc1c-9e99-44d2-a4a7-2411290b1e7e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "R"
			(at 5.08 2.37 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "a1511fd1-bf23-4e24-8f1b-e20ff5e7ec7e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "28a525f3-691f-4cda-a3f9-6ec724704aad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fcaa7dc0-43a0-4add-b990-64732e77e9fa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "781de4c7-a77a-4aa1-8e4f-8e79d3e4a957")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/43d6cde2-eb8d-492c-be49-0ec094214f1c")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.81 1.37)
			(end 8.35 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "756af00e-0c24-42ac-afd4-611b01cadc41")
		)
		(fp_line
			(start 8.35 1.37)
			(end 8.35 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "efa6ab78-9e57-449f-b006-34aff155058d")
		)
		(fp_line
			(start 1.04 0)
			(end 1.81 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84e9ff41-444e-42ba-91d5-4ebe4bbf7577")
		)
		(fp_line
			(start 9.12 0)
			(end 8.35 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b4f96422-1f79-41c9-826f-84fc72e9bff5")
		)
		(fp_line
			(start 1.81 -1.37)
			(end 1.81 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1bdd23e6-e574-46bd-be06-1cfe15f48ad4")
		)
		(fp_line
			(start 8.35 -1.37)
			(end 1.81 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd00fc42-cba2-44db-8bb6-b8f97675b7aa")
		)
		(fp_line
			(start -1.05 1.5)
			(end 11.21 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0dab500e-e12d-4b9d-b5c3-65e29d30b02c")
		)
		(fp_line
			(start 11.21 1.5)
			(end 11.21 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ecefd1f6-1f64-4f89-9939-34ec5b12343d")
		)
		(fp_line
			(start -1.05 -1.5)
			(end -1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4408b462-36fb-4f6b-814a-fb4dd2a627b8")
		)
		(fp_line
			(start 11.21 -1.5)
			(end -1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a424956d-d745-4f95-a31c-14e2fc97a7b7")
		)
		(fp_line
			(start 1.93 1.25)
			(end 8.23 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "06fd27a9-05e4-4d6a-98a2-b35fb24b44ea")
		)
		(fp_line
			(start 8.23 1.25)
			(end 8.23 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d94a84c5-d31c-45a8-aed8-e7927ad907ca")
		)
		(fp_line
			(start 0 0)
			(end 1.93 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e2e7d5fe-43d6-4af1-8a3f-5327e0fd749f")
		)
		(fp_line
			(start 10.16 0)
			(end 8.23 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1302f5c0-d6ec-4311-9154-639b9e76b26d")
		)
		(fp_line
			(start 1.93 -1.25)
			(end 1.93 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "85fe0c98-f008-41bb-96fa-81efb8f9af8c")
		)
		(fp_line
			(start 8.23 -1.25)
			(end 1.93 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3716c769-1a2a-487f-8997-852d70636375")
		)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
			(uuid "d9d90f77-c062-4c5c-aa57-226a33296e04")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 3 "Net-(A1-PadA0)")
			(pintype "passive")
			(uuid "7bde05a9-ed28-4460-ac13-d5fd22d0e769")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "cc8be5e6-ca57-4ec4-83e6-6904afebe5ae")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_arduino-library:Arduino_Pro_Mini_Socket"
		(layer "F.Cu")
		(uuid "4db682e9-ff26-4d31-9efd-6aa2d190b0aa")
		(at 97.12 75.08)
		(descr "https://docs.arduino.cc/retired/boards/arduino-pro-mini")
		(property "Reference" "A1"
			(at -6.858 -17.526 0)
			(layer "F.SilkS")
			(uuid "7ee9c547-9814-417c-9514-5526d4d0c1c4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Arduino_Pro_Mini_Socket"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "a6947628-59d9-4dc8-83c0-0ee71789063e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_arduino-library:Arduino_Pro_Mini_Socket"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9ccbdd3b-0f80-428f-ab48-04deb799db59")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://docs.arduino.cc/retired/boards/arduino-pro-mini"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9dfa2148-f398-4f65-ad2e-93ad18e8d942")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Socket for Arduino Pro Mini"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2d3d7784-58b6-4cea-a37d-6a0430c245c2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Arduino_Pro_Mini_Socket")
		(path "/83c054f9-a0e0-4986-ada7-8460c49a3455")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -8.89 -16.51)
			(end -8.89 16.51)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2e6f5e2a-22c7-4b5e-860d-88340c056828")
		)
		(fp_line
			(start 8.89 -16.51)
			(end -8.89 -16.51)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "76d05282-b574-4519-821b-6e32d342da13")
		)
		(fp_line
			(start 8.89 -16.51)
			(end 8.89 16.51)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22aaf491-c047-4c2b-b8b0-9487784491c9")
		)
		(fp_line
			(start 8.89 16.51)
			(end -8.89 16.51)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2d71810f-a9f7-4505-a2c0-7a4371981161")
		)
		(fp_line
			(start -9.144 -16.764)
			(end 9.144 -16.764)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b6fb28f1-79c8-4dda-8527-5c7d40aa6a34")
		)
		(fp_line
			(start -9.144 16.764)
			(end -9.144 -16.764)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "154468a2-7961-4407-ad00-2788e2c99693")
		)
		(fp_line
			(start 9.144 -16.764)
			(end 9.144 16.764)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "68e87610-a3f6-4a5f-aa98-e5216ce0a82c")
		)
		(fp_line
			(start 9.144 16.764)
			(end -9.144 16.764)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "55c37486-359c-43c3-a6b5-167335d2adbf")
		)
		(fp_line
			(start -8.89 -13.97)
			(end -8.89 16.51)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c49c9bf0-a1de-40c5-ae01-f21912865dbe")
		)
		(fp_line
			(start -8.89 -13.97)
			(end -7.62 -13.97)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e78bef53-1724-4cea-8f3e-3007f5a065aa")
		)
		(fp_line
			(start -8.89 16.51)
			(end -6.35 16.51)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "352028f1-e65c-4bf5-b87e-891f8ac533d3")
		)
		(fp_line
			(start -7.62 -16.51)
			(end -7.62 -13.97)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "71aa46cb-13ee-480a-9d01-9a31d8d19637")
		)
		(fp_line
			(start -7.62 -16.51)
			(end 7.62 -16.51)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63a7197d-1f94-4fcf-bf15-cbccfb58f40b")
		)
		(fp_line
			(start -6.35 -13.97)
			(end -6.35 16.51)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4583d2de-51a2-4ee0-9104-8efa7f04fba9")
		)
		(fp_line
			(start -6.35 -13.97)
			(end 6.35 -13.97)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c3b3487-60df-4c91-8de0-98a5f062b53f")
		)
		(fp_line
			(start 3.4241 -5.1994)
			(end 3.4241 -0.1194)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e3a6d5a-b0f7-4053-9ef4-19ac51a262c7")
		)
		(fp_line
			(start 3.4241 -0.1194)
			(end 5.9641 -0.1194)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6128d3b9-ec18-48c9-ab1d-c7ae8e57dfa6")
		)
		(fp_line
			(start 3.4241 5.214)
			(end 3.4241 10.2946)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3bff2262-030d-401f-9b87-2abaef92a268")
		)
		(fp_line
			(start 5.9641 -5.1994)
			(end 3.4241 -5.1994)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b89b7a1c-e6b1-4613-8073-9148cc95ab76")
		)
		(fp_line
			(start 5.9641 -5.1994)
			(end 5.9641 -0.1194)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "008448d5-c0b0-4e8c-8cf2-bb3ba9426bd4")
		)
		(fp_line
			(start 5.9641 5.214)
			(end 3.4241 5.214)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ca242d3-5e84-42e8-933e-d2cb15e0ab35")
		)
		(fp_line
			(start 5.9641 5.214)
			(end 5.9641 10.2946)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3698985a-ecd5-47ba-b7bf-648bbaec60c5")
		)
		(fp_line
			(start 5.9641 10.2946)
			(end 3.4241 10.2946)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53229112-e816-49b0-838f-2a382ba88829")
		)
		(fp_line
			(start 6.35 -13.97)
			(end 6.35 16.51)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9698211e-80f8-443d-b123-9f4552c25889")
		)
		(fp_line
			(start 6.35 16.51)
			(end 8.89 16.51)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "78b5b7ee-c2d9-48e8-8ed6-082a98fd795b")
		)
		(fp_line
			(start 7.62 -16.51)
			(end 7.62 -13.97)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c96d9fb0-c77d-4a8a-8812-8900d3089ab1")
		)
		(fp_line
			(start 7.62 -13.97)
			(end 8.89 -13.97)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5cb5530b-3192-4d7b-8134-7f99960d6529")
		)
		(fp_line
			(start 8.89 -13.97)
			(end 8.89 16.51)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "117b7b99-8ff6-4438-a5af-8461c00e4603")
		)
		(fp_text user "D0"
			(at -5.715 -10.16 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(uuid "c231d881-a752-476d-a268-29407ac36a0e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(fp_text user "D0"
			(at -5.715 -10.16 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "39913e98-4cc0-4ab0-ba26-7fc1dafd00e6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "BLK"
			(at -8.255 -15.24 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "4e1512a2-9758-476d-abeb-0649a0695eff")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.08)
				)
			)
		)
		(fp_text user "GRN"
			(at 8.255 -15.24 90)
			(layer "F.SilkS")
			(uuid "be2d1c15-202e-4c47-b4ca-cb1a457bc4a6")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.08)
				)
			)
		)
		(pad "A0" thru_hole circle
			(at 7.62 5.08)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 3 "Net-(A1-PadA0)")
			(pinfunction "A0")
			(pintype "bidirectional")
			(uuid "97e14d1f-2f96-4ef7-95a5-9171ee84c5ca")
		)
		(pad "A1" thru_hole circle
			(at 7.62 2.54)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 23 "Net-(J1-Pin_2)")
			(pinfunction "A1")
			(pintype "bidirectional")
			(uuid "40293fbf-32e5-459e-954e-1fd2583fe8c2")
		)
		(pad "A2" thru_hole circle
			(at 7.62 0)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 41 "unconnected-(A1-PadA2)")
			(pinfunction "A2")
			(pintype "bidirectional")
			(uuid "d9eb656b-89af-4768-a457-fc5a7c1b7621")
		)
		(pad "A3" thru_hole circle
			(at 7.62 -2.54)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 28 "unconnected-(A1-PadA3)")
			(pinfunction "A3")
			(pintype "bidirectional")
			(uuid "66f5a55c-9b0f-4ef4-b513-a75ced33672a")
		)
		(pad "A4" thru_hole circle
			(at 4.6941 -1.3894)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 35 "unconnected-(A1-A4{slash}SDA-PadA4)")
			(pinfunction "A4/SDA")
			(pintype "bidirectional")
			(uuid "a9597dda-1c0e-4990-9636-7a11d3012034")
		)
		(pad "A5" thru_hole circle
			(at 4.6941 -3.9294)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 24 "unconnected-(A1-A5{slash}SCL-PadA5)")
			(pinfunction "A5/SCL")
			(pintype "bidirectional")
			(uuid "44a54870-abf2-4751-86a4-49b08d038263")
		)
		(pad "A6" thru_hole circle
			(at 4.6941 9.0246)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 27 "unconnected-(A1-PadA6)")
			(pinfunction "A6")
			(pintype "input")
			(uuid "64c69975-15e8-41f7-beeb-bbb5de85d20c")
		)
		(pad "A7" thru_hole circle
			(at 4.6941 6.484)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 22 "unconnected-(A1-PadA7)")
			(pinfunction "A7")
			(pintype "input")
			(uuid "2ebd6e0d-00d0-4a10-9095-51ad9e92283d")
		)
		(pad "D0" thru_hole circle
			(at -7.62 -10.16)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 39 "unconnected-(A1-D0{slash}RX-PadD0)")
			(pinfunction "D0/RX")
			(pintype "bidirectional")
			(uuid "b4c3378b-21fb-4291-9a7c-807decadd2de")
		)
		(pad "D1" thru_hole circle
			(at -7.62 -12.7)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 43 "unconnected-(A1-D1{slash}TX-PadD1)")
			(pinfunction "D1/TX")
			(pintype "bidirectional")
			(uuid "ec1fe6da-234d-47b0-8489-b4c15a4212a4")
		)
		(pad "D2" thru_hole circle
			(at -7.62 -2.54)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 11 "Net-(A1-D2_INT0)")
			(pinfunction "D2_INT0")
			(pintype "bidirectional")
			(uuid "d4e1dd9e-88a8-4eab-9d7d-6ef49e34101b")
		)
		(pad "D3" thru_hole circle
			(at -7.62 0)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "Net-(A1-D3_INT1)")
			(pinfunction "D3_INT1")
			(pintype "bidirectional")
			(uuid "9ddbf890-1ff5-4639-982a-e6841601ccc9")
		)
		(pad "D4" thru_hole circle
			(at -7.62 2.54)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 32 "Net-(MP1-nSLEEP_HB)")
			(pinfunction "D4")
			(pintype "bidirectional")
			(uuid "4a142c3f-18df-4035-b096-fa52094e5819")
		)
		(pad "D5" thru_hole circle
			(at -7.62 5.08)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 34 "Net-(MP1-IN1)")
			(pinfunction "D5")
			(pintype "bidirectional")
			(uuid "979c3ce0-9ec5-4049-8320-fcad06bd7b16")
		)
		(pad "D6" thru_hole circle
			(at -7.62 7.62)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 21 "Net-(MP1-IN2)")
			(pinfunction "D6")
			(pintype "bidirectional")
			(uuid "9d4b1bbe-a317-4222-a95e-0e3fbe85f7a5")
		)
		(pad "D7" thru_hole circle
			(at -7.62 10.16)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 4 "unconnected-(A1-PadD7)")
			(pinfunction "D7")
			(pintype "bidirectional")
			(uuid "1217c39d-64af-497f-993e-fe650ece85e1")
		)
		(pad "D8" thru_hole circle
			(at -7.62 12.7)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 37 "unconnected-(A1-PadD8)")
			(pinfunction "D8")
			(pintype "bidirectional")
			(uuid "b2cea40d-4527-4449-8ad3-747b0c5c2216")
		)
		(pad "D9" thru_hole circle
			(at -7.62 15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 16 "Net-(U1-RESET)")
			(pinfunction "D9")
			(pintype "bidirectional")
			(uuid "2b351c2f-e8be-475a-9c36-082ffbca1d6e")
		)
		(pad "D10" thru_hole circle
			(at 7.62 15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 10 "Net-(A1-D10_CS)")
			(pinfunction "D10_CS")
			(pintype "bidirectional")
			(uuid "d40a8d0b-2565-445c-8282-c62b697ac009")
		)
		(pad "D11" thru_hole circle
			(at 7.62 12.7)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 12 "Net-(A1-D11_MOSI)")
			(pinfunction "D11_MOSI")
			(pintype "bidirectional")
			(uuid "8a4eaf5d-0027-4cb0-8770-c226b3197f9c")
		)
		(pad "D12" thru_hole circle
			(at 7.62 10.16)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 18 "Net-(A1-D12_MISO)")
			(pinfunction "D12_MISO")
			(pintype "bidirectional")
			(uuid "67708c43-4ed3-40e8-8e4c-60fff06ad553")
		)
		(pad "D13" thru_hole circle
			(at 7.62 7.62)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 5 "Net-(A1-D13_SCK)")
			(pinfunction "D13_SCK")
			(pintype "bidirectional")
			(uuid "812e61e7-6d64-4051-84c8-31322a2fbc46")
		)
		(pad "DTR" thru_hole circle
			(at 6.35 -15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 29 "unconnected-(A1-~{DTR}-PadDTR)")
			(pinfunction "~{DTR}")
			(pintype "input")
			(uuid "85c509f6-3f8e-45c8-9b90-6936c64e71f9")
		)
		(pad "GND1" thru_hole rect
			(at -7.62 -5.08)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "555dab8e-ce0c-4109-b595-a3d3bfb6af46")
		)
		(pad "GND2" thru_hole rect
			(at 7.62 -10.16)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 40 "unconnected-(A1-GND-PadGND2)")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "ca86e65c-2d9c-4b90-bd1f-53e10e85f5a0")
		)
		(pad "GND4" thru_hole rect
			(at -3.81 -15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 33 "unconnected-(A1-GND-PadGND4)")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "9b3acc2b-ad47-4aff-a12b-1403ffe08d63")
		)
		(pad "GND5" thru_hole rect
			(at -6.35 -15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 30 "unconnected-(A1-GND-PadGND5)")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "89759c8a-f9d7-44f4-9221-a2a4822cd43e")
		)
		(pad "RAW" thru_hole circle
			(at 7.62 -12.7)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 31 "+BATT")
			(pinfunction "RAW")
			(pintype "power_in")
			(uuid "8c2b496e-31e2-4b70-89e5-25b620302542")
		)
		(pad "RST1" thru_hole circle
			(at -7.62 -7.62)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 42 "unconnected-(A1-RESET-PadRST1)")
			(pinfunction "RESET")
			(pintype "open_collector")
			(uuid "e81f34b0-aa22-4ecb-91e9-d70d07520f53")
		)
		(pad "RST2" thru_hole circle
			(at 7.62 -7.62)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 36 "unconnected-(A1-RESET-PadRST2)")
			(pinfunction "RESET")
			(pintype "open_collector")
			(uuid "a9dd6b1c-a5e0-43c8-9142-ae648c69f76c")
		)
		(pad "RXI" thru_hole circle
			(at 1.27 -15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 38 "unconnected-(A1-PadRXI)")
			(pinfunction "RXI")
			(pintype "input")
			(uuid "b3340359-c0d7-454c-bdba-0d5ec7df89a0")
		)
		(pad "TXO" thru_hole circle
			(at 3.81 -15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 20 "unconnected-(A1-PadTXO)")
			(pinfunction "TXO")
			(pintype "output")
			(uuid "0983f14f-3597-4efa-821f-d24aac6caa20")
		)
		(pad "Vcc1" thru_hole circle
			(at 7.62 -5.08)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 25 "Net-(J1-Pin_1)")
			(pinfunction "Vcc")
			(pintype "power_in")
			(uuid "ef640d34-5a52-4d58-abf2-5ea036c0a2a1")
		)
		(pad "Vcc2" thru_hole circle
			(at -1.27 -15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 26 "unconnected-(A1-Vcc-PadVcc2)")
			(pinfunction "Vcc")
			(pintype "power_in")
			(uuid "51fa401e-616c-4e52-92fd-e095dd292795")
		)
	)
	(footprint "Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical"
		(layer "F.Cu")
		(uuid "5a481a18-c0df-4f55-9291-9aace9e9a80d")
		(at 139.2 53.25 -90)
		(descr "JST EH series connector, B3B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH vertical")
		(property "Reference" "J1"
			(at 2.5 -2.8 90)
			(layer "F.SilkS")
			(uuid "c0ed3e8a-bd47-4ae9-a3f6-56c1f06af836")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Moisture sensor"
			(at 2.5 3.4 90)
			(layer "F.Fab")
			(uuid "7e644d07-fa35-4fc9-b667-ff18d61ece24")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cff890d7-ae00-4788-b93e-2ec2ff1257b8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9e90fdec-f2a6-4ce1-b434-65d51a861a04")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "06079bbc-9fda-4f0a-aa1d-f9bc15497c59")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/50ef554b-ab33-47eb-a0df-d919a3ca0fdc")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.91 2.61)
			(end -0.41 2.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "04c11d1e-440e-4f93-a2fb-b0cef285aea4")
		)
		(fp_line
			(start -2.61 2.31)
			(end 7.61 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee025f3b-75c5-41d3-8f3d-2b362a532779")
		)
		(fp_line
			(start 7.61 2.31)
			(end 7.61 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d4b57ed8-0190-4eb3-8557-563a0d93c77b")
		)
		(fp_line
			(start -2.61 0.81)
			(end -1.61 0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50d1a447-47a2-4d92-8400-7a3f86dd2579")
		)
		(fp_line
			(start -1.61 0.81)
			(end -1.61 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f79aea1a-01a6-4d4c-b44e-5191db5fcdc1")
		)
		(fp_line
			(start 6.61 0.81)
			(end 6.61 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d7f24b6-c9c5-4a1a-b3c3-520059fde812")
		)
		(fp_line
			(start 7.61 0.81)
			(end 6.61 0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c6f9c161-a6e2-4b58-b99f-211d1840e7b6")
		)
		(fp_line
			(start -2.91 0.11)
			(end -2.91 2.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "385eb614-f536-4efe-9e1a-84c5cc2f92ee")
		)
		(fp_line
			(start -2.61 0)
			(end -2.11 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6147988b-230c-4317-801b-56b3b2dd49db")
		)
		(fp_line
			(start -2.11 0)
			(end -2.11 -1.21)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ddc296f-2fd9-4a0c-beff-aadfe3847bbc")
		)
		(fp_line
			(start 7.11 0)
			(end 7.61 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d53f169c-fa14-4353-bd58-dd3784b7a2c2")
		)
		(fp_line
			(start -2.11 -1.21)
			(end 7.11 -1.21)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "39b1708e-ed8a-49a5-981c-adf7aec30600")
		)
		(fp_line
			(start 7.11 -1.21)
			(end 7.11 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "54ac5e17-2dde-4a3a-b475-4d0990377c3f")
		)
		(fp_line
			(start -2.61 -1.71)
			(end -2.61 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ac80cd0-9fa1-4597-964d-7696b384f046")
		)
		(fp_line
			(start 7.61 -1.71)
			(end -2.61 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cff05ace-d31a-410a-b170-5fb005d86abf")
		)
		(fp_line
			(start -3 2.7)
			(end 8 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "49cf134d-d442-4f7d-923c-64eec016ad9a")
		)
		(fp_line
			(start 8 2.7)
			(end 8 -2.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9a177875-442f-4976-942b-b16b08da7164")
		)
		(fp_line
			(start -3 -2.1)
			(end -3 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6817dcfd-4441-4bab-92a2-d14a1ce3817b")
		)
		(fp_line
			(start 8 -2.1)
			(end -3 -2.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "691dbeb8-3cfc-4808-8ced-9346b4b411f7")
		)
		(fp_line
			(start -2.91 2.61)
			(end -0.41 2.61)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bab734f4-c650-46ba-a9bf-0258e36a1d3c")
		)
		(fp_line
			(start -2.5 2.2)
			(end 7.5 2.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "614db1fc-042e-4e96-a427-c59d14a79a99")
		)
		(fp_line
			(start 7.5 2.2)
			(end 7.5 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "589ba1b1-4ff9-4270-947a-3404a28f65b5")
		)
		(fp_line
			(start -2.91 0.11)
			(end -2.91 2.61)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea0218f6-9122-4fac-82aa-50f4b781da03")
		)
		(fp_line
			(start -2.5 -1.6)
			(end -2.5 2.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "964b2061-3655-466d-9ca4-b864be35b492")
		)
		(fp_line
			(start 7.5 -1.6)
			(end -2.5 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "314c2b27-0205-49f6-8cec-4c1dd4d6185a")
		)
		(fp_text user "${REFERENCE}"
			(at 2.5 1.5 90)
			(layer "F.Fab")
			(uuid "579ca93a-229d-49ac-8f59-96b2a3ea6f94")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 25 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "e956d5ba-8652-4a02-9492-4519e659f7aa")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 270)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 23 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "2e4c709b-6211-459c-ad08-2e99df2e12f3")
		)
		(pad "3" thru_hole oval
			(at 5 0 270)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "340a2b7b-0085-47cb-8222-2c7f2c013f96")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(uuid "65e7e811-967d-4591-83af-2507ee1ee43e")
		(at 120.7 63.83 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
			(uuid "e5cd72bd-4c5a-40e2-a0b3-83ec3d7104c8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "R"
			(at 5.08 2.37 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "01212d8d-db83-4190-b904-f161a6a72d88")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7191b7d7-951a-4c2f-8d33-15ce87468c34")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "55740ef6-1c93-41d1-ae3c-8e8f3cc67fb8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4f61970a-c3fd-4fcb-bbe6-80119a18e97a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/37507b13-167d-4c70-b718-5f571d9dfd37")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 8.35 -1.37)
			(end 1.81 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fdf92886-ec79-41e6-8952-5421efc16222")
		)
		(fp_line
			(start 1.81 -1.37)
			(end 1.81 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b50c3200-b57d-4eb8-b977-6440c73246aa")
		)
		(fp_line
			(start 9.12 0)
			(end 8.35 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22731261-743f-40de-a767-7c56b7db164f")
		)
		(fp_line
			(start 1.04 0)
			(end 1.81 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "80518254-36f4-44f6-8d4d-8e3c03b11582")
		)
		(fp_line
			(start 8.35 1.37)
			(end 8.35 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "653f2d43-0c93-436f-915b-d9bbf008962f")
		)
		(fp_line
			(start 1.81 1.37)
			(end 8.35 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f25037e0-7eef-4f12-b589-5656e983c759")
		)
		(fp_line
			(start 11.21 -1.5)
			(end -1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a818ada1-518b-4a46-a59f-0aaa004b6101")
		)
		(fp_line
			(start -1.05 -1.5)
			(end -1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2c67f79b-bca2-419c-8e3b-9bb9ea8f90b2")
		)
		(fp_line
			(start 11.21 1.5)
			(end 11.21 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca756619-b777-4419-8681-8ab159009683")
		)
		(fp_line
			(start -1.05 1.5)
			(end 11.21 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "957468b4-d9bd-4b07-b16a-7bbfb33ff869")
		)
		(fp_line
			(start 8.23 -1.25)
			(end 1.93 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07dfad2f-f310-4f78-85ba-1f89761b11e7")
		)
		(fp_line
			(start 1.93 -1.25)
			(end 1.93 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a93791a0-ecd3-434f-bf46-442c2d86c740")
		)
		(fp_line
			(start 10.16 0)
			(end 8.23 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be7225db-4db4-47c6-be61-a6373b52bad7")
		)
		(fp_line
			(start 0 0)
			(end 1.93 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "55d810ed-96ff-4054-8768-a1bcc1c5b7d1")
		)
		(fp_line
			(start 8.23 1.25)
			(end 8.23 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "880a1b24-6d8c-4deb-89b9-9f4d00c1a777")
		)
		(fp_line
			(start 1.93 1.25)
			(end 8.23 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "05eb360a-d596-4cdc-b929-3b224de9fabb")
		)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
			(uuid "a33b3eed-f360-405e-8230-10f1816c76ca")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 3 "Net-(A1-PadA0)")
			(pintype "passive")
			(uuid "9dcf6873-1b26-48e5-a57f-a2261af1cc35")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 31 "+BATT")
			(pintype "passive")
			(uuid "a0f46ce4-0389-4019-8354-c839516f3421")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(uuid "9a7bfd8e-88ca-44fc-9667-708fe5ea9d72")
		(at 139 76 -90)
		(descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH vertical")
		(property "Reference" "SC1"
			(at 1.25 -2.8 90)
			(layer "F.SilkS")
			(uuid "e6b2d972-c0a0-4392-a09b-99a2d428977d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Solar_Cell"
			(at 1.25 3.4 90)
			(layer "F.Fab")
			(uuid "679fc4fa-5ec5-4625-b9a0-de1e6a341b4a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5d1014b2-1d6a-49f3-a267-200bc1e8e6f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "24562c38-ed53-4630-9080-cbe14e6079b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Single solar cell"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "01de4a6c-c0bc-47b3-825e-758ba984785d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/3e8849ee-5051-4636-b721-7d1012962f61")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.91 2.61)
			(end -0.41 2.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91279564-335c-4208-98b1-8f91d2349056")
		)
		(fp_line
			(start -2.61 2.31)
			(end 5.11 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "43131bb7-442b-4d25-a5a1-2db2fb5acd6e")
		)
		(fp_line
			(start 5.11 2.31)
			(end 5.11 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c2eed5c-2f9e-4b5d-8a87-7a3fb6f2975b")
		)
		(fp_line
			(start -2.61 0.81)
			(end -1.61 0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bfcd0519-bd00-4044-832d-ceda8fc98ac6")
		)
		(fp_line
			(start -1.61 0.81)
			(end -1.61 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6698f635-4794-4c85-b447-07385542bf18")
		)
		(fp_line
			(start 4.11 0.81)
			(end 4.11 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3f7941f-8dcf-4662-8a57-b7c521b5bcd0")
		)
		(fp_line
			(start 5.11 0.81)
			(end 4.11 0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ef22178-4cd0-4b10-839c-8bc4895a0db8")
		)
		(fp_line
			(start -2.91 0.11)
			(end -2.91 2.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d7df1cf3-5650-4eae-b57b-f526e0131832")
		)
		(fp_line
			(start -2.61 0)
			(end -2.11 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "11a33836-a4c3-47b5-a7ad-ba42a196eea1")
		)
		(fp_line
			(start -2.11 0)
			(end -2.11 -1.21)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f21cabfb-426a-4351-8d0b-29ca66fb0ba1")
		)
		(fp_line
			(start 4.61 0)
			(end 5.11 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "55036f67-06e5-4b66-b78d-f84a872fd540")
		)
		(fp_line
			(start -2.11 -1.21)
			(end 4.61 -1.21)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "57ac73a7-7f04-473d-9ae3-deee54948ad9")
		)
		(fp_line
			(start 4.61 -1.21)
			(end 4.61 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f13aaf4a-3fe8-4380-bf72-39a9a1f20c84")
		)
		(fp_line
			(start -2.61 -1.71)
			(end -2.61 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84511a70-b422-4d53-995c-e9a276665074")
		)
		(fp_line
			(start 5.11 -1.71)
			(end -2.61 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa882a17-f62f-4084-8536-39db76c51bef")
		)
		(fp_line
			(start -3 2.7)
			(end 5.5 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72980128-179e-4c12-9b68-5a2e53eb6e94")
		)
		(fp_line
			(start 5.5 2.7)
			(end 5.5 -2.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "547b5023-72e7-425d-989d-a354da3a98c7")
		)
		(fp_line
			(start -3 -2.1)
			(end -3 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "17e2a8de-139e-46d5-a9bf-c9846c83b460")
		)
		(fp_line
			(start 5.5 -2.1)
			(end -3 -2.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "38515ccd-d7c0-44f0-a0c0-680f607415c2")
		)
		(fp_line
			(start -2.91 2.61)
			(end -0.41 2.61)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f2877123-e047-4764-8559-2f166727e3cf")
		)
		(fp_line
			(start -2.5 2.2)
			(end 5 2.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf4ac299-b7d6-4ed1-a301-e7e675dfe7f0")
		)
		(fp_line
			(start 5 2.2)
			(end 5 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e0bd6607-3a2d-4c07-a8bf-b1ccba7ef7f6")
		)
		(fp_line
			(start -2.91 0.11)
			(end -2.91 2.61)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0470c482-c019-4b57-b8ac-27b8674f0de9")
		)
		(fp_line
			(start -2.5 -1.6)
			(end -2.5 2.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e630f027-108c-4de2-ac64-3560e95a7f0d")
		)
		(fp_line
			(start 5 -1.6)
			(end -2.5 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "171adea2-0fe4-47c6-9a7d-1f3624a96875")
		)
		(fp_text user "${REFERENCE}"
			(at 1.25 1.5 90)
			(layer "F.Fab")
			(uuid "57b77f3b-3492-418f-9777-d6d88529e88b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "Net-(D1-A)")
			(pinfunction "+")
			(pintype "passive")
			(uuid "a990148c-c3f6-41f3-9bd5-4067ce7386c3")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 270)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
			(uuid "1199756e-ee17-45cc-8237-e63ddd65adba")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF_Module:HOPERF_RFM9XW_THT"
		(layer "F.Cu")
		(uuid "a40c2e5d-c40a-4323-903a-603ab316e245")
		(at 118 84)
		(descr "Low Power Long Range Transceiver Module THT-16 (https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf)")
		(tags "Low Power Long Range Transceiver Module LoRa")
		(property "Reference" "U1"
			(at -11.2925 0.4075 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "80cb6bc7-7e53-432c-8828-20b4bb0357b9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "RFM95W-868S2"
			(at 6.8 16.36 0)
			(layer "F.Fab")
			(uuid "49c2228a-6770-4758-bdf1-b4d49f4db0e6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "RF_Module:HOPERF_RFM9XW_THT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "66ef3849-7ba3-4643-a395-41f26e1d00f2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c136edaf-8e0f-4239-acb5-aae7261f457b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Low power long range transceiver module, SPI and parallel interface, 868 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3f655664-fc92-43f5-90ee-5092c1df8362")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "HOPERF*RFM9XW*")
		(path "/94df09c3-4ea9-4454-808c-30bc05018d96")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.6 -1.4)
			(end 0.7 -1.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1e904258-735a-4cc1-b150-1c51b81958ce")
		)
		(fp_line
			(start -1.6 0.7)
			(end -1.6 -1.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "477abf38-e3a4-4f02-bfb9-a96b752a0ce3")
		)
		(fp_line
			(start -1.325 -1.125)
			(end 14.925 -1.125)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73bbe9e0-0c67-490a-b811-958a160b0f5d")
		)
		(fp_line
			(start -1.325 15.125)
			(end -1.325 -1.125)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "87a6ddc9-1b9b-406b-a413-3c26258daff4")
		)
		(fp_line
			(start 14.925 -1.125)
			(end 14.925 15.125)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "730cdcbc-5319-4576-8c98-c044a60e68a8")
		)
		(fp_line
			(start 14.925 15.125)
			(end -1.325 15.125)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1729c322-2c97-420e-8159-f8f3d8f259d6")
		)
		(fp_line
			(start -1.45 -1.25)
			(end 15.05 -1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6fad0020-6c58-4445-b09f-04a0b63c8331")
		)
		(fp_line
			(start -1.45 15.25)
			(end -1.45 -1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "70c22f18-f433-43c7-9d79-6a6ae0349026")
		)
		(fp_line
			(start 15.05 -1.25)
			(end 15.05 15.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "97da258c-3a55-4d29-9c0a-98a7a71c8ba3")
		)
		(fp_line
			(start 15.05 15.25)
			(end -1.45 15.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "390053c5-e2f2-4d87-9e07-697fbcb802d5")
		)
		(fp_line
			(start -1.2 0)
			(end -0.2 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1463b70-f24c-4eae-9d9f-11325fbddd0e")
		)
		(fp_line
			(start -1.2 15)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a207eee1-628a-4f27-9be3-6d2c01bbe881")
		)
		(fp_line
			(start -0.2 -1)
			(end 14.8 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b8251c3-fbc3-46ad-b6e9-97f5f86aaaf9")
		)
		(fp_line
			(start 14.8 -1)
			(end 14.8 15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "776ba8b6-325d-4248-aafe-bdd17593ea21")
		)
		(fp_line
			(start 14.8 15)
			(end -1.2 15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4f200a1d-c725-42bc-8ab8-c1d2ae1bdeeb")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 13 "unconnected-(U1-GND-Pad1)")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "9a41d952-eeae-49bd-af34-51916643c44f")
		)
		(pad "2" thru_hole circle
			(at 0 2)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 18 "Net-(A1-D12_MISO)")
			(pinfunction "MISO")
			(pintype "output")
			(uuid "8d9c90d4-2452-4294-94e3-6d6c0a449f5f")
		)
		(pad "3" thru_hole circle
			(at 0 4)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 12 "Net-(A1-D11_MOSI)")
			(pinfunction "MOSI")
			(pintype "input")
			(uuid "eaa2c154-328f-4612-bd72-0d8a2c44516b")
		)
		(pad "4" thru_hole circle
			(at 0 6)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 5 "Net-(A1-D13_SCK)")
			(pinfunction "SCK")
			(pintype "input")
			(uuid "448244f3-6131-4d09-a7c3-d9a592f9f7cc")
		)
		(pad "5" thru_hole circle
			(at 0 8)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 10 "Net-(A1-D10_CS)")
			(pinfunction "NSS")
			(pintype "input")
			(uuid "8239ae63-7e05-43b1-8677-2cbea400439f")
		)
		(pad "6" thru_hole circle
			(at 0 10)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 16 "Net-(U1-RESET)")
			(pinfunction "RESET")
			(pintype "bidirectional")
			(uuid "c3f1e5c2-e1e5-428e-9bad-cdcd10551882")
		)
		(pad "7" thru_hole circle
			(at 0 12)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 17 "unconnected-(U1-DIO5-Pad7)")
			(pinfunction "DIO5")
			(pintype "bidirectional")
			(uuid "d94dcaff-c85b-4f9a-ae11-c9651a64260c")
		)
		(pad "8" thru_hole circle
			(at 0 14)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 6 "unconnected-(U1-GND-Pad8)")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "57508d8a-ea51-4a9c-8166-1429339a36a0")
		)
		(pad "9" thru_hole circle
			(at 13.6 14)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 44 "Net-(AE1-A)")
			(pinfunction "ANT")
			(pintype "bidirectional")
			(uuid "04b78bec-fb97-4d1a-9a2f-bd8ae3d76338")
		)
		(pad "10" thru_hole circle
			(at 13.6 12)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 14 "unconnected-(U1-GND-Pad10)")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "9b50ac56-3e4a-41c6-80b7-ea62aaabd97b")
		)
		(pad "11" thru_hole circle
			(at 13.6 10)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 8 "unconnected-(U1-DIO3-Pad11)")
			(pinfunction "DIO3")
			(pintype "bidirectional")
			(uuid "659f1bff-05dd-4fd2-b9d7-722dec3ebe91")
		)
		(pad "12" thru_hole circle
			(at 13.6 8)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 19 "unconnected-(U1-DIO4-Pad12)")
			(pinfunction "DIO4")
			(pintype "bidirectional")
			(uuid "f7875210-5473-4162-9c55-9ad7d44c18f8")
		)
		(pad "13" thru_hole circle
			(at 13.6 6)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 9 "unconnected-(U1-3.3V-Pad13)")
			(pinfunction "3.3V")
			(pintype "power_in")
			(uuid "6a4fc26a-a8c8-4942-8290-628895319636")
		)
		(pad "14" thru_hole circle
			(at 13.6 4)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 11 "Net-(A1-D2_INT0)")
			(pinfunction "DIO0")
			(pintype "bidirectional")
			(uuid "8d568b14-68b9-452e-8149-f47cf706b914")
		)
		(pad "15" thru_hole circle
			(at 13.6 2)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "Net-(A1-D3_INT1)")
			(pinfunction "DIO1")
			(pintype "bidirectional")
			(uuid "5c1d5c16-f2a2-474e-b79f-1d53f846c9de")
		)
		(pad "16" thru_hole circle
			(at 13.6 0)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 15 "unconnected-(U1-DIO2-Pad16)")
			(pinfunction "DIO2")
			(pintype "bidirectional")
			(uuid "b7f4b20c-d1f0-47c8-ab29-3e943ab0b9bd")
		)
		(model "${KICAD8_3DMODEL_DIR}/RF_Module.3dshapes/HOPERF_RFM9XW_THT.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "watering:MP6550"
		(layer "F.Cu")
		(uuid "a98fc9de-6c53-459a-b167-4e19f2784570")
		(at 71.92 81.65 90)
		(property "Reference" "MP1"
			(at -8.45 0 0)
			(layer "F.SilkS")
			(uuid "4f10a3f6-b4e7-49c7-b582-99b06f26e792")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "accb7308-d887-45ce-b056-f31edf7c3826")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "watering:MP6550"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ffb1b98d-b1ee-45b9-abd0-40a20d811117")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b1edc984-6be7-447e-ac07-6e1b48fd387d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "56340451-9441-4935-9e3f-d1e23d3c1025")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/e8643223-bbc2-4f9b-807c-486347ebcd85")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.45 -6.58)
			(end -7.45 -6.58)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "bb73be2d-3d58-4c92-b8a5-bd026fd41718")
		)
		(fp_line
			(start -7.45 -6.58)
			(end -7.45 -2.193333)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "32e54e89-04d0-46f3-8238-b3e2744771b7")
		)
		(fp_line
			(start -7.09 -2.193333)
			(end -7.09 2.193333)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "006d65c0-8b2d-4553-9c45-fd52c40fa662")
		)
		(fp_line
			(start -7.45 -2.193333)
			(end -7.09 -2.193333)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "67555a9a-10ac-4ea3-96fe-2e276ea7632b")
		)
		(fp_line
			(start -7.09 2.193333)
			(end -7.45 2.193333)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "1ea257a1-88d7-4796-9393-a1ada7d87473")
		)
		(fp_line
			(start -7.45 2.193333)
			(end -7.45 6.58)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "39eed5d0-6b74-463d-9d0b-f4b2c4f07222")
		)
		(fp_line
			(start 7.45 6.58)
			(end 7.45 -6.58)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "30b5549b-a59f-430e-ba33-31697db5d1cd")
		)
		(fp_line
			(start -7.45 6.58)
			(end 7.45 6.58)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "c075a4d1-c522-4208-8570-2ee068ff7132")
		)
		(fp_line
			(start 7.2 -6.33)
			(end 7.2 6.33)
			(stroke
				(width 0.05)
				(type default)
			)
			(layer "F.CrtYd")
			(uuid "bbfd54b1-9ce7-465f-9c52-d06030e24642")
		)
		(fp_line
			(start -7.2 -6.33)
			(end 7.2 -6.33)
			(stroke
				(width 0.05)
				(type default)
			)
			(layer "F.CrtYd")
			(uuid "6cd7adad-ebcb-40ce-92e9-2c5918c07c83")
		)
		(fp_line
			(start 7.2 6.33)
			(end -7.2 6.33)
			(stroke
				(width 0.05)
				(type default)
			)
			(layer "F.CrtYd")
			(uuid "a8509d30-ce8d-43e7-90f3-feb6a354bf5b")
		)
		(fp_line
			(start -7.2 6.33)
			(end -7.2 -6.33)
			(stroke
				(width 0.05)
				(type default)
			)
			(layer "F.CrtYd")
			(uuid "4aa1b387-792b-4818-8025-0c369cac64aa")
		)
		(pad "1" thru_hole oval
			(at -6.35 5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 48 "unconnected-(MP1-VM-Pad1)")
			(pinfunction "VM")
			(pintype "power_out")
			(thermal_bridge_angle 45)
			(uuid "5f8fceaf-c45a-4d21-92a2-c8c3a69e5679")
		)
		(pad "2" thru_hole oval
			(at -3.81 5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(thermal_bridge_angle 45)
			(uuid "5e83c962-5e36-4757-8b69-a4e25ffd8d7d")
		)
		(pad "3" thru_hole oval
			(at -1.27 5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 21 "Net-(MP1-IN2)")
			(pinfunction "IN2")
			(pintype "input")
			(thermal_bridge_angle 45)
			(uuid "4e55b259-6735-4092-b497-8694016946eb")
		)
		(pad "4" thru_hole oval
			(at 1.27 5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 34 "Net-(MP1-IN1)")
			(pinfunction "IN1")
			(pintype "input")
			(thermal_bridge_angle 45)
			(uuid "2c107436-b308-4639-966a-68ea7e6a84ae")
		)
		(pad "5" thru_hole oval
			(at 3.81 5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 49 "unconnected-(MP1-VISEN-Pad5)")
			(pinfunction "VISEN")
			(pintype "input")
			(thermal_bridge_angle 45)
			(uuid "aa5cb064-71f2-46ab-b7c8-c5530ccdbd7c")
		)
		(pad "6" thru_hole oval
			(at 6.35 5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 32 "Net-(MP1-nSLEEP_HB)")
			(pinfunction "nSLEEP_HB")
			(pintype "input")
			(thermal_bridge_angle 45)
			(uuid "bf640629-fca7-4cf8-8eec-a4c985f56dea")
		)
		(pad "7" thru_hole oval
			(at 6.35 -5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 51 "unconnected-(MP1-V3P3-Pad7)")
			(pinfunction "V3P3")
			(pintype "power_out")
			(thermal_bridge_angle 45)
			(uuid "b697a1fa-fb5c-4d50-9047-d2de08b02fbf")
		)
		(pad "8" thru_hole oval
			(at 3.81 -5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 50 "unconnected-(MP1-ISET-Pad8)")
			(pinfunction "ISET")
			(pintype "free")
			(thermal_bridge_angle 45)
			(uuid "b50c192d-4ccf-428e-a259-f57d693a671c")
		)
		(pad "9" thru_hole oval
			(at 1.27 -5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 46 "Net-(M1--)")
			(pinfunction "OUT1")
			(pintype "output")
			(thermal_bridge_angle 45)
			(uuid "4e726511-2953-4f98-a597-289b1a392e59")
		)
		(pad "10" thru_hole oval
			(at -1.27 -5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 45 "Net-(M1-+)")
			(pinfunction "OUT2")
			(pintype "output")
			(thermal_bridge_angle 45)
			(uuid "13d0781f-9ec7-4793-bd17-d7386b86db08")
		)
		(pad "11" thru_hole oval
			(at -3.81 -5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 47 "unconnected-(MP1-GND-Pad11)")
			(pinfunction "GND")
			(pintype "power_out")
			(thermal_bridge_angle 45)
			(uuid "1ef8466b-d6b4-4a1d-a35e-ca3d0d4dac24")
		)
		(pad "12" thru_hole oval
			(at -6.35 -5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 31 "+BATT")
			(pinfunction "VIN")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "f46c1195-4dd8-44e4-b77c-2add924a968d")
		)
	)
	(footprint "Diode_THT:D_T-1_P10.16mm_Horizontal"
		(layer "F.Cu")
		(uuid "b8c11c30-da3c-4ec6-9aa0-3c6613ea839b")
		(at 129.7 65.84 -90)
		(descr "Diode, T-1 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
		(tags "Diode T-1 series Axial Horizontal pin pitch 10.16mm  length 3.2mm diameter 2.6mm")
		(property "Reference" "D1"
			(at 5.08 -2.42 90)
			(layer "F.SilkS")
			(uuid "c7ec92e3-f2f5-4a54-91b3-3c62396f948f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "D"
			(at 5.08 2.42 90)
			(layer "F.Fab")
			(uuid "804d672f-39b1-43ee-baf3-841dc9bf60f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Diode_THT:D_T-1_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f0bb4f74-009c-4968-a14c-4e1959b1f297")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9ff74c8e-ddbe-4fef-b48e-0773c7893995")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "274ff802-6243-462e-aeed-a53a306140a1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f31aeedf-c38a-4995-9834-a390f574cf1b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9b4b352c-fe33-47ae-a090-0b9bdf0e0214")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/e5152be9-1105-4ec0-adcd-bb88edb27dd7")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 3.36 1.42)
			(end 6.8 1.42)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "47f8c0b6-32d2-4ba6-a611-d677635d0168")
		)
		(fp_line
			(start 6.8 1.42)
			(end 6.8 -1.42)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d740b3cb-a577-416d-9d0f-f3513fde288c")
		)
		(fp_line
			(start 1.24 0)
			(end 3.36 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4584915f-f1fb-482b-9f0b-e4309e988dcd")
		)
		(fp_line
			(start 8.92 0)
			(end 6.8 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "26ce9f12-4fc1-44a1-a377-2a8b7e8403ad")
		)
		(fp_line
			(start 3.36 -1.42)
			(end 3.36 1.42)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cb805bfc-57ca-4c94-8a7a-02dec1b2c407")
		)
		(fp_line
			(start 3.84 -1.42)
			(end 3.84 1.42)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2ed6cb4-f124-4ed6-aa49-4bd80f0a06f7")
		)
		(fp_line
			(start 3.96 -1.42)
			(end 3.96 1.42)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "23a9c2e7-fed6-4698-b083-6d3945accbf2")
		)
		(fp_line
			(start 4.08 -1.42)
			(end 4.08 1.42)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e597af7e-63d6-4ac1-8408-57265dc21353")
		)
		(fp_line
			(start 6.8 -1.42)
			(end 3.36 -1.42)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "554b80df-e2a4-43fc-b2ae-9aadfdf8bc86")
		)
		(fp_line
			(start -1.25 1.55)
			(end 11.41 1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "151b4fc3-3749-418c-ad02-74dfee175f54")
		)
		(fp_line
			(start 11.41 1.55)
			(end 11.41 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "354c75c5-de79-4800-8346-31b0ca02b501")
		)
		(fp_line
			(start -1.25 -1.55)
			(end -1.25 1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "da44d0e1-9d38-4f7d-b6f7-20b76d812285")
		)
		(fp_line
			(start 11.41 -1.55)
			(end -1.25 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d51c26ed-5295-4467-b1b8-376b9b0dc36e")
		)
		(fp_line
			(start 3.48 1.3)
			(end 6.68 1.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2795ae74-2726-4c63-a20a-cf1db28a77c8")
		)
		(fp_line
			(start 6.68 1.3)
			(end 6.68 -1.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "88d2ab68-df34-4236-977d-1b345c47eb25")
		)
		(fp_line
			(start 0 0)
			(end 3.48 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b48cbe57-9dcb-4d6b-a107-53a1928117b1")
		)
		(fp_line
			(start 10.16 0)
			(end 6.68 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4405cfcb-c532-4a23-813b-0180ae12fefa")
		)
		(fp_line
			(start 3.48 -1.3)
			(end 3.48 1.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a0e2fb52-6fc7-44b6-a63f-aae9938ce699")
		)
		(fp_line
			(start 3.86 -1.3)
			(end 3.86 1.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da5695f6-c1a8-4af7-bbad-e012458f7d81")
		)
		(fp_line
			(start 3.96 -1.3)
			(end 3.96 1.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d4a2b779-9286-45e8-af75-4f063090da3b")
		)
		(fp_line
			(start 4.06 -1.3)
			(end 4.06 1.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4fb5f8ac-2c78-4c8e-8a9d-7d06f04159c7")
		)
		(fp_line
			(start 6.68 -1.3)
			(end 3.48 -1.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "af573c94-aa82-4e40-9670-55ecfb3b9d5d")
		)
		(fp_text user "K"
			(at 0 -2 90)
			(layer "F.SilkS")
			(uuid "403d6d1e-33b3-45f2-86c5-ca39d59e49fa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "K"
			(at 0 -2 90)
			(layer "F.Fab")
			(uuid "5cbc23ba-3145-44fa-ab29-82a3a5246ba5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 5.32 0 90)
			(layer "F.Fab")
			(uuid "648a49de-fb7e-4adb-98a6-d836cf77d538")
			(effects
				(font
					(size 0.64 0.64)
					(thickness 0.096)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 31 "+BATT")
			(pinfunction "K")
			(pintype "passive")
			(uuid "37e351e9-d105-4f90-9e54-10c93e661779")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 1 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "652fb51d-2de6-459d-b6b2-9f359b3a9eea")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_T-1_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "f229ba1c-1bbe-47bd-8c13-f55e356fb641")
		(at 155 98)
		(descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x01 2.54mm single row")
		(property "Reference" "AE1"
			(at 0 -2.77 0)
			(layer "F.SilkS")
			(uuid "c5e97529-aaab-4b6d-a33f-6f4ae1dbf629")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Antenna"
			(at 0 2.77 0)
			(layer "F.Fab")
			(uuid "62d3781f-78c8-4774-a870-7f9fd92bbddd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9baf6bfb-5cc7-4aa2-99cc-e3c6a09bcddb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "66e27c74-1a26-480b-9b82-5de704813282")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Antenna"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e038cf99-796a-4cfa-bb5b-5b3265ad5660")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/e45d8474-224a-41d4-b6c2-2369f0b51961")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.33 1.21)
			(end -1.33 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d0e4d231-2c10-4db7-a25d-c3e6d4c53dcd")
		)
		(fp_line
			(start -1.33 1.33)
			(end 1.33 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d0c4b07e-0672-40d7-898b-2661e569b910")
		)
		(fp_line
			(start 0 -1.33)
			(end 1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed01de1e-a62c-443a-b002-78f7a6939bfd")
		)
		(fp_line
			(start 1.33 -1.33)
			(end 1.33 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a443a74f-7166-4a63-abdb-775d9361f77d")
		)
		(fp_line
			(start 1.33 1.21)
			(end 1.33 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "57617002-9328-4060-98f0-11cbd0cf3a06")
		)
		(fp_line
			(start -1.8 -1.8)
			(end 1.75 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2eb0bff-17a9-46a0-bb6c-fee6ee9fd414")
		)
		(fp_line
			(start -1.8 1.75)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "465a90a9-bd47-4dd6-b181-90e4c8d7ee42")
		)
		(fp_line
			(start 1.75 -1.8)
			(end 1.75 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "914907f3-740c-4b9a-a22d-e10ce59cf762")
		)
		(fp_line
			(start 1.75 1.75)
			(end -1.8 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b02e9584-5786-4e22-8c91-e0ef24cb4288")
		)
		(fp_line
			(start -1.27 -1.27)
			(end 0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "78b4b1db-8f55-48e9-ba04-8ad9a87051b0")
		)
		(fp_line
			(start -1.27 1.27)
			(end -1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "776a90fa-1a85-417f-8021-7be3f95e4988")
		)
		(fp_line
			(start 0.635 -1.27)
			(end 1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b1b7d3fb-816e-4929-89fa-11e364eae862")
		)
		(fp_line
			(start 1.27 -0.635)
			(end 1.27 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc09efd0-79cc-4347-b04f-49dd81d5a160")
		)
		(fp_line
			(start 1.27 1.27)
			(end -1.27 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "52685082-faf7-44eb-a31f-e9bfbdfb9395")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4eae2057-1e94-46a2-8174-60a7e6728950")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 44 "Net-(AE1-A)")
			(pinfunction "A")
			(pintype "input")
			(uuid "4b9179c2-3812-42f6-a336-fd0baedf44d2")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(uuid "fb72d073-7fa5-41ea-bae4-ad59ac0a9a16")
		(at 139 65.5 -90)
		(descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH vertical")
		(property "Reference" "BT1"
			(at 1.25 -2.8 90)
			(layer "F.SilkS")
			(uuid "510d113c-ed9f-4b79-b676-32640d1f4fcb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Battery"
			(at 1.25 3.4 90)
			(layer "F.Fab")
			(uuid "26c378f5-3fba-4d86-b1aa-a9a73297f7d5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "22c94c28-5372-4632-aa84-15ec4d686a36")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a6960ec3-d588-4f65-bbee-41ad2dc3da86")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Multiple-cell battery"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b5fbb59e-2c3d-4847-9698-c97e9f9cb62c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/9a6cdd60-789d-40f4-acf3-b73bf427b510")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.91 2.61)
			(end -0.41 2.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2c7b7596-91d1-41c3-815b-ddc6fd92c9a9")
		)
		(fp_line
			(start -2.61 2.31)
			(end 5.11 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eed81209-d95d-4182-b33d-874f00e28b80")
		)
		(fp_line
			(start 5.11 2.31)
			(end 5.11 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2331922-bb1a-4f21-9710-ef62f08a3b17")
		)
		(fp_line
			(start -2.61 0.81)
			(end -1.61 0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "98a1e6ee-d593-4597-b60c-bc472318252a")
		)
		(fp_line
			(start -1.61 0.81)
			(end -1.61 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f89aed06-6949-4807-ad26-8b721d80146b")
		)
		(fp_line
			(start 4.11 0.81)
			(end 4.11 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3a2c6158-5751-4f68-94e2-5f82c75a6000")
		)
		(fp_line
			(start 5.11 0.81)
			(end 4.11 0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "856612e5-28b6-4f0d-ab08-a7f7538ebb53")
		)
		(fp_line
			(start -2.91 0.11)
			(end -2.91 2.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d5afec6a-2cb5-4b4f-a5a3-a2b2123320c4")
		)
		(fp_line
			(start -2.61 0)
			(end -2.11 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97952d9a-5d76-4bd9-9a1d-20987b29440d")
		)
		(fp_line
			(start -2.11 0)
			(end -2.11 -1.21)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "60c11449-a526-4e3e-bc52-9ec09c617b8c")
		)
		(fp_line
			(start 4.61 0)
			(end 5.11 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6c8204a5-a8a5-4c35-8cab-a90fec1ac0fc")
		)
		(fp_line
			(start -2.11 -1.21)
			(end 4.61 -1.21)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fcba1d27-e20a-48c0-a80b-35215d25d45b")
		)
		(fp_line
			(start 4.61 -1.21)
			(end 4.61 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d0da9890-0fb7-48df-95f0-7bf4077188ad")
		)
		(fp_line
			(start -2.61 -1.71)
			(end -2.61 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1e1cbe9-0757-443e-b09f-cdedc7175af7")
		)
		(fp_line
			(start 5.11 -1.71)
			(end -2.61 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7bc9cd52-ad51-4827-abd4-e1fccd8b38ad")
		)
		(fp_line
			(start -3 2.7)
			(end 5.5 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d96f2de7-000f-4b52-86bf-49d46257b8d2")
		)
		(fp_line
			(start 5.5 2.7)
			(end 5.5 -2.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c1427ed-e084-478f-ba25-cb542aadd544")
		)
		(fp_line
			(start -3 -2.1)
			(end -3 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6cff1268-097f-43bb-b5b0-f3af10dd1b59")
		)
		(fp_line
			(start 5.5 -2.1)
			(end -3 -2.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "33a04ba6-cda6-40fb-af60-aa32d13674a0")
		)
		(fp_line
			(start -2.91 2.61)
			(end -0.41 2.61)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7d1e5b2-5f90-4993-8ad1-a1f9341fe429")
		)
		(fp_line
			(start -2.5 2.2)
			(end 5 2.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00845b91-8594-4f95-adbd-715cb4ba98df")
		)
		(fp_line
			(start 5 2.2)
			(end 5 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "538ba9a1-1463-48d3-9268-f4d08b2ae026")
		)
		(fp_line
			(start -2.91 0.11)
			(end -2.91 2.61)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "597c634f-20d1-41e8-aa81-2bbd99c4d4b3")
		)
		(fp_line
			(start -2.5 -1.6)
			(end -2.5 2.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a9d10f8-aacd-4533-b741-080ff450512e")
		)
		(fp_line
			(start 5 -1.6)
			(end -2.5 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b456204-3d87-4f24-9ef5-974090bb042e")
		)
		(fp_text user "${REFERENCE}"
			(at 1.25 1.5 90)
			(layer "F.Fab")
			(uuid "f210fddb-5116-4f62-8c89-0a60d9792caf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 31 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(uuid "70ae1950-a002-4b44-81cf-f8e36183aa2e")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 270)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
			(uuid "0a54be31-780c-4908-b9a0-0304aae3596f")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(segment
		(start 129.7 76)
		(end 139 76)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "f527bbe4-a0bb-4ae2-83d7-ca31d3f3b811")
	)
	(segment
		(start 140.475 66.525)
		(end 140.475 59.525)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "186c2cb1-79de-413d-9d0b-0086f58e33b0")
	)
	(segment
		(start 140.3 77.2)
		(end 139 78.5)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "1b0dc175-bf12-4eed-a21f-9ff297dcbbc7")
	)
	(segment
		(start 140.3 69.3)
		(end 140.3 77.2)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "4f461ee8-a52e-4aee-83ff-aabd4096e4bf")
	)
	(segment
		(start 139 68)
		(end 140.3 69.3)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "5056d365-b8c8-484f-ab13-2e1d4ca3e92f")
	)
	(segment
		(start 80.5 70)
		(end 89.5 70)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "7021dbee-841e-4214-a9a0-f5b28969b361")
	)
	(segment
		(start 103.739179 61.2164)
		(end 106.2164 61.2164)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "72de07e2-75eb-4d4e-867d-7f06c5c38c25")
	)
	(segment
		(start 75.7 84.16)
		(end 75.7 74.8)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "810d7b37-2438-4578-aa23-dc2614c4d337")
	)
	(segment
		(start 122.29 78.5)
		(end 120.7 76.91)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "916abd09-db38-4c2f-8fee-580bc6d6bf8d")
	)
	(segment
		(start 77 85.46)
		(end 75.7 84.16)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "92df62eb-b8f5-472e-aedb-c6b87fbf9013")
	)
	(segment
		(start 139 78.5)
		(end 122.29 78.5)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "9a5c12fc-62c7-44a8-a071-070757316ff5")
	)
	(segment
		(start 120.7 75.7)
		(end 120.7 76.91)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "9bf8536a-d900-4c30-86b3-e37e3475c5bf")
	)
	(segment
		(start 139 68)
		(end 140.475 66.525)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "aed69a46-9261-46ec-9e51-170416dabacc")
	)
	(segment
		(start 75.7 74.8)
		(end 80.5 70)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "bbbf0b08-ab22-4163-acf5-b99085651e6a")
	)
	(segment
		(start 94.955579 70)
		(end 103.739179 61.2164)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "ce925b31-7f21-4929-ad50-0524c5ab778b")
	)
	(segment
		(start 89.5 70)
		(end 94.955579 70)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "e5e1caba-d5e7-433c-9857-4b75557ef4a8")
	)
	(segment
		(start 140.475 59.525)
		(end 139.2 58.25)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "eca1d59c-de00-48b6-b44c-af1293895a1f")
	)
	(segment
		(start 106.2164 61.2164)
		(end 120.7 75.7)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "ffa52377-3d99-4d02-9d8d-e6289f01dd12")
	)
	(segment
		(start 107.34 80.16)
		(end 107.5 80)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "12b57545-7e12-48dc-b39f-08dc5fdc480e")
	)
	(segment
		(start 104.74 80.16)
		(end 107.34 80.16)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "7ede1b55-6f9b-4fd7-a867-f8aa3b84491c")
	)
	(segment
		(start 120.7 63.83)
		(end 120.7 66.75)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "ef3892f4-c862-4a74-a64a-31cca47ba561")
	)
	(via
		(at 107.5 80)
		(size 0.6)
		(drill 0.3)
		(layers "F.Cu" "B.Cu")
		(net 3)
		(uuid "2e284ae3-4e31-4271-b035-742522fb2daa")
	)
	(segment
		(start 120.7 66.8)
		(end 120.7 63.83)
		(width 0.2)
		(layer "B.Cu")
		(net 3)
		(uuid "51998252-5503-4983-9c0b-877ad72288ab")
	)
	(segment
		(start 107.5 80)
		(end 120.7 66.8)
		(width 0.2)
		(layer "B.Cu")
		(net 3)
		(uuid "68a8ad38-6da4-49dc-a052-41dce043a3e6")
	)
	(segment
		(start 110.7 82.7)
		(end 118 90)
		(width 0.2)
		(layer "B.Cu")
		(net 5)
		(uuid "2c58fe9b-8ae5-4e22-80b0-f6c38758098e")
	)
	(segment
		(start 104.74 82.7)
		(end 110.7 82.7)
		(width 0.2)
		(layer "B.Cu")
		(net 5)
		(uuid "f97a07e3-8a30-42bf-b885-97d20db8b461")
	)
	(segment
		(start 105.4964 78.9964)
		(end 108.5 82)
		(width 0.2)
		(layer "B.Cu")
		(net 7)
		(uuid "5a9fa78c-224a-431e-bdda-e09f61af07f0")
	)
	(segment
		(start 127.6 82)
		(end 131.6 86)
		(width 0.2)
		(layer "B.Cu")
		(net 7)
		(uuid "5fcace5c-a6c0-481b-ae36-201aa1e47cfd")
	)
	(segment
		(start 89.5 75.08)
		(end 93.4164 78.9964)
		(width 0.2)
		(layer "B.Cu")
		(net 7)
		(uuid "af28c39f-5a5d-4509-a1f3-2b3648107305")
	)
	(segment
		(start 93.4164 78.9964)
		(end 105.4964 78.9964)
		(width 0.2)
		(layer "B.Cu")
		(net 7)
		(uuid "b8394abd-7b99-4a0c-a08d-5f57f41d24ab")
	)
	(segment
		(start 108.5 82)
		(end 127.6 82)
		(width 0.2)
		(layer "B.Cu")
		(net 7)
		(uuid "c9cfb273-d298-43d4-9a81-ecdf284ac3ab")
	)
	(segment
		(start 104.74 90.32)
		(end 116.32 90.32)
		(width 0.2)
		(layer "F.Cu")
		(net 10)
		(uuid "378f9008-2b29-46eb-aff6-d96d36571058")
	)
	(segment
		(start 116.32 90.32)
		(end 118 92)
		(width 0.2)
		(layer "F.Cu")
		(net 10)
		(uuid "3d19e718-48f1-42e0-8818-490e2528faf7")
	)
	(segment
		(start 95.7436 78.7836)
		(end 89.5 72.54)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "4cfacd61-ac64-43f0-90b3-46e0ead79a63")
	)
	(segment
		(start 109.9136 78.7836)
		(end 95.7436 78.7836)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "55a7b32e-6b7f-4bfa-8984-be6cc36e0d7b")
	)
	(segment
		(start 126.625 83.025)
		(end 114.155 83.025)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "896f00d9-af21-4db5-ae7a-44141e170dd9")
	)
	(segment
		(start 114.155 83.025)
		(end 109.9136 78.7836)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "b66e086d-8ff3-406a-81e5-267ae450a83e")
	)
	(segment
		(start 131.6 88)
		(end 126.625 83.025)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "de36f5b9-eafd-42be-b59e-7816d0a25694")
	)
	(segment
		(start 104.74 87.78)
		(end 117.78 87.78)
		(width 0.2)
		(layer "F.Cu")
		(net 12)
		(uuid "1ecf8419-ddcf-4e99-a950-ea60f71191a5")
	)
	(segment
		(start 117.78 87.78)
		(end 118 88)
		(width 0.2)
		(layer "F.Cu")
		(net 12)
		(uuid "851e5d13-8e3e-4adc-94df-c39dc161fb35")
	)
	(segment
		(start 93.18 94)
		(end 118 94)
		(width 0.2)
		(layer "F.Cu")
		(net 16)
		(uuid "985bd9da-6096-445a-b889-56832740fde1")
	)
	(segment
		(start 89.5 90.32)
		(end 93.18 94)
		(width 0.2)
		(layer "F.Cu")
		(net 16)
		(uuid "c72adc27-77e1-492c-9a85-3d540d4c5e36")
	)
	(segment
		(start 117.24 85.24)
		(end 118 86)
		(width 0.2)
		(layer "F.Cu")
		(net 18)
		(uuid "87f1ab79-8292-469d-95f6-4186def644a1")
	)
	(segment
		(start 104.74 85.24)
		(end 117.24 85.24)
		(width 0.2)
		(layer "F.Cu")
		(net 18)
		(uuid "ac8b8db0-8c9c-43e6-be7a-b6acb1a9b285")
	)
	(segment
		(start 77.22 82.7)
		(end 77 82.92)
		(width 0.2)
		(layer "F.Cu")
		(net 21)
		(uuid "4339854e-f24b-44cf-a935-3773adcd85e9")
	)
	(segment
		(start 89.5 82.7)
		(end 77.22 82.7)
		(width 0.2)
		(layer "F.Cu")
		(net 21)
		(uuid "8613bd6e-70e1-4411-84f3-cecbc58b0c2c")
	)
	(segment
		(start 104.74 77.62)
		(end 126.61 55.75)
		(width 0.2)
		(layer "B.Cu")
		(net 23)
		(uuid "1177c75c-c2b8-4a73-92e5-3e087a05802c")
	)
	(segment
		(start 126.61 55.75)
		(end 139.2 55.75)
		(width 0.2)
		(layer "B.Cu")
		(net 23)
		(uuid "266f1fc4-3637-4de9-a7ce-fe4df092ab44")
	)
	(segment
		(start 139.626346 79.65)
		(end 114.39 79.65)
		(width 0.2)
		(layer "F.Cu")
		(net 25)
		(uuid "2a4c166f-2349-442c-b41f-689c4f47960e")
	)
	(segment
		(start 140.875 78.401346)
		(end 139.626346 79.65)
		(width 0.2)
		(layer "F.Cu")
		(net 25)
		(uuid "7666fa3e-0d74-445b-90b2-41a8ad210014")
	)
	(segment
		(start 139.2 53.25)
		(end 140.875 54.925)
		(width 0.2)
		(layer "F.Cu")
		(net 25)
		(uuid "94e221e9-84c4-4cd3-a686-26f80cb9b2f3")
	)
	(segment
		(start 140.875 54.925)
		(end 140.875 78.401346)
		(width 0.2)
		(layer "F.Cu")
		(net 25)
		(uuid "ca6a209a-1b16-4715-a29e-c9505838010b")
	)
	(segment
		(start 114.39 79.65)
		(end 104.74 70)
		(width 0.2)
		(layer "F.Cu")
		(net 25)
		(uuid "fd39d6e6-a4ea-403b-b1dd-48689143c574")
	)
	(segment
		(start 129.7 65.84)
		(end 138.66 65.84)
		(width 0.2)
		(layer "F.Cu")
		(net 31)
		(uuid "02470da5-e9ce-4b75-b171-6e05a37a3249")
	)
	(segment
		(start 129.7 65.84)
		(end 129.7 62.67)
		(width 0.2)
		(layer "F.Cu")
		(net 31)
		(uuid "42a0aa23-4b68-48de-a916-da168a13d5f1")
	)
	(segment
		(start 129.7 62.67)
		(end 120.7 53.67)
		(width 0.2)
		(layer "F.Cu")
		(net 31)
		(uuid "6e7496d2-48ff-49b4-8264-b3ab17c354ba")
	)
	(segment
		(start 138.66 65.84)
		(end 139 65.5)
		(width 0.2)
		(layer "F.Cu")
		(net 31)
		(uuid "b185c58d-e066-4815-a077-ed9d2af2ffa3")
	)
	(segment
		(start 104.74 62.38)
		(end 111.99 62.38)
		(width 0.2)
		(layer "B.Cu")
		(net 31)
		(uuid "230d3801-02cf-448d-964f-55ad2944d94f")
	)
	(segment
		(start 83.934421 79)
		(end 89.018021 73.9164)
		(width 0.2)
		(layer "B.Cu")
		(net 31)
		(uuid "273fcd0f-7091-4a19-ad80-ee898abeea55")
	)
	(segment
		(start 75.84 79)
		(end 83.934421 79)
		(width 0.2)
		(layer "B.Cu")
		(net 31)
		(uuid "b9fa8af2-65f9-43ee-892a-e35a70327e26")
	)
	(segment
		(start 111.99 62.38)
		(end 120.7 53.67)
		(width 0.2)
		(layer "B.Cu")
		(net 31)
		(uuid "bdd9d275-2164-40a6-9049-b924aefdd5b6")
	)
	(segment
		(start 93.2036 73.9164)
		(end 104.74 62.38)
		(width 0.2)
		(layer "B.Cu")
		(net 31)
		(uuid "cfb1a4a1-5c01-4571-9def-0f49f1d33d40")
	)
	(segment
		(start 66.84 88)
		(end 75.84 79)
		(width 0.2)
		(layer "B.Cu")
		(net 31)
		(uuid "e77da77e-4ddf-491b-b3d1-b5cf1efccb01")
	)
	(segment
		(start 89.018021 73.9164)
		(end 93.2036 73.9164)
		(width 0.2)
		(layer "B.Cu")
		(net 31)
		(uuid "fc9c923e-1590-4cd0-8378-eae952e40115")
	)
	(segment
		(start 89.5 77.62)
		(end 79.32 77.62)
		(width 0.2)
		(layer "F.Cu")
		(net 32)
		(uuid "3ee845bf-a74e-4b89-b693-e92edad12884")
	)
	(segment
		(start 79.32 77.62)
		(end 77 75.3)
		(width 0.2)
		(layer "F.Cu")
		(net 32)
		(uuid "f958adf7-b73c-4885-8e48-38a591034f9b")
	)
	(segment
		(start 77.22 80.16)
		(end 77 80.38)
		(width 0.2)
		(layer "F.Cu")
		(net 34)
		(uuid "4ce68efd-e644-4868-957e-c2206b5899d5")
	)
	(segment
		(start 89.5 80.16)
		(end 77.22 80.16)
		(width 0.2)
		(layer "F.Cu")
		(net 34)
		(uuid "d11e8a72-8414-4dbf-830a-105623dcb13d")
	)
	(segment
		(start 131.6 98)
		(end 155 98)
		(width 0.2)
		(layer "F.Cu")
		(net 44)
		(uuid "817475d2-4dd7-4d27-b0f7-e9bb5d52f975")
	)
	(segment
		(start 66.8 82.96)
		(end 66.84 82.92)
		(width 0.2)
		(layer "F.Cu")
		(net 45)
		(uuid "4e4d2661-751e-43e0-8098-019ab843380d")
	)
	(segment
		(start 57 82.96)
		(end 66.8 82.96)
		(width 0.2)
		(layer "F.Cu")
		(net 45)
		(uuid "bba03158-0dd1-4932-8b85-2b9866d70e38")
	)
	(segment
		(start 66.76 80.46)
		(end 66.84 80.38)
		(width 0.2)
		(layer "F.Cu")
		(net 46)
		(uuid "75e7b643-b610-47a6-aac4-b0d70cda0ad5")
	)
	(segment
		(start 57 80.46)
		(end 66.76 80.46)
		(width 0.2)
		(layer "F.Cu")
		(net 46)
		(uuid "e39df956-0d05-4294-8863-7c611f1667ef")
	)
)
