(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(D1-A)")
	(net 2 "GND")
	(net 3 "Net-(A1-PadA0)")
	(net 4 "unconnected-(U1-ANT-Pad9)")
	(net 5 "Net-(A1-D13_SCK)")
	(net 6 "unconnected-(U1-GND-Pad8)")
	(net 7 "unconnected-(U1-DIO1-Pad15)")
	(net 8 "unconnected-(U1-DIO3-Pad11)")
	(net 9 "unconnected-(U1-3.3V-Pad13)")
	(net 10 "Net-(A1-D10_CS)")
	(net 11 "Net-(A1-D2_INT0)")
	(net 12 "Net-(A1-D11_MOSI)")
	(net 13 "unconnected-(U1-GND-Pad1)")
	(net 14 "unconnected-(U1-GND-Pad10)")
	(net 15 "unconnected-(U1-DIO2-Pad16)")
	(net 16 "Net-(U1-RESET)")
	(net 17 "unconnected-(U1-DIO5-Pad7)")
	(net 18 "Net-(A1-D12_MISO)")
	(net 19 "unconnected-(U1-DIO4-Pad12)")
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 94.42 89)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.76 13.6 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(A1-PadA0)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF_Module:HOPERF_RFM9XW_THT"
		(layer "F.Cu")
		(at 96 51)
		(descr "Low Power Long Range Transceiver Module THT-16 (https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf)")
		(tags "Low Power Long Range Transceiver Module LoRa")
		(property "Reference" "U1"
			(at -24.7925 13.9075 0)
			(layer "F.SilkS")
		)
		(property "Value" "RFM95W-868S2"
			(at 6.8 16.36 0)
			(layer "F.Fab")
		)
		(property "Footprint" "RF_Module:HOPERF_RFM9XW_THT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Low power long range transceiver module, SPI and parallel interface, 868 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "HOPERF*RFM9XW*")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -20.2925 -5.0925 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(U1-GND-Pad1)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 0 2)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(A1-D11_MOSI)")
			(pinfunction "MISO")
			(pintype "output")
		)
		(pad "3" thru_hole circle
			(at 0 4)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(A1-D12_MISO)")
			(pinfunction "MOSI")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 0 6)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(A1-D13_SCK)")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 8)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(A1-D10_CS)")
			(pinfunction "NSS")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at 0 10)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(U1-RESET)")
			(pinfunction "RESET")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at 0 12)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(U1-DIO5-Pad7)")
			(pinfunction "DIO5")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole circle
			(at 0 14)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(U1-GND-Pad8)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at 13.6 14)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(U1-ANT-Pad9)")
			(pinfunction "ANT")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at 13.6 12)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(U1-GND-Pad10)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" thru_hole circle
			(at 13.6 10)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(U1-DIO3-Pad11)")
			(pinfunction "DIO3")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at 13.6 8)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(U1-DIO4-Pad12)")
			(pinfunction "DIO4")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole circle
			(at 13.6 6)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(U1-3.3V-Pad13)")
			(pinfunction "3.3V")
			(pintype "power_in")
		)
		(pad "14" thru_hole circle
			(at 13.6 4)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(A1-D2_INT0)")
			(pinfunction "DIO0")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole circle
			(at 13.6 2)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(U1-DIO1-Pad15)")
			(pinfunction "DIO1")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole circle
			(at 13.6 0)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(U1-DIO2-Pad16)")
			(pinfunction "DIO2")
			(pintype "bidirectional")
		)
		(model "${KICAD8_3DMODEL_DIR}/RF_Module.3dshapes/HOPERF_RFM9XW_THT.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 132 79.5)
		(descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH vertical")
		(property "Reference" "J1"
			(at 1.25 -2.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 1.25 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-A)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
)
