(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.579)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
				(material "Peters SD2692")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.025)
				(material "Elpemer AS 2467 SM-DG")
				(epsilon_r 3.7)
				(loss_tangent 0)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(color "FR4 natural")
				(thickness 1.459)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.025)
				(material "Elpemer AS 2467 SM-DG")
				(epsilon_r 3.7)
				(loss_tangent 0)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
				(material "Peters SD2692")
			)
			(copper_finish "HAL lead-free")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(D1-A)")
	(net 2 "GND")
	(net 3 "Net-(A1-PadA0)")
	(net 4 "unconnected-(A1-PadD7)")
	(net 5 "Net-(A1-D13_SCK)")
	(net 6 "Net-(A1-D3_INT1)")
	(net 7 "unconnected-(U1-DIO3-Pad11)")
	(net 8 "Net-(A1-D10_CS)")
	(net 9 "Net-(A1-D2_INT0)")
	(net 10 "Net-(A1-D11_MOSI)")
	(net 11 "unconnected-(U1-DIO2-Pad16)")
	(net 12 "Net-(U1-RESET)")
	(net 13 "unconnected-(U1-DIO5-Pad7)")
	(net 14 "Net-(A1-D12_MISO)")
	(net 15 "unconnected-(U1-DIO4-Pad12)")
	(net 16 "unconnected-(A1-PadTXO)")
	(net 17 "Net-(MP1-IN2)")
	(net 18 "unconnected-(A1-PadA7)")
	(net 19 "Net-(J1-Pin_2)")
	(net 20 "unconnected-(A1-A5{slash}SCL-PadA5)")
	(net 21 "Net-(J1-Pin_1)")
	(net 22 "unconnected-(A1-Vcc-PadVcc2)")
	(net 23 "unconnected-(A1-PadA6)")
	(net 24 "unconnected-(A1-PadA3)")
	(net 25 "unconnected-(A1-~{DTR}-PadDTR)")
	(net 26 "unconnected-(A1-GND-PadGND5)")
	(net 27 "+BATT")
	(net 28 "Net-(MP1-nSLEEP_HB)")
	(net 29 "unconnected-(A1-GND-PadGND4)")
	(net 30 "Net-(MP1-IN1)")
	(net 31 "unconnected-(A1-A4{slash}SDA-PadA4)")
	(net 32 "unconnected-(A1-RESET-PadRST2)")
	(net 33 "unconnected-(A1-PadD8)")
	(net 34 "unconnected-(A1-PadRXI)")
	(net 35 "unconnected-(A1-D0{slash}RX-PadD0)")
	(net 36 "Net-(J2-Pin_2)")
	(net 37 "unconnected-(A1-RESET-PadRST1)")
	(net 38 "unconnected-(A1-D1{slash}TX-PadD1)")
	(net 39 "Net-(AE1-A)")
	(net 40 "Net-(M1-+)")
	(net 41 "Net-(M1--)")
	(net 42 "unconnected-(MP1-GND-Pad11)")
	(net 43 "unconnected-(MP1-VM-Pad1)")
	(net 44 "unconnected-(MP1-VISEN-Pad5)")
	(net 45 "unconnected-(MP1-ISET-Pad8)")
	(net 46 "unconnected-(MP1-V3P3-Pad7)")
	(net 47 "AE1-B")
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 137 50)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "REF**"
			(at 0 -4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3mm"
			(at 0 4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 130.5 98)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "REF**"
			(at 0 -2.38 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PinHeader_1x01_P2.54mm_Vertical"
			(at 0 2.38 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "AE1-B")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 74.2 67.25 90)
		(descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH vertical")
		(property "Reference" "M1"
			(at -3.75 0.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "Motor_DC"
			(at 1.25 3.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Motor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader*P2.54mm* TerminalBlock*")
		(sheetname "/")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 1.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 40 "Net-(M1-+)")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(pad "2" thru_hole oval
			(at 2.5 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(M1--)")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 110.5 67 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 5.25 2.7 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 5.08 2.37 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(A1-PadA0)")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_arduino-library:Arduino_Pro_Mini_Socket"
		(layer "F.Cu")
		(at 97 76.5)
		(descr "https://docs.arduino.cc/retired/boards/arduino-pro-mini")
		(property "Reference" "A1"
			(at -6.858 -17.526 0)
			(layer "F.SilkS")
		)
		(property "Value" "Arduino_Pro_Mini_Socket"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://docs.arduino.cc/retired/boards/arduino-pro-mini"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Socket for Arduino Pro Mini"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Arduino_Pro_Mini_Socket")
		(sheetname "/")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_text user "D0"
			(at -5.715 -10.16 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "BLK"
			(at -8.255 -15.24 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GRN"
			(at 8.255 -15.24 90)
			(layer "F.SilkS")
		)
		(fp_text user "D0"
			(at -5.715 -10.16 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "A0" thru_hole circle
			(at 7.62 5.08)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(A1-PadA0)")
			(pinfunction "A0")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "A1" thru_hole circle
			(at 7.62 2.54)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J1-Pin_2)")
			(pinfunction "A1")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "A2" thru_hole circle
			(at 7.62 0)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(J2-Pin_2)")
			(pinfunction "A2")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "A3" thru_hole circle
			(at 7.62 -2.54)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(A1-PadA3)")
			(pinfunction "A3")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "A4" thru_hole circle
			(at 4.6941 -1.3894)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(A1-A4{slash}SDA-PadA4)")
			(pinfunction "A4/SDA")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "A5" thru_hole circle
			(at 4.6941 -3.9294)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(A1-A5{slash}SCL-PadA5)")
			(pinfunction "A5/SCL")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "A6" thru_hole circle
			(at 4.6941 9.0246)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(A1-PadA6)")
			(pinfunction "A6")
			(pintype "input")
			(solder_mask_margin 0)
		)
		(pad "A7" thru_hole circle
			(at 4.6941 6.484)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(A1-PadA7)")
			(pinfunction "A7")
			(pintype "input")
			(solder_mask_margin 0)
		)
		(pad "D0" thru_hole circle
			(at -7.62 -10.16)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(A1-D0{slash}RX-PadD0)")
			(pinfunction "D0/RX")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "D1" thru_hole circle
			(at -7.62 -12.7)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(A1-D1{slash}TX-PadD1)")
			(pinfunction "D1/TX")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "D2" thru_hole circle
			(at -7.62 -2.54)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(A1-D2_INT0)")
			(pinfunction "D2_INT0")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "D3" thru_hole circle
			(at -7.62 0)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(A1-D3_INT1)")
			(pinfunction "D3_INT1")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "D4" thru_hole circle
			(at -7.62 2.54)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(MP1-nSLEEP_HB)")
			(pinfunction "D4")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "D5" thru_hole circle
			(at -7.62 5.08)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(MP1-IN1)")
			(pinfunction "D5")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "D6" thru_hole circle
			(at -7.62 7.62)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(MP1-IN2)")
			(pinfunction "D6")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "D7" thru_hole circle
			(at -7.62 10.16)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(A1-PadD7)")
			(pinfunction "D7")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "D8" thru_hole circle
			(at -7.62 12.7)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(A1-PadD8)")
			(pinfunction "D8")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "D9" thru_hole circle
			(at -7.62 15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(U1-RESET)")
			(pinfunction "D9")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "D10" thru_hole circle
			(at 7.62 15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(A1-D10_CS)")
			(pinfunction "D10_CS")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "D11" thru_hole circle
			(at 7.62 12.7)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(A1-D11_MOSI)")
			(pinfunction "D11_MOSI")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "D12" thru_hole circle
			(at 7.62 10.16)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(A1-D12_MISO)")
			(pinfunction "D12_MISO")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "D13" thru_hole circle
			(at 7.62 7.62)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(A1-D13_SCK)")
			(pinfunction "D13_SCK")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "DTR" thru_hole circle
			(at 6.35 -15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(A1-~{DTR}-PadDTR)")
			(pinfunction "~{DTR}")
			(pintype "input")
			(solder_mask_margin 0)
		)
		(pad "GND1" thru_hole rect
			(at -7.62 -5.08)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0)
		)
		(pad "GND2" thru_hole rect
			(at 7.62 -10.16)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0)
		)
		(pad "GND4" thru_hole rect
			(at -3.81 -15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(A1-GND-PadGND4)")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0)
		)
		(pad "GND5" thru_hole rect
			(at -6.35 -15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(A1-GND-PadGND5)")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0)
		)
		(pad "RAW" thru_hole circle
			(at 7.62 -12.7)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "+BATT")
			(pinfunction "RAW")
			(pintype "power_in")
			(solder_mask_margin 0)
		)
		(pad "RST1" thru_hole circle
			(at -7.62 -7.62)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(A1-RESET-PadRST1)")
			(pinfunction "RESET")
			(pintype "open_collector")
			(solder_mask_margin 0)
		)
		(pad "RST2" thru_hole circle
			(at 7.62 -7.62)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(A1-RESET-PadRST2)")
			(pinfunction "RESET")
			(pintype "open_collector")
			(solder_mask_margin 0)
		)
		(pad "RXI" thru_hole circle
			(at 1.27 -15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(A1-PadRXI)")
			(pinfunction "RXI")
			(pintype "input")
			(solder_mask_margin 0)
		)
		(pad "TXO" thru_hole circle
			(at 3.81 -15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(A1-PadTXO)")
			(pinfunction "TXO")
			(pintype "output")
			(solder_mask_margin 0)
		)
		(pad "Vcc1" thru_hole circle
			(at 7.62 -5.08)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J1-Pin_1)")
			(pinfunction "Vcc")
			(pintype "power_in")
			(solder_mask_margin 0)
		)
		(pad "Vcc2" thru_hole circle
			(at -1.27 -15.24)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(A1-Vcc-PadVcc2)")
			(pinfunction "Vcc")
			(pintype "power_in")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 75 50)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "REF**"
			(at 0 -4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3mm"
			(at 0 4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_1.5x1.5mm"
		(layer "F.Cu")
		(at 82.5 98.5)
		(descr "SMD rectangular pad as test Point, square 1.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "Batt"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint_Pad_1.5x1.5mm"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 123.2 49.75 -90)
		(descr "JST EH series connector, B3B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH vertical")
		(property "Reference" "J1"
			(at 2.5 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Moisture sensor"
			(at 2.5 3.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 1.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 21 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(pad "2" thru_hole oval
			(at 2.5 0 270)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(pad "3" thru_hole oval
			(at 5 0 270)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.5x1.5mm"
		(layer "F.Cu")
		(at 82.5 93.5)
		(descr "SMD rectangular pad as test Point, square 1.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "Batt"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint_Pad_1.5x1.5mm"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 27 "+BATT")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 110.5 64.08 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 5.08 2.37 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(A1-PadA0)")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "+BATT")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 98.85 49.79 -90)
		(descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH vertical")
		(property "Reference" "J2"
			(at 1.25 3.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "Level sensor"
			(at 1.25 3.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 1.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 21 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(pad "2" thru_hole oval
			(at 2.5 0 270)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 123 72.5 -90)
		(descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH vertical")
		(property "Reference" "SC1"
			(at 1.25 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Solar_Cell"
			(at 1.25 3.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single solar cell"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 1.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "Net-(D1-A)")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(pad "2" thru_hole oval
			(at 2.5 0 270)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF_Module:HOPERF_RFM9XW_THT"
		(layer "F.Cu")
		(at 110.7925 84.0925)
		(descr "Low Power Long Range Transceiver Module THT-16 (https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf)")
		(tags "Low Power Long Range Transceiver Module LoRa")
		(property "Reference" "U1"
			(at -11.2925 0.4075 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RFM95W-868S2"
			(at 6.8 16.36 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Low power long range transceiver module, SPI and parallel interface, 868 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "HOPERF*RFM9XW*")
		(sheetname "/")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0)
		)
		(pad "2" thru_hole circle
			(at 0 2)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(A1-D12_MISO)")
			(pinfunction "MISO")
			(pintype "output")
			(solder_mask_margin 0)
		)
		(pad "3" thru_hole circle
			(at 0 4)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(A1-D11_MOSI)")
			(pinfunction "MOSI")
			(pintype "input")
			(solder_mask_margin 0)
		)
		(pad "4" thru_hole circle
			(at 0 6)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(A1-D13_SCK)")
			(pinfunction "SCK")
			(pintype "input")
			(solder_mask_margin 0)
		)
		(pad "5" thru_hole circle
			(at 0 8)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(A1-D10_CS)")
			(pinfunction "NSS")
			(pintype "input")
			(solder_mask_margin 0)
		)
		(pad "6" thru_hole circle
			(at 0 10)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(U1-RESET)")
			(pinfunction "RESET")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "7" thru_hole circle
			(at 0 12)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(U1-DIO5-Pad7)")
			(pinfunction "DIO5")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "8" thru_hole circle
			(at 0 14)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0)
		)
		(pad "9" thru_hole circle
			(at 13.6 14)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(AE1-A)")
			(pinfunction "ANT")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "10" thru_hole circle
			(at 13.6 12)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0)
		)
		(pad "11" thru_hole circle
			(at 13.6 10)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(U1-DIO3-Pad11)")
			(pinfunction "DIO3")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "12" thru_hole circle
			(at 13.6 8)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(U1-DIO4-Pad12)")
			(pinfunction "DIO4")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "13" thru_hole circle
			(at 13.6 6)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J1-Pin_1)")
			(pinfunction "3.3V")
			(pintype "power_in")
			(solder_mask_margin 0)
		)
		(pad "14" thru_hole circle
			(at 13.6 4)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(A1-D2_INT0)")
			(pinfunction "DIO0")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "15" thru_hole circle
			(at 13.6 2)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(A1-D3_INT1)")
			(pinfunction "DIO1")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(pad "16" thru_hole circle
			(at 13.6 0)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(U1-DIO2-Pad16)")
			(pinfunction "DIO2")
			(pintype "bidirectional")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/RF_Module.3dshapes/HOPERF_RFM9XW_THT.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 137 98)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "REF**"
			(at 0 -4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3mm"
			(at 0 4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
	)
	(footprint "watering:MP6550"
		(layer "F.Cu")
		(at 79.5 81 90)
		(property "Reference" "MP1"
			(at -8.45 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at -6.35 5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "unconnected-(MP1-VM-Pad1)")
			(pinfunction "VM")
			(pintype "power_out")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole oval
			(at -3.81 5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole oval
			(at -1.27 5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(MP1-IN2)")
			(pinfunction "IN2")
			(pintype "input")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole oval
			(at 1.27 5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(MP1-IN1)")
			(pinfunction "IN1")
			(pintype "input")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "5" thru_hole oval
			(at 3.81 5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(MP1-VISEN-Pad5)")
			(pinfunction "VISEN")
			(pintype "input")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "6" thru_hole oval
			(at 6.35 5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(MP1-nSLEEP_HB)")
			(pinfunction "nSLEEP_HB")
			(pintype "input")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "7" thru_hole oval
			(at 6.35 -5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "unconnected-(MP1-V3P3-Pad7)")
			(pinfunction "V3P3")
			(pintype "power_out")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "8" thru_hole oval
			(at 3.81 -5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(MP1-ISET-Pad8)")
			(pinfunction "ISET")
			(pintype "free")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "9" thru_hole oval
			(at 1.27 -5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(M1--)")
			(pinfunction "OUT1")
			(pintype "output")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "10" thru_hole oval
			(at -1.27 -5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(M1-+)")
			(pinfunction "OUT2")
			(pintype "output")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "11" thru_hole oval
			(at -3.81 -5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(MP1-GND-Pad11)")
			(pinfunction "GND")
			(pintype "power_out")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(pad "12" thru_hole oval
			(at -6.35 -5.08 90)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "+BATT")
			(pinfunction "VIN")
			(pintype "power_in")
			(solder_mask_margin 0)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_THT:D_T-1_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 115 53.92 -90)
		(descr "Diode, T-1 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
		(tags "Diode T-1 series Axial Horizontal pin pitch 10.16mm  length 3.2mm diameter 2.6mm")
		(property "Reference" "D1"
			(at 5.08 -2.42 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 5.08 2.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2 90)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 5.32 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "+BATT")
			(pinfunction "K")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_T-1_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 103.5 47.84 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(J2-Pin_2)")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(pad "2" thru_hole circle
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 75 98)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "REF**"
			(at 0 -4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3mm"
			(at 0 4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 123 62 -90)
		(descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH vertical")
		(property "Reference" "BT1"
			(at 1.25 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Battery"
			(at 1.25 3.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Multiple-cell battery"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Watering.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 1.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 27 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(pad "2" thru_hole oval
			(at 2.5 0 270)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin 0)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF_Antenna:Texas_SWRA416_868MHz_915MHz"
		(layer "B.Cu")
		(at 133.95 79 90)
		(descr "http://www.ti.com/lit/an/swra416/swra416.pdf")
		(tags "PCB antenna")
		(property "Reference" "AE1"
			(at -6 -6.6 90)
			(layer "B.SilkS")
		)
		(property "Value" "Antenna"
			(at 11 3.5 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Antenna"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Watering.kicad_sch")
		(attr smd)
		(fp_text user " any PCB layer."
			(at 1 -4.2 90)
			(layer "Cmts.User")
		)
		(fp_text user "any components on"
			(at 1 -2.2 90)
			(layer "Cmts.User")
		)
		(fp_text user "No metal, traces or "
			(at 1 -0.2 90)
			(layer "Cmts.User")
		)
		(fp_text user "KEEP-OUT ZONE"
			(at 1 2.8 90)
			(layer "Cmts.User")
		)
		(fp_text user "${REFERENCE}"
			(at -0.4 -6.6 90)
			(layer "B.Fab")
		)
		(pad "" thru_hole circle
			(at -9 5.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at -7 0.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at -7 5.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at -5 0.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at -5 5.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at -3 0.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at -3 5.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at -1 0.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at -1 5.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at 1 0.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at 1 5.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at 3 0.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at 3 5.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at 5 0.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at 5 5.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at 7 0.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at 7 5.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at 9 0.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "" thru_hole circle
			(at 9 5.8 270)
			(size 1 1)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(solder_mask_margin 0)
		)
		(pad "1" smd trapezoid
			(at -9 -5.9 270)
			(size 0.4 0.8)
			(rect_delta 0 -0.3)
			(layers "B.Cu")
			(net 39 "Net-(AE1-A)")
			(pinfunction "A")
			(pintype "input")
			(solder_mask_margin 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 128.25 88.7) (xy 128.25 69.3) (xy 140.45 69.3) (xy 140.45 88.7)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "B.Cu")
		(at 128.65 93 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "Ant ext"
			(at 0 1.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 -1.9 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 39 "Net-(AE1-A)")
			(solder_mask_margin 0)
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 47 "AE1-B")
			(solder_mask_margin 0)
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(gr_rect
		(start 71 46)
		(end 141 102)
		(fill no)
		(layer "Edge.Cuts")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 128 102) (xy 128.3 81.8) (xy 128.25 81.8) (xy 128 46) (xy 71 46) (xy 71 102)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 128 102) (xy 128 81.8) (xy 128 46) (xy 71 46) (xy 71 102)
			)
		)
	)
	(embedded_fonts no)
)
