(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(lib_symbols
		(symbol "Connector:Conn_01x03_Pin"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 5.08 0)
			)
			(property "Value" "Conn_01x03_Pin"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x03, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x03_Pin_1_1"
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 0.8636 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 2.54) (xy 0.8636 2.54)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0.8636 -2.413)
					(end 0 -2.667)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 2.667)
					(end 0 2.413)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
			)
		)
		(symbol "Device:Antenna"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "AE"
				(at -1.905 1.905 0)
			)
			(property "Value" "Antenna"
				(at -1.905 0 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Antenna"
				(at 0 0 0)
			)
			(property "ki_keywords" "antenna"
				(at 0 0 0)
			)
			(symbol "Antenna_0_1"
				(polyline
					(pts
						(xy 0 2.54) (xy 0 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 2.54) (xy 0 -2.54) (xy -1.27 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Antenna_1_1"
				(pin input line
					(at 0 -5.08 90)
					(length 2.54)
					(name "A")
					(number "1")
				)
			)
		)
		(symbol "Device:Battery"
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "BT"
				(at 2.54 2.54 0)
			)
			(property "Value" "Battery"
				(at 2.54 0 0)
			)
			(property "Footprint" ""
				(at 0 1.524 90)
			)
			(property "Datasheet" "~"
				(at 0 1.524 90)
			)
			(property "Description" "Multiple-cell battery"
				(at 0 0 0)
			)
			(property "ki_keywords" "batt voltage-source cell"
				(at 0 0 0)
			)
			(symbol "Battery_0_1"
				(rectangle
					(start -2.286 -1.27)
					(end 2.286 -1.524)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -2.286 1.778)
					(end 2.286 1.524)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.524 -2.032)
					(end 1.524 -2.54)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.524 1.016)
					(end 1.524 0.508)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0 -1.016) (xy 0 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -0.508) (xy 0 -0.254)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 0.254)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.778) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 3.048) (xy 1.778 3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 3.556) (xy 1.27 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Battery_1_1"
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "+")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 2.54)
					(name "-")
					(number "2")
				)
			)
		)
		(symbol "Device:D"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "D"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Diode"
				(at 0 0 0)
			)
			(property "Sim.Device" "D"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=K 2=A"
				(at 0 0 0)
			)
			(property "ki_keywords" "diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*"
				(at 0 0 0)
			)
			(symbol "D_0_1"
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27) (xy -1.27 0) (xy 1.27 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "D_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
		)
		(symbol "Device:R"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Device:Solar_Cell"
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SC"
				(at 2.54 2.54 0)
			)
			(property "Value" "Solar_Cell"
				(at 2.54 0 0)
			)
			(property "Footprint" ""
				(at 0 1.524 90)
			)
			(property "Datasheet" "~"
				(at 0 1.524 90)
			)
			(property "Description" "Single solar cell"
				(at 0 0 0)
			)
			(property "ki_keywords" "solar cell"
				(at 0 0 0)
			)
			(symbol "Solar_Cell_0_1"
				(rectangle
					(start -2.032 1.778)
					(end 2.032 1.524)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.3208 1.1938)
					(end 1.27 0.6858)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -2.032 2.286) (xy -3.556 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.762 2.794) (xy -2.286 4.318)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0.762) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.778) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.254 2.667) (xy 1.27 2.667)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 3.175) (xy 0.762 2.159)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 3.048) (xy -2.032 2.286) (xy -2.794 2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.762 3.556) (xy -0.762 2.794) (xy -1.524 2.794)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Solar_Cell_1_1"
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "+")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 2.54)
					(name "-")
					(number "2")
				)
			)
		)
		(symbol "Motor:Motor_DC"
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "M"
				(at 2.54 2.54 0)
			)
			(property "Value" "Motor_DC"
				(at 2.54 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 -2.286 0)
			)
			(property "Datasheet" "~"
				(at 0 -2.286 0)
			)
			(property "Description" "DC Motor"
				(at 0 0 0)
			)
			(property "ki_keywords" "DC Motor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "PinHeader*P2.54mm* TerminalBlock*"
				(at 0 0 0)
			)
			(symbol "Motor_DC_0_0"
				(polyline
					(pts
						(xy -1.27 -3.302) (xy -1.27 0.508) (xy 0 -2.032) (xy 1.27 0.508) (xy 1.27 -3.302)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Motor_DC_0_1"
				(circle
					(center 0 -1.524)
					(radius 3.2512)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 0 -7.112)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -4.7752) (xy 0 -5.1816)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.7272) (xy 0 2.0828)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.032) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Motor_DC_1_1"
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "+")
					(number "1")
				)
				(pin passive line
					(at 0 -7.62 90)
					(length 2.54)
					(name "-")
					(number "2")
				)
			)
		)
		(symbol "PCM_arduino-library:Arduino_Pro_Mini_Socket"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "A"
				(at 0 36.83 0)
			)
			(property "Value" "Arduino_Pro_Mini_Socket"
				(at 0 33.02 0)
			)
			(property "Footprint" "PCM_arduino-library:Arduino_Pro_Mini_Socket"
				(at 0 -36.83 0)
			)
			(property "Datasheet" "https://docs.arduino.cc/retired/boards/arduino-pro-mini"
				(at 0 -33.02 0)
			)
			(property "Description" "Socket for Arduino Pro Mini"
				(at 0 0 0)
			)
			(property "ki_keywords" "Arduino MPU Shield"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Arduino_Pro_Mini_Socket"
				(at 0 0 0)
			)
			(symbol "Arduino_Pro_Mini_Socket_0_0"
				(rectangle
					(start -17.78 30.48)
					(end 17.78 -29.21)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -7.62 10.16) (xy -6.35 10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -7.62 24.13) (xy -6.35 24.13)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -6.35 -22.86) (xy -8.89 -22.86)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -11.43 -16.51) (xy -5.08 -16.51) (xy -5.08 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 -7.62) (xy -5.08 -6.35) (xy -11.43 -6.35)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 2.54) (xy -2.54 -1.27) (xy -13.97 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 12.7) (xy -2.54 16.51) (xy -13.97 16.51)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -10.16 25.4) (xy -7.62 25.4) (xy -7.62 22.86) (xy -10.16 22.86)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -8.89 11.43) (xy -7.62 11.43) (xy -7.62 8.89) (xy -8.89 8.89)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 12.7 -11.43) (xy 10.16 -11.43) (xy 10.16 -16.51) (xy 10.16 -17.78) (xy 8.89 -17.78) (xy 10.16 -17.78)
						(xy 10.16 -24.13) (xy 12.7 -24.13)
					)
					(fill
						(type none)
					)
				)
				(text "Analog"
					(at -2.54 7.62 900)
				)
				(text "Header"
					(at 7.62 -17.78 900)
				)
				(text "I²C"
					(at -5.08 10.16 900)
				)
				(text "Misc."
					(at -5.08 -22.86 900)
				)
				(text "Power"
					(at -5.08 -11.43 900)
				)
				(text "Prog."
					(at 5.08 -17.78 900)
				)
				(text "Serial"
					(at -5.08 24.13 900)
				)
			)
			(symbol "Arduino_Pro_Mini_Socket_0_1"
				(polyline
					(pts
						(xy 7.62 -1.27) (xy 5.08 -1.27) (xy 5.08 8.89)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 26.67) (xy 5.08 26.67) (xy 5.08 16.51)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -10.16 -24.13) (xy -8.89 -24.13) (xy -8.89 -21.59) (xy -10.16 -21.59)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Arduino_Pro_Mini_Socket_1_0"
				(text "GPIO"
					(at 5.08 12.7 900)
				)
			)
			(symbol "Arduino_Pro_Mini_Socket_1_1"
				(pin bidirectional line
					(at -25.4 -1.27 0)
					(length 7.62)
					(name "A0")
					(number "A0")
				)
				(pin bidirectional line
					(at -25.4 1.27 0)
					(length 7.62)
					(name "A1")
					(number "A1")
				)
				(pin bidirectional line
					(at -25.4 3.81 0)
					(length 7.62)
					(name "A2")
					(number "A2")
				)
				(pin bidirectional line
					(at -25.4 6.35 0)
					(length 7.62)
					(name "A3")
					(number "A3")
				)
				(pin bidirectional line
					(at -25.4 8.89 0)
					(length 7.62)
					(name "A4/SDA")
					(number "A4")
				)
				(pin bidirectional clock
					(at -25.4 11.43 0)
					(length 7.62)
					(name "A5/SCL")
					(number "A5")
				)
				(pin input line
					(at -25.4 13.97 0)
					(length 7.62)
					(name "A6")
					(number "A6")
				)
				(pin input line
					(at -25.4 16.51 0)
					(length 7.62)
					(name "A7")
					(number "A7")
				)
				(pin bidirectional line
					(at -25.4 25.4 0)
					(length 7.62)
					(name "D0/RX")
					(number "D0")
				)
				(pin bidirectional line
					(at -25.4 22.86 0)
					(length 7.62)
					(name "D1/TX")
					(number "D1")
				)
				(pin bidirectional line
					(at 25.4 6.35 180)
					(length 7.62)
					(name "D10_CS")
					(number "D10")
				)
				(pin bidirectional line
					(at 25.4 3.81 180)
					(length 7.62)
					(name "D11_MOSI")
					(number "D11")
				)
				(pin bidirectional line
					(at 25.4 1.27 180)
					(length 7.62)
					(name "D12_MISO")
					(number "D12")
				)
				(pin bidirectional clock
					(at 25.4 -1.27 180)
					(length 7.62)
					(name "D13_SCK")
					(number "D13")
				)
				(pin bidirectional line
					(at 25.4 26.67 180)
					(length 7.62)
					(name "D2_INT0")
					(number "D2")
				)
				(pin bidirectional line
					(at 25.4 24.13 180)
					(length 7.62)
					(name "D3_INT1")
					(number "D3")
				)
				(pin bidirectional line
					(at 25.4 21.59 180)
					(length 7.62)
					(name "D4")
					(number "D4")
				)
				(pin bidirectional line
					(at 25.4 19.05 180)
					(length 7.62)
					(name "D5")
					(number "D5")
				)
				(pin bidirectional line
					(at 25.4 16.51 180)
					(length 7.62)
					(name "D6")
					(number "D6")
				)
				(pin bidirectional line
					(at 25.4 13.97 180)
					(length 7.62)
					(name "D7")
					(number "D7")
				)
				(pin bidirectional line
					(at 25.4 11.43 180)
					(length 7.62)
					(name "D8")
					(number "D8")
				)
				(pin bidirectional line
					(at 25.4 8.89 180)
					(length 7.62)
					(name "D9")
					(number "D9")
				)
				(pin input input_low
					(at 25.4 -11.43 180)
					(length 7.62)
					(name "~{DTR}")
					(number "DTR")
				)
				(pin power_in line
					(at -25.4 -13.97 0)
					(length 7.62)
					(name "GND")
					(number "GND1")
				)
				(pin power_in line
					(at -25.4 -16.51 0)
					(length 7.62)
					(name "GND")
					(number "GND2")
				)
				(pin power_in line
					(at 25.4 -21.59 180)
					(length 7.62)
					(name "GND")
					(number "GND4")
				)
				(pin power_in line
					(at 25.4 -24.13 180)
					(length 7.62)
					(name "GND")
					(number "GND5")
				)
				(pin power_in line
					(at -25.4 -6.35 0)
					(length 7.62)
					(name "RAW")
					(number "RAW")
				)
				(pin open_collector input_low
					(at -25.4 -21.59 0)
					(length 7.62)
					(name "RESET")
					(number "RST1")
				)
				(pin open_collector input_low
					(at -25.4 -24.13 0)
					(length 7.62)
					(name "RESET")
					(number "RST2")
				)
				(pin input line
					(at 25.4 -16.51 180)
					(length 7.62)
					(name "RXI")
					(number "RXI")
				)
				(pin output line
					(at 25.4 -13.97 180)
					(length 7.62)
					(name "TXO")
					(number "TXO")
				)
				(pin power_in line
					(at -25.4 -8.89 0)
					(length 7.62)
					(name "Vcc")
					(number "Vcc1")
				)
				(pin power_in line
					(at 25.4 -19.05 180)
					(length 7.62)
					(name "Vcc")
					(number "Vcc2")
				)
			)
		)
		(symbol "RF_Module:RFM95W-868S2"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -10.414 11.684 0)
			)
			(property "Value" "RFM95W-868S2"
				(at 1.524 11.43 0)
			)
			(property "Footprint" ""
				(at -83.82 41.91 0)
			)
			(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf"
				(at -83.82 41.91 0)
			)
			(property "Description" "Low power long range transceiver module, SPI and parallel interface, 868 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16"
				(at 0 0 0)
			)
			(property "ki_keywords" "Low power long range transceiver module"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "HOPERF*RFM9XW*"
				(at 0 0 0)
			)
			(symbol "RFM95W-868S2_0_1"
				(rectangle
					(start -10.16 10.16)
					(end 10.16 -12.7)
					(fill
						(type background)
					)
				)
			)
			(symbol "RFM95W-868S2_1_1"
				(pin power_in line
					(at -2.54 -15.24 90)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 2.54 -15.24 90)
					(length 2.54)
					(name "GND")
					(number "10")
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "DIO3")
					(number "11")
				)
				(pin bidirectional line
					(at 12.7 0 180)
					(length 2.54)
					(name "DIO4")
					(number "12")
				)
				(pin power_in line
					(at 0 12.7 270)
					(length 2.54)
					(name "3.3V")
					(number "13")
				)
				(pin bidirectional line
					(at 12.7 -10.16 180)
					(length 2.54)
					(name "DIO0")
					(number "14")
				)
				(pin bidirectional line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "DIO1")
					(number "15")
				)
				(pin bidirectional line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "DIO2")
					(number "16")
				)
				(pin output line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "MISO")
					(number "2")
				)
				(pin input line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "MOSI")
					(number "3")
				)
				(pin input line
					(at -12.7 7.62 0)
					(length 2.54)
					(name "SCK")
					(number "4")
				)
				(pin input line
					(at -12.7 0 0)
					(length 2.54)
					(name "NSS")
					(number "5")
				)
				(pin bidirectional line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "RESET")
					(number "6")
				)
				(pin bidirectional line
					(at 12.7 2.54 180)
					(length 2.54)
					(name "DIO5")
					(number "7")
				)
				(pin power_in line
					(at 0 -15.24 90)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin bidirectional line
					(at 12.7 7.62 180)
					(length 2.54)
					(name "ANT")
					(number "9")
				)
			)
		)
		(symbol "power:+BATT"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+BATT"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+BATT\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power battery"
				(at 0 0 0)
			)
			(symbol "+BATT_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+BATT_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "watering:Driver_Motor{colon}Pololu_MP6550"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "MP1"
				(at -0.635 16.51 0)
			)
			(property "Value" "~"
				(at -0.635 13.97 0)
			)
			(property "Footprint" "watering:MP6550"
				(at -5.08 13.97 0)
			)
			(property "Datasheet" ""
				(at -5.08 13.97 0)
			)
			(property "Description" ""
				(at -5.08 13.97 0)
			)
			(symbol "Driver_Motor{colon}Pololu_MP6550_1_1"
				(rectangle
					(start -10.16 12.7)
					(end 8.89 -11.43)
					(fill
						(type background)
					)
				)
				(pin power_out line
					(at 11.43 7.62 180)
					(length 2.54)
					(name "VM")
					(number "1")
				)
				(pin output line
					(at 11.43 -1.27 180)
					(length 2.54)
					(name "OUT2")
					(number "10")
				)
				(pin power_out line
					(at -12.7 -10.16 0)
					(length 2.54)
					(name "GND")
					(number "11")
				)
				(pin power_in line
					(at 11.43 11.43 180)
					(length 2.54)
					(name "VIN")
					(number "12")
				)
				(pin power_out line
					(at -12.7 -6.35 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin input line
					(at -12.7 8.89 0)
					(length 2.54)
					(name "IN2")
					(number "3")
				)
				(pin input line
					(at -12.7 11.43 0)
					(length 2.54)
					(name "IN1")
					(number "4")
				)
				(pin input line
					(at 11.43 -7.62 180)
					(length 2.54)
					(name "VISEN")
					(number "5")
				)
				(pin input line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "nSLEEP_HB")
					(number "6")
				)
				(pin power_out line
					(at 11.43 2.54 180)
					(length 2.54)
					(name "V3P3")
					(number "7")
				)
				(pin free line
					(at -12.7 -1.27 0)
					(length 2.54)
					(name "ISET")
					(number "8")
				)
				(pin output line
					(at 11.43 -3.81 180)
					(length 2.54)
					(name "OUT1")
					(number "9")
				)
			)
		)
	)
	(junction
		(at 229.87 59.69)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 86.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 40.64 82.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 229.87 59.69) (xy 229.87 62.23)
		)
	)
	(wire
		(pts
			(xy 158.75 40.64) (xy 158.75 110.49)
		)
	)
	(wire
		(pts
			(xy 110.49 45.72) (xy 171.45 45.72)
		)
	)
	(wire
		(pts
			(xy 50.8 50.8) (xy 50.8 63.5)
		)
	)
	(wire
		(pts
			(xy 229.87 72.39) (xy 229.87 86.36)
		)
	)
	(wire
		(pts
			(xy 229.87 59.69) (xy 195.58 59.69)
		)
	)
	(wire
		(pts
			(xy 156.21 95.25) (xy 182.88 95.25)
		)
	)
	(wire
		(pts
			(xy 44.45 73.66) (xy 44.45 48.26)
		)
	)
	(wire
		(pts
			(xy 123.19 58.42) (xy 123.19 102.87)
		)
	)
	(wire
		(pts
			(xy 163.83 82.55) (xy 133.35 82.55)
		)
	)
	(wire
		(pts
			(xy 110.49 63.5) (xy 128.27 63.5)
		)
	)
	(wire
		(pts
			(xy 156.21 110.49) (xy 158.75 110.49)
		)
	)
	(wire
		(pts
			(xy 110.49 43.18) (xy 142.24 43.18)
		)
	)
	(wire
		(pts
			(xy 125.73 60.96) (xy 125.73 97.79)
		)
	)
	(wire
		(pts
			(xy 195.58 73.66) (xy 198.12 73.66)
		)
	)
	(wire
		(pts
			(xy 110.49 55.88) (xy 120.65 55.88)
		)
	)
	(wire
		(pts
			(xy 168.91 48.26) (xy 168.91 60.96)
		)
	)
	(wire
		(pts
			(xy 241.3 34.29) (xy 246.38 34.29)
		)
	)
	(wire
		(pts
			(xy 110.49 38.1) (xy 133.35 38.1)
		)
	)
	(wire
		(pts
			(xy 246.38 34.29) (xy 246.38 86.36)
		)
	)
	(wire
		(pts
			(xy 123.19 102.87) (xy 130.81 102.87)
		)
	)
	(wire
		(pts
			(xy 44.45 48.26) (xy 35.56 48.26)
		)
	)
	(wire
		(pts
			(xy 29.21 82.55) (xy 40.64 82.55)
		)
	)
	(wire
		(pts
			(xy 229.87 86.36) (xy 246.38 86.36)
		)
	)
	(wire
		(pts
			(xy 110.49 60.96) (xy 125.73 60.96)
		)
	)
	(wire
		(pts
			(xy 168.91 60.96) (xy 171.45 60.96)
		)
	)
	(wire
		(pts
			(xy 50.8 63.5) (xy 59.69 63.5)
		)
	)
	(wire
		(pts
			(xy 59.69 73.66) (xy 44.45 73.66)
		)
	)
	(wire
		(pts
			(xy 163.83 113.03) (xy 163.83 82.55)
		)
	)
	(wire
		(pts
			(xy 198.12 73.66) (xy 198.12 106.68)
		)
	)
	(wire
		(pts
			(xy 110.49 40.64) (xy 158.75 40.64)
		)
	)
	(wire
		(pts
			(xy 142.24 43.18) (xy 142.24 64.77)
		)
	)
	(wire
		(pts
			(xy 233.68 34.29) (xy 229.87 34.29)
		)
	)
	(wire
		(pts
			(xy 204.47 71.12) (xy 204.47 93.98)
		)
	)
	(wire
		(pts
			(xy 171.45 45.72) (xy 171.45 58.42)
		)
	)
	(wire
		(pts
			(xy 128.27 100.33) (xy 130.81 100.33)
		)
	)
	(wire
		(pts
			(xy 110.49 66.04) (xy 130.81 66.04)
		)
	)
	(wire
		(pts
			(xy 128.27 63.5) (xy 128.27 100.33)
		)
	)
	(wire
		(pts
			(xy 133.35 82.55) (xy 133.35 38.1)
		)
	)
	(wire
		(pts
			(xy 59.69 66.04) (xy 40.64 66.04)
		)
	)
	(wire
		(pts
			(xy 130.81 66.04) (xy 130.81 95.25)
		)
	)
	(wire
		(pts
			(xy 130.81 97.79) (xy 125.73 97.79)
		)
	)
	(wire
		(pts
			(xy 40.64 66.04) (xy 40.64 82.55)
		)
	)
	(wire
		(pts
			(xy 195.58 71.12) (xy 204.47 71.12)
		)
	)
	(wire
		(pts
			(xy 156.21 113.03) (xy 163.83 113.03)
		)
	)
	(wire
		(pts
			(xy 110.49 48.26) (xy 168.91 48.26)
		)
	)
	(wire
		(pts
			(xy 110.49 58.42) (xy 123.19 58.42)
		)
	)
	(wire
		(pts
			(xy 35.56 50.8) (xy 50.8 50.8)
		)
	)
	(wire
		(pts
			(xy 142.24 64.77) (xy 171.45 64.77)
		)
	)
	(wire
		(pts
			(xy 120.65 107.95) (xy 130.81 107.95)
		)
	)
	(wire
		(pts
			(xy 198.12 106.68) (xy 204.47 106.68)
		)
	)
	(wire
		(pts
			(xy 120.65 55.88) (xy 120.65 107.95)
		)
	)
	(wire
		(pts
			(xy 195.58 59.69) (xy 195.58 58.42)
		)
	)
	(wire
		(pts
			(xy 229.87 58.42) (xy 229.87 59.69)
		)
	)
	(wire
		(pts
			(xy 229.87 34.29) (xy 229.87 50.8)
		)
	)
	(symbol
		(lib_id "power:+BATT")
		(at 40.64 90.17 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR07"
			(at 40.64 86.36 0)
		)
		(property "Value" "+BATT"
			(at 40.64 95.25 0)
		)
		(property "Footprint" ""
			(at 40.64 90.17 0)
		)
		(property "Datasheet" ""
			(at 40.64 90.17 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+BATT\""
			(at 40.64 90.17 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 40.64 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 43.18 85.0899 0)
		)
		(property "Value" "R"
			(at 43.18 87.6299 0)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 38.862 86.36 90)
		)
		(property "Datasheet" "~"
			(at 40.64 86.36 0)
		)
		(property "Description" "Resistor"
			(at 40.64 86.36 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:Solar_Cell")
		(at 238.76 34.29 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SC1"
			(at 236.601 27.94 90)
		)
		(property "Value" "Solar_Cell"
			(at 236.601 30.48 90)
		)
		(property "Footprint" "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
			(at 237.236 34.29 90)
		)
		(property "Datasheet" "~"
			(at 237.236 34.29 90)
		)
		(property "Description" "Single solar cell"
			(at 238.76 34.29 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Watering"
				(path
					(reference "SC1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 29.21 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 31.75 85.0899 0)
		)
		(property "Value" "R"
			(at 31.75 87.6299 0)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 27.432 86.36 90)
		)
		(property "Datasheet" "~"
			(at 29.21 86.36 0)
		)
		(property "Description" "Resistor"
			(at 29.21 86.36 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x03_Pin")
		(at 30.48 50.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J1"
			(at 31.115 43.18 0)
		)
		(property "Value" "Moisture sensor"
			(at 31.115 45.72 0)
		)
		(property "Footprint" "Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical"
			(at 30.48 50.8 0)
		)
		(property "Datasheet" "~"
			(at 30.48 50.8 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 30.48 50.8 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project ""
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 171.45 76.2 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR05"
			(at 165.1 76.2 0)
		)
		(property "Value" "GND"
			(at 167.64 76.1999 90)
		)
		(property "Footprint" ""
			(at 171.45 76.2 0)
		)
		(property "Datasheet" ""
			(at 171.45 76.2 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 171.45 76.2 0)
		)
		(pin "1")
		(instances
			(project "Watering"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 29.21 90.17 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR06"
			(at 29.21 96.52 0)
		)
		(property "Value" "GND"
			(at 29.21 95.25 0)
		)
		(property "Footprint" ""
			(at 29.21 90.17 0)
		)
		(property "Datasheet" ""
			(at 29.21 90.17 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 29.21 90.17 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 35.56 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR8"
			(at 35.56 59.69 0)
		)
		(property "Value" "GND"
			(at 35.56 58.42 0)
		)
		(property "Footprint" ""
			(at 35.56 53.34 0)
		)
		(property "Datasheet" ""
			(at 35.56 53.34 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 35.56 53.34 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+BATT")
		(at 59.69 71.12 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 63.5 71.12 0)
		)
		(property "Value" "+BATT"
			(at 55.88 71.1199 90)
		)
		(property "Footprint" ""
			(at 59.69 71.12 0)
		)
		(property "Datasheet" ""
			(at 59.69 71.12 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+BATT\""
			(at 59.69 71.12 0)
		)
		(pin "1")
		(instances
			(project "Watering"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PCM_arduino-library:Arduino_Pro_Mini_Socket")
		(at 85.09 64.77 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "A1"
			(at 85.09 29.21 0)
		)
		(property "Value" "Arduino_Pro_Mini_Socket"
			(at 85.09 31.75 0)
		)
		(property "Footprint" "PCM_arduino-library:Arduino_Pro_Mini_Socket"
			(at 85.09 101.6 0)
		)
		(property "Datasheet" "https://docs.arduino.cc/retired/boards/arduino-pro-mini"
			(at 85.09 97.79 0)
		)
		(property "Description" "Socket for Arduino Pro Mini"
			(at 85.09 64.77 0)
		)
		(pin "D5")
		(pin "TXO")
		(pin "Vcc2")
		(pin "RXI")
		(pin "D6")
		(pin "D11")
		(pin "A1")
		(pin "A4")
		(pin "A3")
		(pin "A2")
		(pin "D8")
		(pin "D7")
		(pin "RAW")
		(pin "D3")
		(pin "GND4")
		(pin "GND2")
		(pin "Vcc1")
		(pin "D4")
		(pin "D2")
		(pin "D12")
		(pin "RST2")
		(pin "A0")
		(pin "A7")
		(pin "RST1")
		(pin "A5")
		(pin "D9")
		(pin "A6")
		(pin "D1")
		(pin "D0")
		(pin "GND5")
		(pin "DTR")
		(pin "D13")
		(pin "D10")
		(pin "GND1")
		(instances
			(project "Watering"
				(path
					(reference "A1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Motor:Motor_DC")
		(at 204.47 99.06 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "M1"
			(at 209.55 100.3299 0)
		)
		(property "Value" "Motor_DC"
			(at 209.55 102.8699 0)
		)
		(property "Footprint" "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
			(at 204.47 101.346 0)
		)
		(property "Datasheet" "~"
			(at 204.47 101.346 0)
		)
		(property "Description" "DC Motor"
			(at 204.47 99.06 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Watering"
				(path
					(reference "M1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "RF_Module:RFM95W-868S2")
		(at 143.51 102.87 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 145.7041 87.63 0)
		)
		(property "Value" "RFM95W-868S2"
			(at 145.7041 90.17 0)
		)
		(property "Footprint" "RF_Module:HOPERF_RFM9XW_THT"
			(at 59.69 60.96 0)
		)
		(property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf"
			(at 59.69 60.96 0)
		)
		(property "Description" "Low power long range transceiver module, SPI and parallel interface, 868 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16"
			(at 143.51 102.87 0)
		)
		(pin "3")
		(pin "13")
		(pin "2")
		(pin "9")
		(pin "4")
		(pin "15")
		(pin "7")
		(pin "6")
		(pin "8")
		(pin "1")
		(pin "14")
		(pin "5")
		(pin "11")
		(pin "10")
		(pin "16")
		(pin "12")
		(instances
			(project "Watering"
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:Battery")
		(at 229.87 67.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "BT1"
			(at 233.68 65.4684 0)
		)
		(property "Value" "Battery"
			(at 233.68 68.0084 0)
		)
		(property "Footprint" "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
			(at 229.87 65.786 90)
		)
		(property "Datasheet" "~"
			(at 229.87 65.786 90)
		)
		(property "Description" "Multiple-cell battery"
			(at 229.87 67.31 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Watering"
				(path
					(reference "BT1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 59.69 78.74 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 53.34 78.74 0)
		)
		(property "Value" "GND"
			(at 55.88 78.7399 90)
		)
		(property "Footprint" ""
			(at 59.69 78.74 0)
		)
		(property "Datasheet" ""
			(at 59.69 78.74 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 59.69 78.74 0)
		)
		(pin "1")
		(instances
			(project "Watering"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+BATT")
		(at 229.87 59.69 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 226.06 59.69 0)
		)
		(property "Value" "+BATT"
			(at 233.68 59.6899 90)
		)
		(property "Footprint" ""
			(at 229.87 59.69 0)
		)
		(property "Datasheet" ""
			(at 229.87 59.69 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+BATT\""
			(at 229.87 59.69 0)
		)
		(pin "1")
		(instances
			(project "Watering"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 229.87 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 229.87 92.71 0)
		)
		(property "Value" "GND"
			(at 229.87 91.44 0)
		)
		(property "Footprint" ""
			(at 229.87 86.36 0)
		)
		(property "Datasheet" ""
			(at 229.87 86.36 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 229.87 86.36 0)
		)
		(pin "1")
		(instances
			(project "Watering"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:Antenna")
		(at 182.88 90.17 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "AE1"
			(at 185.42 89.5349 0)
		)
		(property "Value" "Antenna"
			(at 185.42 92.0749 0)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical"
			(at 182.88 90.17 0)
		)
		(property "Datasheet" "~"
			(at 182.88 90.17 0)
		)
		(property "Description" "Antenna"
			(at 182.88 90.17 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "AE1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:D")
		(at 229.87 54.61 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 232.41 53.3399 90)
		)
		(property "Value" "D"
			(at 232.41 55.8799 90)
		)
		(property "Footprint" "Diode_THT:D_T-1_P10.16mm_Horizontal"
			(at 229.87 54.61 0)
		)
		(property "Datasheet" "~"
			(at 229.87 54.61 0)
		)
		(property "Description" "Diode"
			(at 229.87 54.61 0)
		)
		(property "Sim.Device" "D"
			(at 229.87 54.61 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 229.87 54.61 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Watering"
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "watering:Driver_Motor{colon}Pololu_MP6550")
		(at 184.15 69.85 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "MP1"
			(at 183.515 53.34 0)
		)
		(property "Value" "~"
			(at 183.515 55.88 0)
		)
		(property "Footprint" "watering:MP6550"
			(at 179.07 55.88 0)
		)
		(property "Datasheet" ""
			(at 179.07 55.88 0)
		)
		(property "Description" ""
			(at 179.07 55.88 0)
		)
		(pin "3")
		(pin "4")
		(pin "1")
		(pin "11")
		(pin "6")
		(pin "5")
		(pin "7")
		(pin "8")
		(pin "10")
		(pin "9")
		(pin "12")
		(pin "2")
		(instances
			(project "Watering"
				(path
					(reference "MP1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
