(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+5V")
	(net 2 "GND")
	(net 3 "+19V")
	(net 4 "unconnected-(U1-Clock-Pad6)")
	(net 5 "unconnected-(U1-UART-Pad4)")
	(net 6 "unconnected-(U1-VREF-Pad9)")
	(net 7 "unconnected-(U1-DIAG-Pad10)")
	(net 8 "unconnected-(U1-UART-Pad5)")
	(net 9 "unconnected-(U2-UART-Pad5)")
	(net 10 "unconnected-(U2-UART-Pad4)")
	(net 11 "unconnected-(U2-Clock-Pad6)")
	(net 12 "unconnected-(U2-VREF-Pad9)")
	(net 13 "unconnected-(U2-DIAG-Pad10)")
	(net 14 "unconnected-(U3-UART-Pad4)")
	(net 15 "unconnected-(U3-UART-Pad5)")
	(net 16 "unconnected-(U3-VREF-Pad9)")
	(net 17 "unconnected-(U3-DIAG-Pad10)")
	(net 18 "unconnected-(U3-Clock-Pad6)")
	(net 19 "unconnected-(U4-UART-Pad5)")
	(net 20 "unconnected-(U4-VREF-Pad9)")
	(net 21 "unconnected-(U4-Clock-Pad6)")
	(net 22 "Net-(JMS1-C)")
	(net 23 "Net-(JMS2-C)")
	(net 24 "unconnected-(U4-UART-Pad4)")
	(net 25 "unconnected-(U4-DIAG-Pad10)")
	(net 26 "Net-(CM1-Pin_1)")
	(net 27 "Net-(CM1-Pin_4)")
	(net 28 "Net-(CM1-Pin_2)")
	(net 29 "Net-(CM1-Pin_3)")
	(net 30 "Net-(CM2-Pin_3)")
	(net 31 "Net-(CM2-Pin_4)")
	(net 32 "Net-(CM2-Pin_1)")
	(net 33 "Net-(CM2-Pin_2)")
	(net 34 "Net-(CM3-Pin_4)")
	(net 35 "Net-(CM3-Pin_2)")
	(net 36 "Net-(CM3-Pin_1)")
	(net 37 "Net-(CM3-Pin_3)")
	(net 38 "Net-(CM4-Pin_1)")
	(net 39 "Net-(CM4-Pin_3)")
	(net 40 "Net-(CM4-Pin_4)")
	(net 41 "Net-(CM4-Pin_2)")
	(net 42 "Net-(ArduinoConnection1-D7)")
	(net 43 "Net-(ArduinoConnection1-D2)")
	(net 44 "Net-(ArduinoConnection1-D4)")
	(net 45 "Net-(ArduinoConnection1-D8)")
	(net 46 "Net-(ArduinoConnection1-D6)")
	(net 47 "Net-(ArduinoConnection1-D11)")
	(net 48 "Net-(ArduinoConnection1-D3)")
	(net 49 "Net-(ArduinoConnection1-D10)")
	(net 50 "Net-(ArduinoConnection1-D9)")
	(net 51 "Net-(ArduinoConnection1-D5)")
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 111.76 128.28)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "CM3"
			(at 3.81 4.435 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 9.95 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(CM3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(CM3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(CM3-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(CM3-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 111.785 118.765)
		(descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x02 2.54mm single row")
		(property "Reference" "SW2"
			(at 3.785 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW_SPDT_XKB_DMx-xxxx-1"
			(at 0 5.31 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Position switch"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW?XKB?DM??16U??1*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(ArduinoConnection1-D10)")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
		(layer "F.Cu")
		(at 86.868 157.988 90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers")
		(tags "solder jumper open")
		(property "Reference" "JMS2"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_3_Open"
			(at 0 1.9 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "0v"
			(at 1.2 2.005 90)
			(layer "F.SilkS")
		)
		(fp_text user "5v"
			(at -1.8 2.005 90)
			(layer "F.SilkS")
		)
		(pad "1" smd custom
			(at -1.3 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "+5V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 23 "Net-(JMS2-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.55 0.75) (xy -0.55 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 111.76 86.36)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "CM1"
			(at 3.81 3.81 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 9.95 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(CM1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(CM1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(CM1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(CM1-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TMC2209:Bigtreetech_TMC2209"
		(layer "F.Cu")
		(at 99.695 107.315)
		(property "Reference" "U2"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "TMC2209:Bigtreetech_TMC2209"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -7.62 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(ArduinoConnection1-D11)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.62 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(JMS1-C)")
			(pinfunction "MS1")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at -7.62 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(JMS2-C)")
			(pinfunction "MS2")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -7.62 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(U2-UART-Pad4)")
			(pinfunction "UART")
			(pintype "input+no_connect")
		)
		(pad "5" thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(U2-UART-Pad5)")
			(pinfunction "UART")
			(pintype "input+no_connect")
		)
		(pad "6" thru_hole circle
			(at -7.62 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(U2-Clock-Pad6)")
			(pinfunction "Clock")
			(pintype "input+no_connect")
		)
		(pad "7" thru_hole circle
			(at -7.62 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(ArduinoConnection1-D5)")
			(pinfunction "STEP")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at -7.62 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(ArduinoConnection1-D4)")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "9" thru_hole roundrect
			(at -5.08 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 12 "unconnected-(U2-VREF-Pad9)")
			(pinfunction "VREF")
			(pintype "passive+no_connect")
		)
		(pad "10" thru_hole roundrect
			(at -2.54 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 13 "unconnected-(U2-DIAG-Pad10)")
			(pinfunction "DIAG")
			(pintype "passive+no_connect")
		)
		(pad "11" thru_hole rect
			(at 5.08 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+19V")
			(pinfunction "VM")
			(pintype "power_in")
		)
		(pad "12" thru_hole circle
			(at 5.08 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 5.08 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(CM2-Pin_3)")
			(pinfunction "A2")
			(pintype "output")
		)
		(pad "14" thru_hole circle
			(at 5.08 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(CM2-Pin_1)")
			(pinfunction "A1")
			(pintype "output")
		)
		(pad "15" thru_hole circle
			(at 5.08 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(CM2-Pin_2)")
			(pinfunction "B1")
			(pintype "output")
		)
		(pad "16" thru_hole circle
			(at 5.08 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(CM2-Pin_4)")
			(pinfunction "B2")
			(pintype "output")
		)
		(pad "17" thru_hole circle
			(at 5.08 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "VCC_IO")
			(pintype "power_in")
		)
		(pad "18" thru_hole circle
			(at 5.08 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "19" thru_hole roundrect
			(at -3.81 -3.175)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left top_right bottom_left bottom_right)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 115 164)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "TMC2209:Bigtreetech_TMC2209"
		(layer "F.Cu")
		(at 99.645 86.36)
		(property "Reference" "U1"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "TMC2209:Bigtreetech_TMC2209"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -7.62 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(ArduinoConnection1-D11)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.62 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(JMS1-C)")
			(pinfunction "MS1")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at -7.62 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(JMS2-C)")
			(pinfunction "MS2")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -7.62 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(U1-UART-Pad4)")
			(pinfunction "UART")
			(pintype "input+no_connect")
		)
		(pad "5" thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(U1-UART-Pad5)")
			(pinfunction "UART")
			(pintype "input+no_connect")
		)
		(pad "6" thru_hole circle
			(at -7.62 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(U1-Clock-Pad6)")
			(pinfunction "Clock")
			(pintype "input+no_connect")
		)
		(pad "7" thru_hole circle
			(at -7.62 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(ArduinoConnection1-D3)")
			(pinfunction "STEP")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at -7.62 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(ArduinoConnection1-D2)")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "9" thru_hole roundrect
			(at -5.08 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 6 "unconnected-(U1-VREF-Pad9)")
			(pinfunction "VREF")
			(pintype "passive+no_connect")
		)
		(pad "10" thru_hole roundrect
			(at -2.54 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 7 "unconnected-(U1-DIAG-Pad10)")
			(pinfunction "DIAG")
			(pintype "passive+no_connect")
		)
		(pad "11" thru_hole rect
			(at 5.08 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+19V")
			(pinfunction "VM")
			(pintype "power_in")
		)
		(pad "12" thru_hole circle
			(at 5.08 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 5.08 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(CM1-Pin_3)")
			(pinfunction "A2")
			(pintype "output")
		)
		(pad "14" thru_hole circle
			(at 5.08 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(CM1-Pin_1)")
			(pinfunction "A1")
			(pintype "output")
		)
		(pad "15" thru_hole circle
			(at 5.08 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(CM1-Pin_2)")
			(pinfunction "B1")
			(pintype "output")
		)
		(pad "16" thru_hole circle
			(at 5.08 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(CM1-Pin_4)")
			(pinfunction "B2")
			(pintype "output")
		)
		(pad "17" thru_hole circle
			(at 5.08 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "VCC_IO")
			(pintype "power_in")
		)
		(pad "18" thru_hole circle
			(at 5.08 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "19" thru_hole roundrect
			(at -3.81 -3.175)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left top_right bottom_left bottom_right)
		)
	)
	(footprint "TMC2209:Bigtreetech_TMC2209"
		(layer "F.Cu")
		(at 99.695 128.27)
		(property "Reference" "U3"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "TMC2209:Bigtreetech_TMC2209"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -7.62 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(ArduinoConnection1-D11)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.62 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(JMS1-C)")
			(pinfunction "MS1")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at -7.62 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(JMS2-C)")
			(pinfunction "MS2")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -7.62 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(U3-UART-Pad4)")
			(pinfunction "UART")
			(pintype "input+no_connect")
		)
		(pad "5" thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(U3-UART-Pad5)")
			(pinfunction "UART")
			(pintype "input+no_connect")
		)
		(pad "6" thru_hole circle
			(at -7.62 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(U3-Clock-Pad6)")
			(pinfunction "Clock")
			(pintype "input+no_connect")
		)
		(pad "7" thru_hole circle
			(at -7.62 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(ArduinoConnection1-D6)")
			(pinfunction "STEP")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at -7.62 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(ArduinoConnection1-D7)")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "9" thru_hole roundrect
			(at -5.08 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 16 "unconnected-(U3-VREF-Pad9)")
			(pinfunction "VREF")
			(pintype "passive+no_connect")
		)
		(pad "10" thru_hole roundrect
			(at -2.54 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 17 "unconnected-(U3-DIAG-Pad10)")
			(pinfunction "DIAG")
			(pintype "passive+no_connect")
		)
		(pad "11" thru_hole rect
			(at 5.08 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+19V")
			(pinfunction "VM")
			(pintype "power_in")
		)
		(pad "12" thru_hole circle
			(at 5.08 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 5.08 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(CM3-Pin_3)")
			(pinfunction "A2")
			(pintype "output")
		)
		(pad "14" thru_hole circle
			(at 5.08 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(CM3-Pin_1)")
			(pinfunction "A1")
			(pintype "output")
		)
		(pad "15" thru_hole circle
			(at 5.08 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(CM3-Pin_2)")
			(pinfunction "B1")
			(pintype "output")
		)
		(pad "16" thru_hole circle
			(at 5.08 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(CM3-Pin_4)")
			(pinfunction "B2")
			(pintype "output")
		)
		(pad "17" thru_hole circle
			(at 5.08 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "VCC_IO")
			(pintype "power_in")
		)
		(pad "18" thru_hole circle
			(at 5.08 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "19" thru_hole roundrect
			(at -3.81 -3.175)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left top_right bottom_left bottom_right)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 111.76 139.7)
		(descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x02 2.54mm single row")
		(property "Reference" "SW3"
			(at 3.81 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW_SPDT_XKB_DMx-xxxx-1"
			(at 0 5.31 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Position switch"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW?XKB?DM??16U??1*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(ArduinoConnection1-D10)")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TMC2209:Bigtreetech_TMC2209"
		(layer "F.Cu")
		(at 99.695 149.225)
		(property "Reference" "U4"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "TMC2209:Bigtreetech_TMC2209"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -7.62 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(ArduinoConnection1-D11)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.62 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(JMS1-C)")
			(pinfunction "MS1")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at -7.62 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(JMS2-C)")
			(pinfunction "MS2")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -7.62 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(U4-UART-Pad4)")
			(pinfunction "UART")
			(pintype "input+no_connect")
		)
		(pad "5" thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(U4-UART-Pad5)")
			(pinfunction "UART")
			(pintype "input+no_connect")
		)
		(pad "6" thru_hole circle
			(at -7.62 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(U4-Clock-Pad6)")
			(pinfunction "Clock")
			(pintype "input+no_connect")
		)
		(pad "7" thru_hole circle
			(at -7.62 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(ArduinoConnection1-D9)")
			(pinfunction "STEP")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at -7.62 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(ArduinoConnection1-D8)")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "9" thru_hole roundrect
			(at -5.08 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 20 "unconnected-(U4-VREF-Pad9)")
			(pinfunction "VREF")
			(pintype "passive+no_connect")
		)
		(pad "10" thru_hole roundrect
			(at -2.54 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 25 "unconnected-(U4-DIAG-Pad10)")
			(pinfunction "DIAG")
			(pintype "passive+no_connect")
		)
		(pad "11" thru_hole rect
			(at 5.08 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+19V")
			(pinfunction "VM")
			(pintype "power_in")
		)
		(pad "12" thru_hole circle
			(at 5.08 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 5.08 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(CM4-Pin_3)")
			(pinfunction "A2")
			(pintype "output")
		)
		(pad "14" thru_hole circle
			(at 5.08 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(CM4-Pin_1)")
			(pinfunction "A1")
			(pintype "output")
		)
		(pad "15" thru_hole circle
			(at 5.08 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(CM4-Pin_2)")
			(pinfunction "B1")
			(pintype "output")
		)
		(pad "16" thru_hole circle
			(at 5.08 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(CM4-Pin_4)")
			(pinfunction "B2")
			(pintype "output")
		)
		(pad "17" thru_hole circle
			(at 5.08 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "VCC_IO")
			(pintype "power_in")
		)
		(pad "18" thru_hole circle
			(at 5.08 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "19" thru_hole roundrect
			(at -3.81 -3.175)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left top_right bottom_left bottom_right)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 108 160.655)
		(descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x02 2.54mm single row")
		(property "Reference" "SW4"
			(at 0 -2.655 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW_SPDT_XKB_DMx-xxxx-1"
			(at 0 5.31 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Position switch"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW?XKB?DM??16U??1*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(ArduinoConnection1-D10)")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 93.975 76.2 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "Pwr5v1"
			(at 1.905 -2.535 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
		(layer "F.Cu")
		(at 86.868 151.638 90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers")
		(tags "solder jumper open")
		(property "Reference" "JMS1"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_3_Open"
			(at 0 1.9 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "5v"
			(at -1.15 2.005 90)
			(layer "F.SilkS")
		)
		(fp_text user "0v"
			(at 1.85 2.005 90)
			(layer "F.SilkS")
		)
		(pad "1" smd custom
			(at -1.3 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "+5V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 22 "Net-(JMS1-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.55 0.75) (xy -0.55 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 86.106 124.714 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R_EN1"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 5.08 2.37 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 -2.286 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(ArduinoConnection1-D11)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 111.76 107.325)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "CM2"
			(at 3.81 3.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 9.95 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(CM2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(CM2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(CM2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(CM2-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 115 73)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 1 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 87 164)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 86.36 86.995)
		(descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x10 2.54mm single row")
		(property "Reference" "ArduinoConnection1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x10_Pin"
			(at 0 25.19 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -1.905 10.795 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(ArduinoConnection1-D2)")
			(pinfunction "D2")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(ArduinoConnection1-D3)")
			(pinfunction "D3")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(ArduinoConnection1-D4)")
			(pinfunction "D4")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(ArduinoConnection1-D5)")
			(pinfunction "D5")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(ArduinoConnection1-D6)")
			(pinfunction "D6")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(ArduinoConnection1-D7)")
			(pinfunction "D7")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(ArduinoConnection1-D8)")
			(pinfunction "D8")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(ArduinoConnection1-D9)")
			(pinfunction "D9")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(ArduinoConnection1-D10)")
			(pinfunction "D10")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(ArduinoConnection1-D11)")
			(pinfunction "D11")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 103.4525 76.175 90)
		(descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x02 2.54mm single row")
		(property "Reference" "PWR19v1"
			(at 1.88 -3.1225 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 5.31 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 3.81 90)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+19V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 87 73)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 93.98 72.39 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "Pwr5v"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 111.76 149.225)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "CM4"
			(at 3.81 3.81 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 9.95 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(CM4-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(CM4-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(CM4-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(CM4-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 111.76 97.79)
		(descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x02 2.54mm single row")
		(property "Reference" "SW1"
			(at 3.81 0.635 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW_SPDT_XKB_DMx-xxxx-1"
			(at 0 5.31 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Position switch"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW?XKB?DM??16U??1*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(ArduinoConnection1-D10)")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 86.106 148.009 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R_SW1"
			(at 5.08 2.286 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 1.451 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "TMC2209 PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 2.286 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(ArduinoConnection1-D10)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 103.4525 72.39 90)
		(descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x02 2.54mm single row")
		(property "Reference" "Pwr19v"
			(at 0 -2.77 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 5.31 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 3.81 90)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+19V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 84 70.025)
		(end 118 167)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "D2\n"
		(at 87.63 87.63 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 84.455 70.485) (xy 116.84 70.485) (xy 116.84 166.1) (xy 84.455 166.1)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+19V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 106.165531 78.994) (xy 105.41 77.724) (xy 105.41 70.612) (xy 109.982 70.612) (xy 109.982 77.978)
				(xy 109.474 83.82) (xy 109.347 145.415) (xy 106.045 145.415)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 84.455 70.485) (xy 116.84 70.485) (xy 116.84 166.1) (xy 84.455 166.1)
			)
		)
	)
)
