(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-DOUT)")
  (net 2 "GND")
  (net 3 "+5V")
  (net 4 "Net-(D2-DOUT)")
  (net 5 "Net-(D3-DOUT)")
  (net 6 "Net-(D4-DOUT)")
  (net 7 "Net-(D5-DOUT)")
  (net 8 "Net-(D6-DOUT)")
  (net 9 "Net-(D7-DOUT)")
  (net 10 "unconnected-(D8-DOUT-Pad1)")
  (net 11 "Net-(D1-DIN)")
  (footprint "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (layer "F.Cu")
    (at 130 73)
    (descr "3.5mm x 3.5mm PLCC4 Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf")
    (tags "LED RGB NeoPixel Mini PLCC-4 3535")
    (property "Sheetfile" "LED PCB V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel Mini addressable")
    (attr smd)
    (fp_text reference "D5" (at 0 -2.75) (layer "F.SilkS"))
    (fp_text value "SK6812MINI" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D5-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect (at -1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect (at 1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(D4-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect (at 1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (layer "F.Cu")
    (at 100 59)
    (descr "3.5mm x 3.5mm PLCC4 Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf")
    (tags "LED RGB NeoPixel Mini PLCC-4 3535")
    (property "Sheetfile" "LED PCB V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel Mini addressable")
    (attr smd)
    (fp_text reference "D2" (at 0 -2.75) (layer "F.SilkS"))
    (fp_text value "SK6812MINI" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(D2-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect (at -1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect (at 1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(D1-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect (at 1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (layer "F.Cu")
    (at 100 45)
    (descr "3.5mm x 3.5mm PLCC4 Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf")
    (tags "LED RGB NeoPixel Mini PLCC-4 3535")
    (property "Sheetfile" "LED PCB V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel Mini addressable")
    (attr smd)
    (fp_text reference "D1" (at 0 -2.75) (layer "F.SilkS"))
    (fp_text value "SK6812MINI" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(D1-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect (at -1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect (at 1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D1-DIN)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect (at 1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical" (layer "F.Cu")
    (at 102.97 50.05 180)
    (descr "JST EH series connector, B3B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (property "Sheetfile" "LED PCB V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 2.5 -2.8) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x03_Pin" (at 2.5 3.4) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 3 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D1-DIN)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (layer "F.Cu")
    (at 115 73)
    (descr "3.5mm x 3.5mm PLCC4 Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf")
    (tags "LED RGB NeoPixel Mini PLCC-4 3535")
    (property "Sheetfile" "LED PCB V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel Mini addressable")
    (attr smd)
    (fp_text reference "D4" (at 0 -2.75) (layer "F.SilkS"))
    (fp_text value "SK6812MINI" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(D4-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect (at -1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect (at 1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(D3-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect (at 1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (layer "F.Cu")
    (at 115 45)
    (descr "3.5mm x 3.5mm PLCC4 Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf")
    (tags "LED RGB NeoPixel Mini PLCC-4 3535")
    (property "Sheetfile" "LED PCB V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel Mini addressable")
    (attr smd)
    (fp_text reference "D8" (at 0 -2.75) (layer "F.SilkS"))
    (fp_text value "SK6812MINI" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "unconnected-(D8-DOUT-Pad1)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect (at -1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect (at 1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D7-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect (at 1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (layer "F.Cu")
    (at 100 72.875)
    (descr "3.5mm x 3.5mm PLCC4 Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf")
    (tags "LED RGB NeoPixel Mini PLCC-4 3535")
    (property "Sheetfile" "LED PCB V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel Mini addressable")
    (attr smd)
    (fp_text reference "D3" (at 0 -2.75) (layer "F.SilkS"))
    (fp_text value "SK6812MINI" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.665) (layer "F.Fab"))
    (pad "1" smd rect (at -1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(D3-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect (at -1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect (at 1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(D2-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect (at 1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (layer "F.Cu")
    (at 130 59)
    (descr "3.5mm x 3.5mm PLCC4 Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf")
    (tags "LED RGB NeoPixel Mini PLCC-4 3535")
    (property "Sheetfile" "LED PCB V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel Mini addressable")
    (attr smd)
    (fp_text reference "D6" (at 0 -2.75) (layer "F.SilkS"))
    (fp_text value "SK6812MINI" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.5 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D6-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect (at -1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect (at 1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D5-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect (at 1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (layer "F.Cu")
    (at 130 45)
    (descr "3.5mm x 3.5mm PLCC4 Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf")
    (tags "LED RGB NeoPixel Mini PLCC-4 3535")
    (property "Sheetfile" "LED PCB V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel Mini addressable")
    (attr smd)
    (fp_text reference "D7" (at 0 -2.75) (layer "F.SilkS"))
    (fp_text value "SK6812MINI" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.5 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D7-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect (at -1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect (at 1.75 0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D6-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect (at 1.75 -0.875) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 104 48) (end 126 70)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect (start 97 41) (end 133 77)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "5V" (at 102.108 53.848 -90) (layer "B.SilkS"))
  (gr_text "JLCJLCJLCJLC" (at 119.888 42.926) (layer "B.SilkS"))
  (gr_text "GND" (at 97.282 54.61 -90) (layer "B.SilkS"))
  (gr_text "Data" (at 99.568 54.864 -90) (layer "B.SilkS"))
  (gr_text "Data" (at 100.838 54.864 90) (layer "F.SilkS"))
  (gr_text "GND" (at 98.552 54.61 90) (layer "F.SilkS"))
  (gr_text "5v" (at 103.378 53.848 90) (layer "F.SilkS"))
)
