(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(D1-DIN)")
  (net 3 "+5V")
  (net 4 "Net-(D1-DOUT)")
  (net 5 "Net-(D2-DOUT)")
  (net 6 "unconnected-(D3-DIN-Pad2)")
  (net 7 "Net-(D4-DOUT)")
  (net 8 "Net-(D5-DOUT)")
  (net 9 "Net-(D6-DOUT)")
  (net 10 "VS")
  (net 11 "Net-(D7-DOUT)")
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 114.21 77.8)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D7" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D6-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D7-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 129.63 85.42)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D4" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(D2-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D4-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 122.01 77.8)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D6" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D5-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D6-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 114.3 85.42)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D8" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D7-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "VS") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 129.63 77.8)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D5" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D4-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D5-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 122.01 93.04)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D1" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(D1-DIN)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(D1-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 114.39 93.04)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D3" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "unconnected-(D3-DIN-Pad2)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(D1-DIN)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 129.63 93.04)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D2" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(D1-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(D2-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (zone (net 3) (net_name "+5V") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 106.68 71.12)
        (xy 106.68 101.6)
        (xy 137.16 101.6)
        (xy 137.16 71.12)
      )
    )
  )
)
