(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-DIN)")
  (net 2 "Net-(D1-DOUT)")
  (net 3 "Net-(D2-DOUT)")
  (net 4 "unconnected-(D3-DIN-Pad2)")
  (net 5 "Net-(D4-DOUT)")
  (net 6 "Net-(D5-DOUT)")
  (net 7 "Net-(D6-DOUT)")
  (net 8 "Net-(D7-DOUT)")
  (net 9 "Net-(D1-VSS)")
  (net 10 "Net-(D1-VDD)")
  (net 11 "Net-(D8-DOUT)")
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 106.25 105.8 -90)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D7" (at 0 -3.5 90) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6 270) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D1-VSS)") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6 270) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D6-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6 270) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D1-VDD)") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6 270) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D7-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 133.6 119.5)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D4" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D1-VSS)") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(D2-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D1-VDD)") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(D4-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 119.9 105.85 -90)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D6" (at 0 -3.5 90) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6 270) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D1-VSS)") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6 270) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(D5-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6 270) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D1-VDD)") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6 270) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D6-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 106.25 119.45)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D8" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D1-VSS)") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D7-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D1-VDD)") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D8-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 133.75 105.85 -90)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D5" (at 0 -3.5 90) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6 270) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D1-VSS)") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6 270) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(D4-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6 270) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D1-VDD)") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6 270) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(D5-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 119.95 133.15)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D1" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D1-VSS)") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(D1-DIN)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D1-VDD)") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(D1-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 106.1 133.15)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D3" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D1-VSS)") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "unconnected-(D3-DIN-Pad2)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D1-VDD)") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(D1-DIN)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 133.6 133.35)
    (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
    (tags "LED RGB NeoPixel PLCC-4 5050")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr smd)
    (fp_text reference "D2" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D1-VSS)") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(D1-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D1-VDD)") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(D2-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector:FanPinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 102.92 125.95)
    (descr "3-pin CPU fan Through hole pin header, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf")
    (tags "pin header 3-pin CPU fan")
    (property "Sheetfile" "LED PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fan, tacho output, 3-pin connector")
    (property "ki_keywords" "Fan Motor tacho")
    (attr through_hole)
    (fp_text reference "M1" (at 2.5 -3.4) (layer "F.SilkS"))
    (fp_text value "Fan_3pin" (at 2.55 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.45 1.8) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D8-DOUT)") (pinfunction "Tacho") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 2.03 1.73) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D1-VDD)") (pinfunction "+") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 2.03 1.73) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D1-VSS)") (pinfunction "-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 109.5 109) (end 130.4 130)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect (start 101.4 102) (end 138 138)
    (fill none) (layer "Edge.Cuts"))
)
