(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Connector:Conn_01x03_Pin" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 5.08 0))
      (property "Value" "Conn_01x03_Pin" (at 0 -5.08 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x03, script generated" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (at 0 0 0))
      (symbol "Conn_01x03_Pin_1_1"
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 2.54)
            (xy 0.8636 2.54)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (rectangle (start 0.8636 2.667) (end 0 2.413)
          (fill (type outline))
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
      )
    )
    (symbol "LED:SK6812MINI" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 5.08 5.715 0))
      (property "Value" "SK6812MINI" (at 1.27 -5.715 0))
      (property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (at 1.27 -7.62 0))
      (property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf" (at 2.54 -9.525 0))
      (property "ki_keywords" "RGB LED NeoPixel Mini addressable" (at 0 0 0))
      (property "ki_description" "RGB LED with integrated controller" (at 0 0 0))
      (property "ki_fp_filters" "LED*SK6812MINI*PLCC*3.5x3.5mm*P1.75mm*" (at 0 0 0))
      (symbol "SK6812MINI_0_0"
        (text "RGB" (at 2.286 -4.191 0))
      )
      (symbol "SK6812MINI_0_1"
        (polyline
          (pts
            (xy 1.27 -3.556)
            (xy 1.778 -3.556)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 1.778 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.699 -3.556)
            (xy 2.667 -3.556)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.286 -2.54)
            (xy 1.27 -3.556)
            (xy 1.27 -3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.286 -1.524)
            (xy 1.27 -2.54)
            (xy 1.27 -2.032)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.683 -1.016)
            (xy 3.683 -3.556)
            (xy 3.683 -4.064)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.699 -1.524)
            (xy 2.667 -1.524)
            (xy 3.683 -3.556)
            (xy 4.699 -1.524)
          )
          (fill (type none))
        )
        (rectangle (start 5.08 5.08) (end -5.08 -5.08)
          (fill (type background))
        )
      )
      (symbol "SK6812MINI_1_1"
        (pin output line (at 7.62 0 180) (length 2.54)
          (name "DOUT")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "VSS")
          (number "2")
        )
        (pin input line (at -7.62 0 0) (length 2.54)
          (name "DIN")
          (number "3")
        )
        (pin power_in line (at 0 7.62 270) (length 2.54)
          (name "VDD")
          (number "4")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+5V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 158.75 101.6) (diameter 0) (color 0 0 0 0))
  (junction (at 173.99 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 204.47 101.6) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 189.23 101.6) (diameter 0) (color 0 0 0 0))
  (junction (at 101.6 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 101.6) (diameter 0) (color 0 0 0 0))
  (junction (at 204.47 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 189.23 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 173.99 101.6) (diameter 0) (color 0 0 0 0))
  (junction (at 113.03 101.6) (diameter 0) (color 0 0 0 0))
  (junction (at 143.51 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 143.51 101.6) (diameter 0) (color 0 0 0 0))
  (junction (at 158.75 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 113.03 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 101.6 101.6) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 92.71 101.6) (xy 92.71 96.52)))
  (wire (pts (xy 128.27 86.36) (xy 143.51 86.36)))
  (wire (pts (xy 189.23 101.6) (xy 204.47 101.6)))
  (wire (pts (xy 92.71 86.36) (xy 101.6 86.36)))
  (wire (pts (xy 92.71 91.44) (xy 92.71 86.36)))
  (wire (pts (xy 143.51 86.36) (xy 158.75 86.36)))
  (wire (pts (xy 158.75 86.36) (xy 173.99 86.36)))
  (wire (pts (xy 173.99 86.36) (xy 189.23 86.36)))
  (wire (pts (xy 204.47 101.6) (xy 219.71 101.6)))
  (wire (pts (xy 92.71 93.98) (xy 105.41 93.98)))
  (wire (pts (xy 158.75 101.6) (xy 173.99 101.6)))
  (wire (pts (xy 189.23 86.36) (xy 204.47 86.36)))
  (wire (pts (xy 204.47 86.36) (xy 219.71 86.36)))
  (wire (pts (xy 128.27 101.6) (xy 143.51 101.6)))
  (wire (pts (xy 101.6 101.6) (xy 113.03 101.6)))
  (wire (pts (xy 173.99 101.6) (xy 189.23 101.6)))
  (wire (pts (xy 143.51 101.6) (xy 158.75 101.6)))
  (wire (pts (xy 113.03 86.36) (xy 128.27 86.36)))
  (wire (pts (xy 101.6 101.6) (xy 92.71 101.6)))
  (wire (pts (xy 113.03 101.6) (xy 128.27 101.6)))
  (wire (pts (xy 101.6 86.36) (xy 113.03 86.36)))
  (symbol (lib_id "LED:SK6812MINI") (at 204.47 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D7" (at 217.17 90.3321 0))
    (property "Value" "SK6812MINI" (at 217.17 92.8721 0))
    (property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (at 205.74 101.6 0))
    (property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf" (at 207.01 103.505 0))
    (pin "3")
    (pin "2")
    (pin "4")
    (pin "1")
    (instances
      (project "LED PCB V2"
        (path
          (reference "D7") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "LED:SK6812MINI") (at 158.75 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D4" (at 171.45 90.3321 0))
    (property "Value" "SK6812MINI" (at 171.45 92.8721 0))
    (property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (at 160.02 101.6 0))
    (property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf" (at 161.29 103.505 0))
    (pin "3")
    (pin "2")
    (pin "4")
    (pin "1")
    (instances
      (project "LED PCB V2"
        (path
          (reference "D4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 101.6 101.6 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR02" (at 101.6 107.95 0))
    (property "Value" "GND" (at 101.6 106.68 0))
    (property "Footprint" "" (at 101.6 101.6 0))
    (property "Datasheet" "" (at 101.6 101.6 0))
    (pin "1")
    (instances
      (project "LED PCB V2"
        (path
          (reference "#PWR02") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "LED:SK6812MINI") (at 219.71 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D8" (at 232.41 90.3321 0))
    (property "Value" "SK6812MINI" (at 232.41 92.8721 0))
    (property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (at 220.98 101.6 0))
    (property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf" (at 222.25 103.505 0))
    (pin "3")
    (pin "2")
    (pin "4")
    (pin "1")
    (instances
      (project "LED PCB V2"
        (path
          (reference "D8") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 101.6 86.36 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR01" (at 101.6 90.17 0))
    (property "Value" "+5V" (at 101.6 81.28 0))
    (property "Footprint" "" (at 101.6 86.36 0))
    (property "Datasheet" "" (at 101.6 86.36 0))
    (pin "1")
    (instances
      (project "LED PCB V2"
        (path
          (reference "#PWR01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "LED:SK6812MINI") (at 113.03 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D1" (at 125.73 90.3321 0))
    (property "Value" "SK6812MINI" (at 125.73 92.8721 0))
    (property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (at 114.3 101.6 0))
    (property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf" (at 115.57 103.505 0))
    (pin "3")
    (pin "2")
    (pin "4")
    (pin "1")
    (instances
      (project "LED PCB V2"
        (path
          (reference "D1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "LED:SK6812MINI") (at 128.27 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D2" (at 140.97 90.3321 0))
    (property "Value" "SK6812MINI" (at 140.97 92.8721 0))
    (property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (at 129.54 101.6 0))
    (property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf" (at 130.81 103.505 0))
    (pin "3")
    (pin "2")
    (pin "4")
    (pin "1")
    (instances
      (project "LED PCB V2"
        (path
          (reference "D2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:Conn_01x03_Pin") (at 87.63 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "J1" (at 88.265 86.36 0))
    (property "Value" "Conn_01x03_Pin" (at 88.265 88.9 0))
    (property "Footprint" "Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical" (at 87.63 93.98 0))
    (property "Datasheet" "~" (at 87.63 93.98 0))
    (pin "3")
    (pin "1")
    (pin "2")
    (instances
      (project "LED PCB V2"
        (path
          (reference "J1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "LED:SK6812MINI") (at 143.51 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D3" (at 156.21 90.3321 0))
    (property "Value" "SK6812MINI" (at 156.21 92.8721 0))
    (property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (at 144.78 101.6 0))
    (property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf" (at 146.05 103.505 0))
    (pin "3")
    (pin "2")
    (pin "4")
    (pin "1")
    (instances
      (project "LED PCB V2"
        (path
          (reference "D3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "LED:SK6812MINI") (at 173.99 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D5" (at 186.69 90.3321 0))
    (property "Value" "SK6812MINI" (at 186.69 92.8721 0))
    (property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (at 175.26 101.6 0))
    (property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf" (at 176.53 103.505 0))
    (pin "3")
    (pin "2")
    (pin "4")
    (pin "1")
    (instances
      (project "LED PCB V2"
        (path
          (reference "D5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "LED:SK6812MINI") (at 189.23 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D6" (at 201.93 90.3321 0))
    (property "Value" "SK6812MINI" (at 201.93 92.8721 0))
    (property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm" (at 190.5 101.6 0))
    (property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf" (at 191.77 103.505 0))
    (pin "3")
    (pin "2")
    (pin "4")
    (pin "1")
    (instances
      (project "LED PCB V2"
        (path
          (reference "D6") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
